# Static Call Graph for image .\MAXREFDES82\MAXREFDES82.axf

#<CALLGRAPH># ARM Linker, 5050169: Last Updated: Mon Mar 21 01:01:19 2016

### Maximum Stack Usage = 2832 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ MainTask ⇒ Calibration ⇒ GUI_Delay ⇒ GUI_Exec ⇒ GUI_Exec1 ⇒ WM_Exec ⇒ _DrawNext ⇒ WM__Paint ⇒ GUI_MEMDEV_Draw ⇒ GUI_MEMDEV_CopyToLCD ⇒ GUI_MEMDEV_CopyToLCDAt ⇒ GUI_MEMDEV__WriteToActiveOpaque ⇒ _WriteToActiveOpaque_8 ⇒ LCD__DrawBitmap_1bpp ⇒ LCD_FillRect

### Mutually Recursive functions

- ADC_IRQHandler ⇒ ADC_IRQHandler
- BusFault_Handler ⇒ BusFault_Handler
- _Findy1 ⇒ _Findy1
- _Findx1 ⇒ _Findx1
- _Findx0 ⇒ _Findx0
- WM_InvalidateWindowAndDescsEx ⇒ WM_InvalidateWindowAndDescsEx
- WM__InvalidateRect ⇒ WM__InvalidateRect
- WM__InvalidateDrawAndDescs ⇒ WM__InvalidateDrawAndDescs
- WM_SendToParent ⇒ WM__SendMessage
- WM__UpdateChildPositions ⇒ WM_ResizeWindow
- _MoveDescendents ⇒ _MoveDescendents
- _PopFreeBlock ⇒ _EnlargeBlocks
- _Alloc ⇒ _InitOnce
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- _DeleteAllChildren ⇒ WM_DeleteWindow
- _PaintTransChildren ⇒ _PaintTransChildren
- ErrorHandler ⇒ ErrorHandler
- InvertAlpha ⇒ InvertAlpha

  ### Function Pointers

  - ADC_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - BSP_LCD_DrawBitmap16bpp from lcdconf_stm32f429i_disco_mb1075_1.o(i.BSP_LCD_DrawBitmap16bpp) referenced from lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)
  - BSP_LCD_DrawBitmap8bpp from lcdconf_stm32f429i_disco_mb1075_1.o(i.BSP_LCD_DrawBitmap8bpp) referenced from lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)
  - BusFault_Handler from stm32f4xx_it.o(i.BusFault_Handler) referenced from startup_stm32f429xx.o(RESET)
  - CAN1_RX0_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - CAN1_TX_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - CAN2_RX0_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - CAN2_RX1_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - CAN2_SCE_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - CAN2_TX_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - CDC_Itf_Control from usbd_cdc_interface.o(i.CDC_Itf_Control) referenced 2 times from usbd_cdc_interface.o(.data)
  - CDC_Itf_DeInit from usbd_cdc_interface.o(i.CDC_Itf_DeInit) referenced 2 times from usbd_cdc_interface.o(.data)
  - CDC_Itf_Init from usbd_cdc_interface.o(i.CDC_Itf_Init) referenced 2 times from usbd_cdc_interface.o(.data)
  - CDC_Itf_Receive from usbd_cdc_interface.o(i.CDC_Itf_Receive) referenced 2 times from usbd_cdc_interface.o(.data)
  - CUSTOM_CopyBuffer from lcdconf_stm32f429i_disco_mb1075_1.o(i.CUSTOM_CopyBuffer) referenced from lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)
  - CUSTOM_CopyRect from lcdconf_stm32f429i_disco_mb1075_1.o(i.CUSTOM_CopyRect) referenced from lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)
  - CUSTOM_FillRect from lcdconf_stm32f429i_disco_mb1075_1.o(i.CUSTOM_FillRect) referenced from lcdconf_stm32f429i_disco_mb1075_1.o(i.CUSTOM_FillRect)
  - CUSTOM_FillRect from lcdconf_stm32f429i_disco_mb1075_1.o(i.CUSTOM_FillRect) referenced from lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)
  - Color2IndexBulk_M1555IDMA2D from lcdconf_stm32f429i_disco_mb1075_1.o(i.Color2IndexBulk_M1555IDMA2D) referenced from lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)
  - Color2IndexBulk_M4444IDMA2D from lcdconf_stm32f429i_disco_mb1075_1.o(i.Color2IndexBulk_M4444IDMA2D) referenced from lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)
  - Color2IndexBulk_M565DMA2D from lcdconf_stm32f429i_disco_mb1075_1.o(i.Color2IndexBulk_M565DMA2D) referenced from lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)
  - Color2IndexBulk_M8888IDMA2D from lcdconf_stm32f429i_disco_mb1075_1.o(i.Color2IndexBulk_M8888IDMA2D) referenced from lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)
  - Color2IndexBulk_M888DMA2D from lcdconf_stm32f429i_disco_mb1075_1.o(i.Color2IndexBulk_M888DMA2D) referenced from lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)
  - DCMI_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DMA1_Stream0_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DMA1_Stream1_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DMA1_Stream2_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DMA1_Stream3_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DMA1_Stream4_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DMA1_Stream5_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DMA1_Stream6_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DMA1_Stream7_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DMA2D_AlphaBlending from lcdconf_stm32f429i_disco_mb1075_1.o(i.DMA2D_AlphaBlending) referenced from lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)
  - DMA2D_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DMA2D_MixColors from lcdconf_stm32f429i_disco_mb1075_1.o(i.DMA2D_MixColors) referenced from lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)
  - DMA2_Stream0_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DMA2_Stream1_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DMA2_Stream2_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DMA2_Stream3_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DMA2_Stream4_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DMA2_Stream5_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DMA2_Stream6_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DMA2_Stream7_IRQHandler from stm32f4xx_it.o(i.DMA2_Stream7_IRQHandler) referenced from startup_stm32f429xx.o(RESET)
  - DebugMon_Handler from stm32f4xx_it.o(i.DebugMon_Handler) referenced from startup_stm32f429xx.o(RESET)
  - ETH_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - ETH_WKUP_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - FLASH_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - FMC_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - FPU_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - GUIMONO_DispChar from gui_charm.o(i.GUIMONO_DispChar) referenced 2 times from f6x8.o(.constdata)
  - GUIMONO_GetCharDistX from gui_charm.o(i.GUIMONO_GetCharDistX) referenced 2 times from f6x8.o(.constdata)
  - GUIMONO_GetFontInfo from gui_charm.o(i.GUIMONO_GetFontInfo) referenced 2 times from f6x8.o(.constdata)
  - GUIMONO_IsInFont from gui_charm.o(i.GUIMONO_IsInFont) referenced 2 times from f6x8.o(.constdata)
  - GUI_MEMDEV_Paint1Static from guidev_staticdevices.o(i.GUI_MEMDEV_Paint1Static) referenced from wm.o(i._Paint1)
  - GUI_MEMDEV__WriteToActiveAlpha from guidev_writetoactivealpha.o(i.GUI_MEMDEV__WriteToActiveAlpha) referenced from guidev_32.o(i._GetDevFunc)
  - GUI_USAGE_BM_AddHLine from guidev_usagebm.o(i.GUI_USAGE_BM_AddHLine) referenced from guidev_usagebm.o(.constdata)
  - GUI_USAGE_BM_AddPixel from guidev_usagebm.o(i.GUI_USAGE_BM_AddPixel) referenced from guidev_usagebm.o(.constdata)
  - GUI_USAGE_BM_Clear from guidev_usagebm.o(i.GUI_USAGE_BM_Clear) referenced from guidev_usagebm.o(.constdata)
  - GUI_USAGE_BM_GetNextDirty from guidev_usagebm.o(i.GUI_USAGE_BM_GetNextDirty) referenced from guidev_usagebm.o(.constdata)
  - GUI_X_ExecIdle from gui_x.o(i.GUI_X_ExecIdle) referenced 2 times from gui_waitevent.o(.data)
  - GUI__MixColors from gui__alpha.o(i.GUI__MixColors) referenced 2 times from gui__alpha.o(.data)
  - GUI__MixColorsBulk from gui__alpha.o(i.GUI__MixColorsBulk) referenced 2 times from gui__alpha.o(.data)
  - HASH_RNG_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - HardFault_Handler from stm32f4xx_it.o(i.HardFault_Handler) referenced from startup_stm32f429xx.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - I2C3_ER_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - I2C3_EV_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - Index2ColorBulk_M1555IDMA2D from lcdconf_stm32f429i_disco_mb1075_1.o(i.Index2ColorBulk_M1555IDMA2D) referenced from lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)
  - Index2ColorBulk_M4444IDMA2D from lcdconf_stm32f429i_disco_mb1075_1.o(i.Index2ColorBulk_M4444IDMA2D) referenced from lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)
  - Index2ColorBulk_M565DMA2D from lcdconf_stm32f429i_disco_mb1075_1.o(i.Index2ColorBulk_M565DMA2D) referenced from lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)
  - Index2ColorBulk_M8888IDMA2D from lcdconf_stm32f429i_disco_mb1075_1.o(i.Index2ColorBulk_M8888IDMA2D) referenced from lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)
  - Index2ColorBulk_M888DMA2D from lcdconf_stm32f429i_disco_mb1075_1.o(i.Index2ColorBulk_M888DMA2D) referenced from lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)
  - LCD_Color2Index_8666 from guicc_8666.o(i.LCD_Color2Index_8666) referenced from guicc_8666.o(.constdata)
  - LCD_DrawHLine from lcd.o(i.LCD_DrawHLine) referenced from gui_core.o(.constdata)
  - LCD_DrawPixel from lcd.o(i.LCD_DrawPixel) referenced from gui_core.o(.constdata)
  - LCD_GetpPalConvTableBM from lcd_color.o(i.LCD_GetpPalConvTableBM) referenced 2 times from gui_core.o(.data)
  - LCD_Index2Color_8666 from guicc_8666.o(i.LCD_Index2Color_8666) referenced from guicc_8666.o(.constdata)
  - LCD_Index2Color_888 from guicc_888_index2color.o(i.LCD_Index2Color_888) referenced from gui__alpha.o(i.GUI__DoAlphaBlending)
  - LCD_Index2Color_8888 from guicc_8888_index2color.o(i.LCD_Index2Color_8888) referenced from guicc_8888.o(.constdata)
  - LCD_Index2Color_8888 from guicc_8888_index2color.o(i.LCD_Index2Color_8888) referenced from guidev_writetoactivealpha.o(i.GUI_MEMDEV__WriteToActiveAlpha)
  - LCD_Index2Color_8888 from guicc_8888_index2color.o(i.LCD_Index2Color_8888) referenced from gui__alpha.o(i.GUI__DoAlphaBlending)
  - LCD_Index2Color_M565 from guicc_m565.o(i.LCD_Index2Color_M565) referenced from guicc_m565.o(.constdata)
  - LCD_Index2Color_M888 from guicc_m888_index2color.o(i.LCD_Index2Color_M888) referenced from guicc_m888.o(.constdata)
  - LCD_MixColorsBulk from lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_MixColorsBulk) referenced from lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)
  - LCD_SetPixelAA4_NoTrans from lcd_aa.o(i.LCD_SetPixelAA4_NoTrans) referenced from lcd_aa.o(i.LCD__GetPfSetPixel)
  - LCD_SetPixelAA4_Trans from lcd_aa.o(i.LCD_SetPixelAA4_Trans) referenced from lcd_aa.o(i.LCD__GetPfSetPixel)
  - LCD_SetPixelAA8_NoTrans from lcd_aa.o(i.LCD_SetPixelAA8_NoTrans) referenced from lcd_aa.o(i.LCD__GetPfSetPixel)
  - LCD_SetPixelAA8_Trans from lcd_aa.o(i.LCD_SetPixelAA8_Trans) referenced from lcd_aa.o(i.LCD__GetPfSetPixel)
  - LTDC_ER_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - LTDC_IRQHandler from stm32f4xx_it.o(i.LTDC_IRQHandler) referenced from startup_stm32f429xx.o(RESET)
  - MemManage_Handler from stm32f4xx_it.o(i.MemManage_Handler) referenced from startup_stm32f429xx.o(RESET)
  - NMI_Handler from stm32f4xx_it.o(i.NMI_Handler) referenced from startup_stm32f429xx.o(RESET)
  - OTG_FS_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - OTG_FS_WKUP_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - OTG_HS_EP1_IN_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - OTG_HS_EP1_OUT_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - OTG_HS_IRQHandler from stm32f4xx_it.o(i.OTG_HS_IRQHandler) referenced from startup_stm32f429xx.o(RESET)
  - OTG_HS_WKUP_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - PVD_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - PendSV_Handler from stm32f4xx_it.o(i.PendSV_Handler) referenced from startup_stm32f429xx.o(RESET)
  - RCC_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - RTC_WKUP_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - Reset_Handler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - SAI1_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - SDIO_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - SPI1_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - SPI2_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - SPI3_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - SPI4_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - SPI5_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - SPI6_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - SVC_Handler from stm32f4xx_it.o(i.SVC_Handler) referenced from startup_stm32f429xx.o(RESET)
  - SysTick_Handler from stm32f4xx_it.o(i.SysTick_Handler) referenced from startup_stm32f429xx.o(RESET)
  - SystemInit from system_stm32f4xx.o(i.SystemInit) referenced from startup_stm32f429xx.o(.text)
  - TAMP_STAMP_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - TIM1_BRK_TIM9_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - TIM1_TRG_COM_TIM11_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - TIM1_UP_TIM10_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - TIM2_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - TIM3_IRQHandler from stm32f4xx_it.o(i.TIM3_IRQHandler) referenced from startup_stm32f429xx.o(RESET)
  - TIM4_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - TIM5_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - TIM6_DAC_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - TIM7_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - TIM8_BRK_TIM12_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - TIM8_TRG_COM_TIM14_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - TIM8_UP_TIM13_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - UART4_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - UART5_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - UART7_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - UART8_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - UART_DMAError from stm32f4xx_hal_uart.o(i.UART_DMAError) referenced from stm32f4xx_hal_uart.o(i.HAL_UART_Transmit_DMA)
  - UART_DMATransmitCplt from stm32f4xx_hal_uart.o(i.UART_DMATransmitCplt) referenced from stm32f4xx_hal_uart.o(i.HAL_UART_Transmit_DMA)
  - UART_DMATxHalfCplt from stm32f4xx_hal_uart.o(i.UART_DMATxHalfCplt) referenced from stm32f4xx_hal_uart.o(i.HAL_UART_Transmit_DMA)
  - USART1_IRQHandler from stm32f4xx_it.o(i.USART1_IRQHandler) referenced from startup_stm32f429xx.o(RESET)
  - USART2_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - USART3_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - USART6_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - USBD_CDC_DataIn from usbd_cdc.o(i.USBD_CDC_DataIn) referenced 2 times from usbd_cdc.o(.data)
  - USBD_CDC_DataOut from usbd_cdc.o(i.USBD_CDC_DataOut) referenced 2 times from usbd_cdc.o(.data)
  - USBD_CDC_DeInit from usbd_cdc.o(i.USBD_CDC_DeInit) referenced 2 times from usbd_cdc.o(.data)
  - USBD_CDC_EP0_RxReady from usbd_cdc.o(i.USBD_CDC_EP0_RxReady) referenced 2 times from usbd_cdc.o(.data)
  - USBD_CDC_GetDeviceQualifierDescriptor from usbd_cdc.o(i.USBD_CDC_GetDeviceQualifierDescriptor) referenced 2 times from usbd_cdc.o(.data)
  - USBD_CDC_GetFSCfgDesc from usbd_cdc.o(i.USBD_CDC_GetFSCfgDesc) referenced 2 times from usbd_cdc.o(.data)
  - USBD_CDC_GetHSCfgDesc from usbd_cdc.o(i.USBD_CDC_GetHSCfgDesc) referenced 2 times from usbd_cdc.o(.data)
  - USBD_CDC_GetOtherSpeedCfgDesc from usbd_cdc.o(i.USBD_CDC_GetOtherSpeedCfgDesc) referenced 2 times from usbd_cdc.o(.data)
  - USBD_CDC_Init from usbd_cdc.o(i.USBD_CDC_Init) referenced 2 times from usbd_cdc.o(.data)
  - USBD_CDC_Setup from usbd_cdc.o(i.USBD_CDC_Setup) referenced 2 times from usbd_cdc.o(.data)
  - USBD_VCP_ConfigStrDescriptor from usbd_desc.o(i.USBD_VCP_ConfigStrDescriptor) referenced 2 times from usbd_desc.o(.data)
  - USBD_VCP_DeviceDescriptor from usbd_desc.o(i.USBD_VCP_DeviceDescriptor) referenced 2 times from usbd_desc.o(.data)
  - USBD_VCP_InterfaceStrDescriptor from usbd_desc.o(i.USBD_VCP_InterfaceStrDescriptor) referenced 2 times from usbd_desc.o(.data)
  - USBD_VCP_LangIDStrDescriptor from usbd_desc.o(i.USBD_VCP_LangIDStrDescriptor) referenced 2 times from usbd_desc.o(.data)
  - USBD_VCP_ManufacturerStrDescriptor from usbd_desc.o(i.USBD_VCP_ManufacturerStrDescriptor) referenced 2 times from usbd_desc.o(.data)
  - USBD_VCP_ProductStrDescriptor from usbd_desc.o(i.USBD_VCP_ProductStrDescriptor) referenced 2 times from usbd_desc.o(.data)
  - USBD_VCP_SerialStrDescriptor from usbd_desc.o(i.USBD_VCP_SerialStrDescriptor) referenced 2 times from usbd_desc.o(.data)
  - UsageFault_Handler from stm32f4xx_it.o(i.UsageFault_Handler) referenced from startup_stm32f429xx.o(RESET)
  - WM__Paint1 from wm.o(i.WM__Paint1) referenced from wm.o(i._Paint1)
  - WWDG_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - _CalcSizeOfChar from gui_uc_encodenone.o(i._CalcSizeOfChar) referenced from gui_uc_encodenone.o(.constdata)
  - _Color2IndexBulk from guicc_m565.o(i._Color2IndexBulk) referenced 3 times from guicc_m565.o(.constdata)
  - _Color2IndexBulk_1616I from guicc_1616i.o(i._Color2IndexBulk_1616I) referenced from guicc_1616i.o(.constdata)
  - _Color2IndexBulk_88666I from guicc_88666i.o(i._Color2IndexBulk_88666I) referenced from guicc_88666i.o(.constdata)
  - _Color2IndexBulk_M1555I from guicc_m1555i.o(i._Color2IndexBulk_M1555I) referenced from guicc_m1555i.o(.constdata)
  - _Color2IndexBulk_M4444I from guicc_m4444i.o(i._Color2IndexBulk_M4444I) referenced from guicc_m4444i.o(.constdata)
  - _Color2IndexBulk_M8888I from guicc_m8888i.o(i._Color2IndexBulk_M8888I) referenced from guicc_m8888i.o(.constdata)
  - _Color2Index_0 from guicc_0.o(i._Color2Index_0) referenced from guicc_0.o(.constdata)
  - _Color2Index_16 from guicc_16.o(i._Color2Index_16) referenced from guicc_16.o(.constdata)
  - _Color2Index_1616I from guicc_1616i.o(i._Color2Index_1616I) referenced from guicc_1616i.o(.constdata)
  - _Color2Index_88666I from guicc_88666i.o(i._Color2Index_88666I) referenced from guicc_88666i.o(.constdata)
  - _Color2Index_8888 from guicc_8888.o(i._Color2Index_8888) referenced from guicc_8888.o(.constdata)
  - _Color2Index_M1555I from guicc_m1555i.o(i._Color2Index_M1555I) referenced from guicc_m1555i.o(.constdata)
  - _Color2Index_M4444I from guicc_m4444i.o(i._Color2Index_M4444I) referenced from guicc_m4444i.o(.constdata)
  - _Color2Index_M565 from guicc_m565.o(i._Color2Index_M565) referenced from guicc_m565.o(.constdata)
  - _Color2Index_M888 from guicc_m888.o(i._Color2Index_M888) referenced from guicc_m888.o(.constdata)
  - _Color2Index_M8888I from guicc_m8888i.o(i._Color2Index_M8888I) referenced from guicc_m8888i.o(.constdata)
  - _CopyBuffer from guidrv_lin_32.o(i._CopyBuffer) referenced from guidrv_lin_32.o(i._GetDevFunc)
  - _DrawBitmap from guidrv_lin_32.o(i._DrawBitmap) referenced 2 times from guidrv_lin_32.o(.constdata)
  - _DrawBitmapCW from lcd_rotatecw.o(i._DrawBitmapCW) referenced 2 times from lcd_rotatecw.o(.data)
  - _DrawHLine from guidrv_lin_32.o(i._DrawHLine) referenced 2 times from guidrv_lin_32.o(.constdata)
  - _DrawVLine from guidrv_lin_32.o(i._DrawVLine) referenced 2 times from guidrv_lin_32.o(.constdata)
  - _Encode from gui_uc_encodenone.o(i._Encode) referenced from gui_uc_encodenone.o(.constdata)
  - _FillRect from guidrv_lin_32.o(i._FillRect) referenced 2 times from guidrv_lin_32.o(.constdata)
  - _GUI_USAGE_BM_Delete from guidev_usagebm.o(i._GUI_USAGE_BM_Delete) referenced from guidev_usagebm.o(.constdata)
  - _GetCharCode from gui_uc_encodenone.o(i._GetCharCode) referenced from gui_uc_encodenone.o(.constdata)
  - _GetCharSize from gui_uc_encodenone.o(i._GetCharSize) referenced from gui_uc_encodenone.o(.constdata)
  - _GetDevData from guidrv_lin_32.o(i._GetDevData) referenced 2 times from guidrv_lin_32.o(.constdata)
  - _GetDevFunc from guidrv_lin_32.o(i._GetDevFunc) referenced 2 times from guidrv_lin_32.o(.constdata)
  - _GetDevProp from guidrv_lin_32.o(i._GetDevProp) referenced 2 times from guidrv_lin_32.o(.constdata)
  - _GetIndexMask_0 from guicc_0.o(i._GetIndexMask_0) referenced from guicc_0.o(.constdata)
  - _GetIndexMask_16 from guicc_16.o(i._GetIndexMask_16) referenced from guicc_16.o(.constdata)
  - _GetIndexMask_1616I from guicc_1616i.o(i._GetIndexMask_1616I) referenced from guicc_1616i.o(.constdata)
  - _GetIndexMask_8666 from guicc_8666.o(i._GetIndexMask_8666) referenced from guicc_8666.o(.constdata)
  - _GetIndexMask_88666I from guicc_88666i.o(i._GetIndexMask_88666I) referenced from guicc_88666i.o(.constdata)
  - _GetIndexMask_8888 from guicc_8888.o(i._GetIndexMask_8888) referenced from guicc_8888.o(.constdata)
  - _GetIndexMask_M1555I from guicc_m1555i.o(i._GetIndexMask_M1555I) referenced from guicc_m1555i.o(.constdata)
  - _GetIndexMask_M4444I from guicc_m4444i.o(i._GetIndexMask_M4444I) referenced from guicc_m4444i.o(.constdata)
  - _GetIndexMask_M565 from guicc_m565.o(i._GetIndexMask_M565) referenced from guicc_m565.o(.constdata)
  - _GetIndexMask_M888 from guicc_m888.o(i._GetIndexMask_M888) referenced from guicc_m888.o(.constdata)
  - _GetIndexMask_M8888I from guicc_m8888i.o(i._GetIndexMask_M8888I) referenced from guicc_m8888i.o(.constdata)
  - _GetPixelIndex from guidrv_lin_32.o(i._GetPixelIndex) referenced 2 times from guidrv_lin_32.o(.constdata)
  - _GetPos from guidrv_lin_32.o(i._GetPos) referenced from guidrv_lin_32.o(i._GetDevFunc)
  - _GetRect from guidrv_lin_32.o(i._GetRect) referenced 2 times from guidrv_lin_32.o(.constdata)
  - _Index2ColorBulk from guicc_m565.o(i._Index2ColorBulk) referenced 3 times from guicc_m565.o(.constdata)
  - _Index2ColorBulk_1616I from guicc_1616i.o(i._Index2ColorBulk_1616I) referenced from guicc_1616i.o(.constdata)
  - _Index2ColorBulk_88666I from guicc_88666i.o(i._Index2ColorBulk_88666I) referenced from guicc_88666i.o(.constdata)
  - _Index2ColorBulk_M1555I from guicc_m1555i.o(i._Index2ColorBulk_M1555I) referenced from guicc_m1555i.o(.constdata)
  - _Index2ColorBulk_M4444I from guicc_m4444i.o(i._Index2ColorBulk_M4444I) referenced from guicc_m4444i.o(.constdata)
  - _Index2ColorBulk_M8888I from guicc_m8888i.o(i._Index2ColorBulk_M8888I) referenced from guicc_m8888i.o(.constdata)
  - _Index2Color_0 from guicc_0.o(i._Index2Color_0) referenced from guicc_0.o(.constdata)
  - _Index2Color_16 from guicc_16.o(i._Index2Color_16) referenced from guicc_16.o(.constdata)
  - _Index2Color_1616I from guicc_1616i.o(i._Index2Color_1616I) referenced from guicc_1616i.o(.constdata)
  - _Index2Color_88666I from guicc_88666i.o(i._Index2Color_88666I) referenced from guicc_88666i.o(.constdata)
  - _Index2Color_M1555I from guicc_m1555i.o(i._Index2Color_M1555I) referenced from guicc_m1555i.o(.constdata)
  - _Index2Color_M4444I from guicc_m4444i.o(i._Index2Color_M4444I) referenced from guicc_m4444i.o(.constdata)
  - _Index2Color_M8888I from guicc_m8888i.o(i._Index2Color_M8888I) referenced from guicc_m8888i.o(.constdata)
  - _Init from guidrv_lin_32.o(i._Init) referenced from guidrv_lin_32.o(i._GetDevFunc)
  - _LCD_GetpPalConvTable from lcdconf_stm32f429i_disco_mb1075_1.o(i._LCD_GetpPalConvTable) referenced from lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)
  - _Log2VisBuffered from gui_charline.o(i._Log2VisBuffered) referenced 2 times from gui_charline.o(.data)
  - _Off from guidrv_lin_32.o(i._Off) referenced from guidrv_lin_32.o(i._GetDevFunc)
  - _On from guidrv_lin_32.o(i._On) referenced from guidrv_lin_32.o(i._GetDevFunc)
  - _OnExit from gui_core.o(i._OnExit) referenced from gui_core.o(i.GUI__Config)
  - _OnExit from gui__alpha.o(i._OnExit) referenced from gui__alpha.o(i.GUI__GetAlphaBuffer)
  - _OnExit from lcd_color.o(i._OnExit) referenced from lcd_color.o(i.LCD_InitColors)
  - _OnExit from wm.o(i._OnExit) referenced from wm.o(i.WM_Init)
  - _OnExit from gui_alloc.o(i._OnExit) referenced from gui_alloc.o(i._InitOnce)
  - _ReadRect from guidrv_lin_32.o(i._ReadRect) referenced from guidrv_lin_32.o(i._GetDevFunc)
  - _Rect2TextRect from lcd_rotatecw.o(i._Rect2TextRect) referenced 2 times from lcd_rotatecw.o(.data)
  - _SetAlpha from guidrv_lin_32.o(i._SetAlpha) referenced from guidrv_lin_32.o(i._GetDevFunc)
  - _SetAlphaMode from guidrv_lin_32.o(i._SetAlphaMode) referenced from guidrv_lin_32.o(i._GetDevFunc)
  - _SetBkColor from lcd.o(i._SetBkColor) referenced from lcd.o(.constdata)
  - _SetChroma from guidrv_lin_32.o(i._SetChroma) referenced from guidrv_lin_32.o(i._GetDevFunc)
  - _SetChromaMode from guidrv_lin_32.o(i._SetChromaMode) referenced from guidrv_lin_32.o(i._GetDevFunc)
  - _SetColor from lcd.o(i._SetColor) referenced from lcd.o(.constdata)
  - _SetDevFunc from guidrv_lin_32.o(i._SetDevFunc) referenced from guidrv_lin_32.o(i._GetDevFunc)
  - _SetDrawMode from lcd.o(i._SetDrawMode) referenced from lcd.o(.constdata)
  - _SetOrg from guidrv_lin_32.o(i._SetOrg) referenced 2 times from guidrv_lin_32.o(.constdata)
  - _SetPixelIndex from guidrv_lin_32.o(i._SetPixelIndex) referenced 2 times from guidrv_lin_32.o(.constdata)
  - _SetPos from guidrv_lin_32.o(i._SetPos) referenced from guidrv_lin_32.o(i._GetDevFunc)
  - _SetSize from guidrv_lin_32.o(i._SetSize) referenced from guidrv_lin_32.o(i._GetDevFunc)
  - _SetVRAMAddr from guidrv_lin_32.o(i._SetVRAMAddr) referenced from guidrv_lin_32.o(i._GetDevFunc)
  - _SetVSize from guidrv_lin_32.o(i._SetVSize) referenced from guidrv_lin_32.o(i._GetDevFunc)
  - _SetVis from guidrv_lin_32.o(i._SetVis) referenced from guidrv_lin_32.o(i._GetDevFunc)
  - _ShowBuffer from guidrv_lin_32.o(i._ShowBuffer) referenced from guidrv_lin_32.o(i._GetDevFunc)
  - _TransformRect from lcd_rotatecw.o(i._TransformRect) referenced 2 times from lcd_rotatecw.o(.data)
  - _XorPixel from guidrv_lin_32.o(i._XorPixel) referenced 2 times from guidrv_lin_32.o(.constdata)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f429xx.o(.text)
  - _cbPaintMemDev from wm.o(i._cbPaintMemDev) referenced from wm.o(i.WM__Paint)
  - _sputc from printfa.o(i._sputc) referenced from printfa.o(i.__0sprintf)
  - cbBackWin from wm.o(i.cbBackWin) referenced from wm.o(i.WM_Init)
  - main from maxrefdes82.o(i.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f429xx.o(RESET)

  CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  CAN2_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  CAN2_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  CAN2_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  CAN2_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DCMI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DMA1_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DMA1_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DMA1_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DMA1_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DMA1_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DMA1_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DMA1_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DMA1_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DMA2D_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DMA2_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DMA2_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DMA2_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DMA2_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DMA2_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DMA2_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DMA2_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  ETH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  ETH_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  FMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  HASH_RNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  I2C3_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  I2C3_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  LTDC_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  OTG_FS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  OTG_FS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  OTG_HS_EP1_IN_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  OTG_HS_EP1_OUT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  OTG_HS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  RTC_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  SAI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  SPI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  SPI5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  SPI6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  TAMP_STAMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  TIM1_BRK_TIM9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  TIM1_TRG_COM_TIM11_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  TIM1_UP_TIM10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  TIM6_DAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  TIM8_BRK_TIM12_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  TIM8_TRG_COM_TIM14_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  TIM8_UP_TIM13_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  UART7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  UART8_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  USART6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  ___aeabi_memcpy8$move (Thumb, 0 bytes, Stack size 8 bytes, memmovea.o(.text), UNUSED)

  __aeabi_memcpy (Thumb, 64 bytes, Stack size 8 bytes, memmovea.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_memcpy
  [Called By]
  - >> _DrawBitmap
  - >> _CopyBuffer

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 8 bytes, memmovea.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_memcpy4
  [Called By]
  - >> HAL_PCD_Init
  - >> Calibration
  - >> MainTask
  - >> HAL_LTDC_ConfigLayer
  - >> _EnlargeBlocks
  - >> _DrawBitLine32BPP_DDB
  - >> GUI_SaveContext_W
  - >> GUI_RestoreContext

  __aeabi_memmove (Thumb, 0 bytes, Stack size 8 bytes, memmovea.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_memmove
  [Called By]
  - >> _RemoveHoles

  __aeabi_memmove4 (Thumb, 0 bytes, Stack size 8 bytes, memmovea.o(.text), UNUSED)

  __aeabi_memmove8 (Thumb, 0 bytes, Stack size 8 bytes, memmovea.o(.text), UNUSED)

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> GUI_USAGE_BM_AddHLine
  - >> _memset$wrapper
  - >> __aeabi_memclr

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> GUI_USAGE_BM_Clear

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 18 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  strlen (Thumb, 14 bytes, Stack size 0 bytes, strlen.o(.text))
  [Called By]

  - >> Calibration
  - >> MainTask

  __aeabi_dadd (Thumb, 322 bytes, Stack size 48 bytes, dadd.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = __aeabi_dadd ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_lasr
  - >> __aeabi_llsl
  - >> _double_round
  - >> _double_epilogue
  [Called By]
  - >> __aeabi_dsub
  - >> __aeabi_drsub
  - >> Calibration
  - >> MainTask
  - >> _fp_digits

  __aeabi_dsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = __aeabi_dsub ⇒ __aeabi_dadd ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_dadd
  [Called By]
  - >> MainTask

  __aeabi_drsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = __aeabi_drsub ⇒ __aeabi_dadd ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_dadd
  [Called By]
  - >> MainTask

  __aeabi_dmul (Thumb, 228 bytes, Stack size 48 bytes, dmul.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> MainTask
  - >> _fp_digits

  __aeabi_ddiv (Thumb, 222 bytes, Stack size 32 bytes, ddiv.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = __aeabi_ddiv ⇒ _double_round
  [Calls]
  - >> _double_round
  [Called By]
  - >> Calibration
  - >> MainTask
  - >> _fp_digits

  __aeabi_i2d (Thumb, 34 bytes, Stack size 16 bytes, dflti.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = __aeabi_i2d ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> Calibration
  - >> MainTask

  __aeabi_ui2d (Thumb, 26 bytes, Stack size 16 bytes, dfltui.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = __aeabi_ui2d ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> MainTask

  __aeabi_d2iz (Thumb, 62 bytes, Stack size 16 bytes, dfixi.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_d2iz
  [Calls]
  - >> __aeabi_llsr
  [Called By]
  - >> MainTask

  __aeabi_cdcmpeq (Thumb, 0 bytes, Stack size 0 bytes, cdcmple.o(.text), UNUSED)

  __aeabi_cdcmple (Thumb, 48 bytes, Stack size 0 bytes, cdcmple.o(.text))
  [Called By]

  - >> MainTask

  __aeabi_cdrcmple (Thumb, 48 bytes, Stack size 0 bytes, cdrcmple.o(.text))
  [Called By]

  - >> MainTask
  - >> _fp_digits

  __aeabi_uidiv (Thumb, 0 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)

  __aeabi_uidivmod (Thumb, 44 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)
  [Called By]

  - >> _printf_core

  __aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _printf_core
  - >> _fp_digits

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text))
  [Called By]

  - >> __aeabi_dadd
  - >> __aeabi_uldivmod
  - >> _double_epilogue
  - >> __aeabi_d2ulz

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text))
  [Called By]

  - >> __aeabi_d2iz
  - >> __aeabi_uldivmod
  - >> _double_epilogue
  - >> __aeabi_d2ulz

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  __aeabi_lasr (Thumb, 36 bytes, Stack size 0 bytes, llsshr.o(.text))
  [Called By]

  - >> __aeabi_dadd

  _ll_sshift_r (Thumb, 0 bytes, Stack size 0 bytes, llsshr.o(.text), UNUSED)

  __I$use$fp (Thumb, 0 bytes, Stack size 8 bytes, iusefp.o(.text), UNUSED)

  _double_round (Thumb, 30 bytes, Stack size 8 bytes, depilogue.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = _double_round
  [Called By]
  - >> __aeabi_ddiv
  - >> __aeabi_dadd
  - >> _double_epilogue

  _double_epilogue (Thumb, 156 bytes, Stack size 32 bytes, depilogue.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_llsr
  - >> __aeabi_llsl
  - >> _double_round
  [Called By]
  - >> __aeabi_ui2d
  - >> __aeabi_i2d
  - >> __aeabi_dmul
  - >> __aeabi_dadd

  __aeabi_d2ulz (Thumb, 48 bytes, Stack size 0 bytes, dfixul.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _fp_digits

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __decompress (Thumb, 0 bytes, Stack size unknown bytes, __dczerorl2.o(.text), UNUSED)

  __decompress1 (Thumb, 86 bytes, Stack size unknown bytes, __dczerorl2.o(.text), UNUSED)

  BSP_LED_Init (Thumb, 78 bytes, Stack size 40 bytes, stm32f429i_discovery.o(i.BSP_LED_Init))
  [Stack]

  - Max Depth = 80
  - Call Chain = BSP_LED_Init ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  - >> HAL_GPIO_WritePin
  [Called By]
  - >> main

  BSP_LED_Toggle (Thumb, 16 bytes, Stack size 0 bytes, stm32f429i_discovery.o(i.BSP_LED_Toggle))
  [Calls]

  - >> HAL_GPIO_TogglePin
  [Called By]
  - >> Calibration
  - >> ErrorHandler
  - >> MainTask

  BSP_SDRAM_Init (Thumb, 92 bytes, Stack size 8 bytes, stm32f429i_discovery_sdram.o(i.BSP_SDRAM_Init))
  [Stack]

  - Max Depth = 88
  - Call Chain = BSP_SDRAM_Init ⇒ BSP_SDRAM_Initialization_sequence ⇒ HAL_SDRAM_SendCommand ⇒ FMC_SDRAM_SendCommand
  [Calls]
  - >> HAL_SDRAM_Init
  - >> BSP_SDRAM_Initialization_sequence
  - >> MspInit
  [Called By]
  - >> main

  BSP_SDRAM_Initialization_sequence (Thumb, 132 bytes, Stack size 40 bytes, stm32f429i_discovery_sdram.o(i.BSP_SDRAM_Initialization_sequence))
  [Stack]

  - Max Depth = 80
  - Call Chain = BSP_SDRAM_Initialization_sequence ⇒ HAL_SDRAM_SendCommand ⇒ FMC_SDRAM_SendCommand
  [Calls]
  - >> HAL_Delay
  - >> HAL_SDRAM_SendCommand
  - >> HAL_SDRAM_ProgramRefreshRate
  [Called By]
  - >> BSP_SDRAM_Init

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.BusFault_Handler))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f429xx.o(RESET)

  Calibration (Thumb, 844 bytes, Stack size 1712 bytes, maintask.o(i.Calibration))
  [Stack]

  - Max Depth = 2392
  - Call Chain = Calibration ⇒ GUI_Delay ⇒ GUI_Exec ⇒ GUI_Exec1 ⇒ WM_Exec ⇒ _DrawNext ⇒ WM__Paint ⇒ GUI_MEMDEV_Draw ⇒ GUI_MEMDEV_CopyToLCD ⇒ GUI_MEMDEV_CopyToLCDAt ⇒ GUI_MEMDEV__WriteToActiveOpaque ⇒ _WriteToActiveOpaque_8 ⇒ LCD__DrawBitmap_1bpp ⇒ LCD_FillRect
  [Calls]
  - >> __aeabi_i2d
  - >> __aeabi_ddiv
  - >> __aeabi_dadd
  - >> SPIx_Write_2
  - >> HAL_GPIO_WritePin
  - >> HAL_GPIO_ReadPin
  - >> GUI_SetTextMode
  - >> GUI_FillRectEx
  - >> GUI_DispStringInRectEx
  - >> GUI_Delay
  - >> GUI_Clear
  - >> BSP_LED_Toggle
  - >> ReadMAX11254Results
  - >> strlen
  - >> __aeabi_memcpy4
  [Called By]
  - >> MainTask

  ConfigureMAX11254 (Thumb, 284 bytes, Stack size 24 bytes, maintask.o(i.ConfigureMAX11254))
  [Stack]

  - Max Depth = 128
  - Call Chain = ConfigureMAX11254 ⇒ SPIx_Write_2 ⇒ SPIx_Error ⇒ SPIx_Init ⇒ SPIx_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> SPIx_Write_2
  - >> HAL_GPIO_WritePin
  [Called By]
  - >> MainTask

  ConfigureSPIandGPIO (Thumb, 124 bytes, Stack size 48 bytes, maintask.o(i.ConfigureSPIandGPIO))
  [Stack]

  - Max Depth = 136
  - Call Chain = ConfigureSPIandGPIO ⇒ SPIx_Init ⇒ SPIx_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  - >> HAL_Delay
  - >> SPIx_Init
  - >> HAL_GPIO_WritePin
  [Called By]
  - >> MainTask

  DMA2_Stream7_IRQHandler (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.DMA2_Stream7_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA2_Stream7_IRQHandler ⇒ HAL_DMA_IRQHandler
  [Calls]
  - >> HAL_DMA_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f429xx.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  FLASH_Erase_Sector (Thumb, 90 bytes, Stack size 0 bytes, stm32f4xx_hal_flash_ex.o(i.FLASH_Erase_Sector))
  [Called By]

  - >> HAL_FLASHEx_Erase

  FLASH_FlushCaches (Thumb, 80 bytes, Stack size 0 bytes, stm32f4xx_hal_flash_ex.o(i.FLASH_FlushCaches))
  [Called By]

  - >> HAL_FLASHEx_Erase

  FLASH_WaitForLastOperation (Thumb, 80 bytes, Stack size 16 bytes, stm32f4xx_hal_flash.o(i.FLASH_WaitForLastOperation))
  [Stack]

  - Max Depth = 16
  - Call Chain = FLASH_WaitForLastOperation
  [Calls]
  - >> HAL_GetTick
  - >> FLASH_SetErrorCode
  [Called By]
  - >> HAL_FLASH_Program
  - >> HAL_FLASHEx_Erase

  FMC_SDRAM_Init (Thumb, 76 bytes, Stack size 12 bytes, stm32f4xx_ll_fmc.o(i.FMC_SDRAM_Init))
  [Stack]

  - Max Depth = 12
  - Call Chain = FMC_SDRAM_Init
  [Called By]
  - >> HAL_SDRAM_Init

  FMC_SDRAM_ProgramRefreshRate (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_ll_fmc.o(i.FMC_SDRAM_ProgramRefreshRate))
  [Called By]

  - >> HAL_SDRAM_ProgramRefreshRate

  FMC_SDRAM_SendCommand (Thumb, 72 bytes, Stack size 24 bytes, stm32f4xx_ll_fmc.o(i.FMC_SDRAM_SendCommand))
  [Stack]

  - Max Depth = 24
  - Call Chain = FMC_SDRAM_SendCommand
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_SDRAM_SendCommand

  FMC_SDRAM_Timing_Init (Thumb, 124 bytes, Stack size 20 bytes, stm32f4xx_ll_fmc.o(i.FMC_SDRAM_Timing_Init))
  [Stack]

  - Max Depth = 20
  - Call Chain = FMC_SDRAM_Timing_Init
  [Called By]
  - >> HAL_SDRAM_Init

  GL_FillCircle (Thumb, 184 bytes, Stack size 40 bytes, gui_circ.o(i.GL_FillCircle))
  [Stack]

  - Max Depth = 40
  - Call Chain = GL_FillCircle
  [Called By]
  - >> GUI_FillCircle

  GL_SetDefault (Thumb, 58 bytes, Stack size 8 bytes, gui_setdefault.o(i.GL_SetDefault))
  [Stack]

  - Max Depth = 8
  - Call Chain = GL_SetDefault
  [Calls]
  - >> GUI_SetTextMode
  - >> GUI_SetFont
  - >> GUI_SetColor
  - >> GUI_SetBkColor
  - >> GUI_SetPenSize
  - >> GUI_SetTextAlign
  - >> GUI_SetLineStyle
  - >> GUI_SetDrawMode
  [Called By]
  - >> WM_SetDefault

  GUICC_M1555I_SetCustColorConv (Thumb, 8 bytes, Stack size 0 bytes, guicc_m1555i.o(i.GUICC_M1555I_SetCustColorConv))
  [Called By]

  - >> LCD_X_Config

  GUICC_M4444I_SetCustColorConv (Thumb, 8 bytes, Stack size 0 bytes, guicc_m4444i.o(i.GUICC_M4444I_SetCustColorConv))
  [Called By]

  - >> LCD_X_Config

  GUICC_M565_SetCustColorConv (Thumb, 8 bytes, Stack size 0 bytes, guicc_m565.o(i.GUICC_M565_SetCustColorConv))
  [Called By]

  - >> LCD_X_Config

  GUICC_M8888I_SetCustColorConv (Thumb, 8 bytes, Stack size 0 bytes, guicc_m8888i.o(i.GUICC_M8888I_SetCustColorConv))
  [Called By]

  - >> LCD_X_Config

  GUICC_M888_SetCustColorConv (Thumb, 8 bytes, Stack size 0 bytes, guicc_m888.o(i.GUICC_M888_SetCustColorConv))
  [Called By]

  - >> LCD_X_Config

  GUIMONO_DispChar (Thumb, 302 bytes, Stack size 104 bytes, gui_charm.o(i.GUIMONO_DispChar))
  [Stack]

  - Max Depth = 208
  - Call Chain = GUIMONO_DispChar ⇒ LCD_DrawBitmap ⇒ LCD_FillRect
  [Calls]
  - >> LCD_FillRect
  - >> LCD_SetDrawMode
  - >> LCD_DrawBitmap
  [Address Reference Count : 2]
  - f6x8.o(.constdata)
  - f8x16.o(.constdata)

  GUIMONO_GetCharDistX (Thumb, 18 bytes, Stack size 0 bytes, gui_charm.o(i.GUIMONO_GetCharDistX))
  [Address Reference Count : 2]

  - f6x8.o(.constdata)
  - f8x16.o(.constdata)

  GUIMONO_GetFontInfo (Thumb, 6 bytes, Stack size 0 bytes, gui_charm.o(i.GUIMONO_GetFontInfo))
  [Address Reference Count : 2]

  - f6x8.o(.constdata)
  - f8x16.o(.constdata)

  GUIMONO_IsInFont (Thumb, 56 bytes, Stack size 0 bytes, gui_charm.o(i.GUIMONO_IsInFont))
  [Address Reference Count : 2]

  - f6x8.o(.constdata)
  - f8x16.o(.constdata)

  GUI_ALLOC_AllocNoInit (Thumb, 10 bytes, Stack size 0 bytes, gui_alloc.o(i.GUI_ALLOC_AllocNoInit))
  [Stack]

  - Max Depth = 96
  - Call Chain = GUI_ALLOC_AllocNoInit ⇒ _Alloc ⇒ _InitOnce (Cycle)
  [Calls]
  - >> _Alloc
  [Called By]
  - >> _WriteToActiveOpaque_HT
  - >> _WriteToActiveOpaque_8
  - >> GUI_MEMDEV__CreateFixed
  - >> GUI_ALLOC_AllocZero

  GUI_ALLOC_AllocZero (Thumb, 36 bytes, Stack size 16 bytes, gui_alloc_alloczero.o(i.GUI_ALLOC_AllocZero))
  [Stack]

  - Max Depth = 112
  - Call Chain = GUI_ALLOC_AllocZero ⇒ GUI_ALLOC_AllocNoInit ⇒ _Alloc ⇒ _InitOnce (Cycle)
  [Calls]
  - >> GUI__memset
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> GUI_ALLOC_AllocNoInit
  [Called By]
  - >> WM_CreateWindowAsChild
  - >> GUI_USAGE_BM_Create
  - >> GUI_MEMDEV__CreateFixed

  GUI_ALLOC_AssignMemory (Thumb, 12 bytes, Stack size 0 bytes, gui_alloc.o(i.GUI_ALLOC_AssignMemory))
  [Called By]

  - >> GUI_X_Config

  GUI_ALLOC_Free (Thumb, 50 bytes, Stack size 8 bytes, gui_alloc.o(i.GUI_ALLOC_Free))
  [Stack]

  - Max Depth = 40
  - Call Chain = GUI_ALLOC_Free ⇒ _AddFreeMemory ⇒ _RemoveFreeBlock
  [Calls]
  - >> _PushFreeBlock
  - >> _AddFreeMemory
  [Called By]
  - >> _EnlargeBlocks
  - >> WM_DeleteWindow
  - >> _WriteToActiveOpaque_HT
  - >> _WriteToActiveOpaque_8
  - >> _GUI_USAGE_BM_Delete
  - >> GUI_TIMER_Delete
  - >> WM_DeleteTimer
  - >> GUI_USAGE_DecUseCnt
  - >> GUI_MEMDEV__CreateFixed
  - >> GUI_MEMDEV_Delete

  GUI_ALLOC_FreeFixedBlock (Thumb, 18 bytes, Stack size 0 bytes, gui_alloc.o(i.GUI_ALLOC_FreeFixedBlock))
  [Called By]

  - >> GUI_DEVICE_Delete
  - >> _OnExit
  - >> _OnExit

  GUI_ALLOC_GetFixedBlock (Thumb, 170 bytes, Stack size 24 bytes, gui_alloc.o(i.GUI_ALLOC_GetFixedBlock))
  [Stack]

  - Max Depth = 168
  - Call Chain = GUI_ALLOC_GetFixedBlock ⇒ _InitOnce ⇒ _EnlargeBlocks ⇒ _Alloc ⇒ _InitOnce (Cycle)
  [Calls]
  - >> _RemoveHoles
  - >> _RemoveFreeBlock
  - >> _InitOnce
  - >> _AddFreeMemory
  [Called By]
  - >> GUI_DEVICE_Create
  - >> GUI__GetAlphaBuffer
  - >> _InitOnce
  - >> LCD_InitColors

  GUI_ALLOC_GetMaxSize (Thumb, 58 bytes, Stack size 8 bytes, gui_alloc.o(i.GUI_ALLOC_GetMaxSize))
  [Stack]

  - Max Depth = 152
  - Call Chain = GUI_ALLOC_GetMaxSize ⇒ _InitOnce ⇒ _EnlargeBlocks ⇒ _Alloc ⇒ _InitOnce (Cycle)
  [Calls]
  - >> _InitOnce
  [Called By]
  - >> GUI_ALLOC_RequestSize

  GUI_ALLOC_LockH (Thumb, 24 bytes, Stack size 0 bytes, gui_alloc.o(i.GUI_ALLOC_LockH))
  [Calls]

  - >> GUI_ALLOC_h2p
  [Called By]
  - >> WM__InitIVRSearch
  - >> WM__DetachWindow
  - >> WM__ClipAtParentBorders
  - >> WM__ActivateClipRect
  - >> WM_InvalidateWindowAndDescsEx
  - >> WM_InvalidateRect
  - >> WM_DeleteWindow
  - >> WM_CreateWindowAsChild
  - >> _cbPaintMemDev
  - >> _SetClipRectUserIntersect
  - >> _PaintTransChildren
  - >> _Paint1Trans
  - >> _Invalidate1Abs
  - >> _Findy1
  - >> _Findx1
  - >> _Findx0
  - >> _FindNext_IVR
  - >> _Exec1Input
  - >> WM__PaintWinAndOverlays
  - >> GUI_MEMDEV__WriteToActiveAlpha
  - >> _XorPixel
  - >> _XY2PTR
  - >> _SetPixelIndex
  - >> _GetRect
  - >> _FillRect
  - >> _DrawVLine
  - >> _DrawBitmap
  - >> WM_ResizeWindow
  - >> _WriteToActiveOpaque_HT
  - >> _WriteToActiveOpaque_8
  - >> GUI_MEMDEV_WriteAt
  - >> _Unlink
  - >> _RemoveFromLinList
  - >> GUI_TIMER__GetNextTimerLin
  - >> GUI_TIMER__GetFirstTimer
  - >> GUI_TIMER_GetFlag
  - >> WM_DeleteTimer
  - >> WM_SetSize
  - >> GUI_MEMDEV_GetDataPtr
  - >> _CreateStaticDevice
  - >> GUI_MEMDEV_SetOrg
  - >> GUI_MEMDEV_ReduceYSize
  - >> GUI_MEMDEV_GetYSize
  - >> GUI_MEMDEV_Clear
  - >> GUI_USAGE_DecUseCnt
  - >> GUI_USAGE_BM_Create
  - >> GUI_MEMDEV__WriteToActiveOpaque
  - >> GUI_MEMDEV__WriteToActiveAt
  - >> GUI_MEMDEV__CreateFixed
  - >> GUI_MEMDEV_Select
  - >> GUI_MEMDEV_GetBitsPerPixel
  - >> GUI_MEMDEV_CopyToLCDAt
  - >> WM__GetClientRectEx
  - >> WM_BringToBottom
  - >> GUI_MEMDEV_Delete
  - >> GUI_ALLOC_AllocZero
  - >> WM__Paint1
  - >> WM__Paint
  - >> WM__InvalidateRect
  - >> WM__InvalidateDrawAndDescs
  - >> WM__InsertWindowIntoList
  - >> WM__MoveWindow
  - >> _MoveDescendents
  - >> WM__UpdateChildPositions

  GUI_ALLOC_RequestSize (Thumb, 36 bytes, Stack size 8 bytes, gui_alloc.o(i.GUI_ALLOC_RequestSize))
  [Stack]

  - Max Depth = 160
  - Call Chain = GUI_ALLOC_RequestSize ⇒ GUI_ALLOC_GetMaxSize ⇒ _InitOnce ⇒ _EnlargeBlocks ⇒ _Alloc ⇒ _InitOnce (Cycle)
  [Calls]
  - >> GUI_ALLOC_GetMaxSize
  [Called By]
  - >> GUI_MEMDEV__CreateFixed

  GUI_ALLOC_UnlockH (Thumb, 42 bytes, Stack size 0 bytes, gui_alloc.o(i.GUI_ALLOC_UnlockH))
  [Called By]

  - >> WM__InitIVRSearch
  - >> WM__DetachWindow
  - >> WM__ClipAtParentBorders
  - >> WM__ActivateClipRect
  - >> WM_InvalidateWindowAndDescsEx
  - >> WM_InvalidateRect
  - >> WM_DeleteWindow
  - >> WM_CreateWindowAsChild
  - >> _cbPaintMemDev
  - >> _SetClipRectUserIntersect
  - >> _PaintTransChildren
  - >> _Paint1Trans
  - >> _Invalidate1Abs
  - >> _Findy1
  - >> _Findx1
  - >> _Findx0
  - >> _FindNext_IVR
  - >> _Exec1Input
  - >> WM__PaintWinAndOverlays
  - >> GUI_MEMDEV__WriteToActiveAlpha
  - >> _XorPixel
  - >> _XY2PTR
  - >> _SetPixelIndex
  - >> _GetRect
  - >> _FillRect
  - >> _DrawVLine
  - >> _DrawBitmap
  - >> WM_ResizeWindow
  - >> _WriteToActiveOpaque_HT
  - >> _WriteToActiveOpaque_8
  - >> GUI_MEMDEV_WriteAt
  - >> _Unlink
  - >> _RemoveFromLinList
  - >> GUI_TIMER__GetNextTimerLin
  - >> GUI_TIMER__GetFirstTimer
  - >> GUI_TIMER_GetFlag
  - >> WM_DeleteTimer
  - >> WM_SetSize
  - >> GUI_MEMDEV_GetDataPtr
  - >> _CreateStaticDevice
  - >> GUI_MEMDEV_SetOrg
  - >> GUI_MEMDEV_ReduceYSize
  - >> GUI_MEMDEV_GetYSize
  - >> GUI_MEMDEV_Clear
  - >> GUI_USAGE_DecUseCnt
  - >> GUI_USAGE_BM_Create
  - >> GUI_MEMDEV__WriteToActiveOpaque
  - >> GUI_MEMDEV__WriteToActiveAt
  - >> GUI_MEMDEV__CreateFixed
  - >> GUI_MEMDEV_Select
  - >> GUI_MEMDEV_GetBitsPerPixel
  - >> GUI_MEMDEV_CopyToLCDAt
  - >> WM__GetClientRectEx
  - >> WM_BringToBottom
  - >> GUI_MEMDEV_Delete
  - >> GUI_ALLOC_AllocZero
  - >> WM__Paint1
  - >> WM__Paint
  - >> WM__InvalidateRect
  - >> WM__InvalidateDrawAndDescs
  - >> WM__InsertWindowIntoList
  - >> WM__MoveWindow
  - >> _MoveDescendents
  - >> WM__UpdateChildPositions

  GUI_ALLOC_h2p (Thumb, 20 bytes, Stack size 0 bytes, gui_alloc.o(i.GUI_ALLOC_h2p))
  [Called By]

  - >> GUI_ALLOC_LockH
  - >> WM_SelectWindow
  - >> WM_InvalidateWindowAndDescsEx
  - >> WM_DeleteWindow
  - >> WM_CreateWindowAsChild
  - >> _PaintTransChildren
  - >> _Paint1
  - >> _Invalidate1Abs
  - >> _Findy1
  - >> _Findx1
  - >> _Findx0
  - >> _FindNext_IVR
  - >> _DrawNext
  - >> WM__PaintWinAndOverlays
  - >> WM_GetWindowRect
  - >> WM__GetFirstSibling
  - >> WM__SendMessageNoPara
  - >> WM__GetPrevSibling
  - >> WM_GetParent
  - >> WM_GetWindowOrgX
  - >> _CreateStaticDevice
  - >> WM__SendMessage
  - >> WM__DeleteAssocTimer
  - >> WM_GetFirstChild
  - >> WM__RemoveWindowFromList
  - >> WM__IsWindow
  - >> WM__InvalidateRect
  - >> WM__InvalidateParent
  - >> WM__InvalidateDrawAndDescs
  - >> WM__InsertWindowIntoList
  - >> WM__GetTopLevelLayer

  GUI_CalcColorDist (Thumb, 60 bytes, Stack size 8 bytes, gui_calccolordist.o(i.GUI_CalcColorDist))
  [Stack]

  - Max Depth = 8
  - Call Chain = GUI_CalcColorDist
  [Called By]
  - >> _Color2Index_0

  GUI_Clear (Thumb, 28 bytes, Stack size 8 bytes, gui_core.o(i.GUI_Clear))
  [Stack]

  - Max Depth = 24
  - Call Chain = GUI_Clear ⇒ GUI_GotoXY
  [Calls]
  - >> GUI_GotoXY
  [Called By]
  - >> Calibration
  - >> MainTask
  - >> cbBackWin

  GUI_ClearRect (Thumb, 90 bytes, Stack size 32 bytes, gui_core.o(i.GUI_ClearRect))
  [Stack]

  - Max Depth = 168
  - Call Chain = GUI_ClearRect ⇒ WM__InitIVRSearch ⇒ WM__GetNextIVR ⇒ WM__ActivateClipRect ⇒ _SetClipRectUserIntersect ⇒ LCD_SetClipRectEx ⇒ GUI__IntersectRects
  [Calls]
  - >> LCD_FillRect
  - >> LCD_SetDrawMode
  - >> WM__InitIVRSearch
  - >> WM__GetNextIVR
  [Called By]
  - >> MainTask

  GUI_DEVICE_Create (Thumb, 76 bytes, Stack size 24 bytes, gui_device.o(i.GUI_DEVICE_Create))
  [Stack]

  - Max Depth = 192
  - Call Chain = GUI_DEVICE_Create ⇒ GUI_ALLOC_GetFixedBlock ⇒ _InitOnce ⇒ _EnlargeBlocks ⇒ _Alloc ⇒ _InitOnce (Cycle)
  [Calls]
  - >> GUI_ALLOC_GetFixedBlock
  [Called By]
  - >> GUI_DEVICE_CreateAndLink
  - >> GUI_MEMDEV__CreateFixed

  GUI_DEVICE_CreateAndLink (Thumb, 36 bytes, Stack size 16 bytes, gui_device.o(i.GUI_DEVICE_CreateAndLink))
  [Stack]

  - Max Depth = 208
  - Call Chain = GUI_DEVICE_CreateAndLink ⇒ GUI_DEVICE_Create ⇒ GUI_ALLOC_GetFixedBlock ⇒ _InitOnce ⇒ _EnlargeBlocks ⇒ _Alloc ⇒ _InitOnce (Cycle)
  [Calls]
  - >> GUI_DEVICE_Link
  - >> GUI_DEVICE_Create
  [Called By]
  - >> LCD_X_Config

  GUI_DEVICE_Delete (Thumb, 4 bytes, Stack size 0 bytes, gui_device.o(i.GUI_DEVICE_Delete))
  [Calls]

  - >> GUI_ALLOC_FreeFixedBlock
  [Called By]
  - >> GUI_MEMDEV__CreateFixed
  - >> GUI_MEMDEV_Delete

  GUI_DEVICE_Link (Thumb, 130 bytes, Stack size 16 bytes, gui_device.o(i.GUI_DEVICE_Link))
  [Stack]

  - Max Depth = 16
  - Call Chain = GUI_DEVICE_Link
  [Called By]
  - >> GUI_DEVICE_CreateAndLink
  - >> GUI_MEMDEV_Select

  GUI_DEVICE_Unlink (Thumb, 4 bytes, Stack size 0 bytes, gui_device.o(i.GUI_DEVICE_Unlink))
  [Calls]

  - >> _UnlinkDevice
  [Called By]
  - >> LCD_SelectLCD

  GUI_DEVICE__GetpDriver (Thumb, 32 bytes, Stack size 0 bytes, gui_device.o(i.GUI_DEVICE__GetpDriver))
  [Called By]

  - >> LCD_SetVSizeEx
  - >> LCD_SetVRAMAddrEx
  - >> LCD_SetSizeEx
  - >> LCD_SetDevFunc
  - >> emWin_LCD_Init
  - >> WM_Init
  - >> LCD_GetPaletteEx
  - >> _GetDevProp
  - >> LCD_SetLUTEntryEx
  - >> LCD_GetNumLayers
  - >> LCD_InitLUT
  - >> LCD_GetPosEx
  - >> GUI_MEMDEV_CreateEx
  - >> GUI__ManageCacheEx

  GUI_Delay (Thumb, 42 bytes, Stack size 16 bytes, gui_time.o(i.GUI_Delay))
  [Stack]

  - Max Depth = 680
  - Call Chain = GUI_Delay ⇒ GUI_Exec ⇒ GUI_Exec1 ⇒ WM_Exec ⇒ _DrawNext ⇒ WM__Paint ⇒ GUI_MEMDEV_Draw ⇒ GUI_MEMDEV_CopyToLCD ⇒ GUI_MEMDEV_CopyToLCDAt ⇒ GUI_MEMDEV__WriteToActiveOpaque ⇒ _WriteToActiveOpaque_8 ⇒ LCD__DrawBitmap_1bpp ⇒ LCD_FillRect
  [Calls]
  - >> GUI_X_GetTime
  - >> GUI_X_Delay
  - >> GUI_Exec
  [Called By]
  - >> Calibration

  GUI_DispStringInRectEx (Thumb, 122 bytes, Stack size 48 bytes, gui_dispstringinrectex.o(i.GUI_DispStringInRectEx))
  [Stack]

  - Max Depth = 312
  - Call Chain = GUI_DispStringInRectEx ⇒ GUI_DispStringInRectMax ⇒ GUI__DispStringInRect ⇒ GUI__DispLine ⇒ WM__InitIVRSearch ⇒ WM__GetNextIVR ⇒ WM__ActivateClipRect ⇒ _SetClipRectUserIntersect ⇒ LCD_SetClipRectEx ⇒ GUI__IntersectRects
  [Calls]
  - >> WM_SetUserClipRect
  - >> GUI__IntersectRects
  - >> GUI__DispStringInRect
  - >> GUI_DispStringInRectMax
  - >> _SetRotation
  [Called By]
  - >> Calibration
  - >> MainTask

  GUI_DispStringInRectMax (Thumb, 68 bytes, Stack size 32 bytes, gui_dispstringinrect.o(i.GUI_DispStringInRectMax))
  [Stack]

  - Max Depth = 264
  - Call Chain = GUI_DispStringInRectMax ⇒ GUI__DispStringInRect ⇒ GUI__DispLine ⇒ WM__InitIVRSearch ⇒ WM__GetNextIVR ⇒ WM__ActivateClipRect ⇒ _SetClipRectUserIntersect ⇒ LCD_SetClipRectEx ⇒ GUI__IntersectRects
  [Calls]
  - >> WM_SetUserClipRect
  - >> GUI__IntersectRects
  - >> GUI__DispStringInRect
  [Called By]
  - >> GUI_DispStringInRectEx

  GUI_Exec (Thumb, 20 bytes, Stack size 8 bytes, gui_exec.o(i.GUI_Exec))
  [Stack]

  - Max Depth = 664
  - Call Chain = GUI_Exec ⇒ GUI_Exec1 ⇒ WM_Exec ⇒ _DrawNext ⇒ WM__Paint ⇒ GUI_MEMDEV_Draw ⇒ GUI_MEMDEV_CopyToLCD ⇒ GUI_MEMDEV_CopyToLCDAt ⇒ GUI_MEMDEV__WriteToActiveOpaque ⇒ _WriteToActiveOpaque_8 ⇒ LCD__DrawBitmap_1bpp ⇒ LCD_FillRect
  [Calls]
  - >> GUI_Exec1
  [Called By]
  - >> GUI_Delay

  GUI_Exec1 (Thumb, 40 bytes, Stack size 8 bytes, gui_exec.o(i.GUI_Exec1))
  [Stack]

  - Max Depth = 656
  - Call Chain = GUI_Exec1 ⇒ WM_Exec ⇒ _DrawNext ⇒ WM__Paint ⇒ GUI_MEMDEV_Draw ⇒ GUI_MEMDEV_CopyToLCD ⇒ GUI_MEMDEV_CopyToLCDAt ⇒ GUI_MEMDEV__WriteToActiveOpaque ⇒ _WriteToActiveOpaque_8 ⇒ LCD__DrawBitmap_1bpp ⇒ LCD_FillRect
  [Calls]
  - >> WM_Exec
  [Called By]
  - >> GUI_Exec

  GUI_FillCircle (Thumb, 44 bytes, Stack size 16 bytes, gui_circ.o(i.GUI_FillCircle))
  [Stack]

  - Max Depth = 152
  - Call Chain = GUI_FillCircle ⇒ WM__InitIVRSearch ⇒ WM__GetNextIVR ⇒ WM__ActivateClipRect ⇒ _SetClipRectUserIntersect ⇒ LCD_SetClipRectEx ⇒ GUI__IntersectRects
  [Calls]
  - >> WM__InitIVRSearch
  - >> WM__GetNextIVR
  - >> GL_FillCircle
  [Called By]
  - >> MainTask

  GUI_FillRect (Thumb, 68 bytes, Stack size 32 bytes, gui_fillrect.o(i.GUI_FillRect))
  [Stack]

  - Max Depth = 168
  - Call Chain = GUI_FillRect ⇒ WM__InitIVRSearch ⇒ WM__GetNextIVR ⇒ WM__ActivateClipRect ⇒ _SetClipRectUserIntersect ⇒ LCD_SetClipRectEx ⇒ GUI__IntersectRects
  [Calls]
  - >> LCD_FillRect
  - >> WM__InitIVRSearch
  - >> WM__GetNextIVR
  [Called By]
  - >> GUI_FillRectEx

  GUI_FillRectEx (Thumb, 20 bytes, Stack size 0 bytes, gui_fillrectex.o(i.GUI_FillRectEx))
  [Stack]

  - Max Depth = 168
  - Call Chain = GUI_FillRectEx ⇒ GUI_FillRect ⇒ WM__InitIVRSearch ⇒ WM__GetNextIVR ⇒ WM__ActivateClipRect ⇒ _SetClipRectUserIntersect ⇒ LCD_SetClipRectEx ⇒ GUI__IntersectRects
  [Calls]
  - >> GUI_FillRect
  [Called By]
  - >> Calibration
  - >> MainTask

  GUI_GetBitsPerPixelEx (Thumb, 14 bytes, Stack size 0 bytes, lcd_getex.o(i.GUI_GetBitsPerPixelEx))
  [Called By]

  - >> GUI__DoAlphaBlending
  - >> LCD_ReadRectEx
  - >> _WriteToActiveOpaque_HT
  - >> _WriteToActiveOpaque_8

  GUI_GetCharDistX (Thumb, 12 bytes, Stack size 0 bytes, gui_char.o(i.GUI_GetCharDistX))
  [Called By]

  - >> GUI__GetLineDistX

  GUI_GetCharDistXEx (Thumb, 10 bytes, Stack size 0 bytes, gui_char.o(i.GUI_GetCharDistXEx))
  [Called By]

  - >> GUI__GetOverlap

  GUI_GetClientRect (Thumb, 10 bytes, Stack size 0 bytes, gui_getclientrect.o(i.GUI_GetClientRect))
  [Stack]

  - Max Depth = 16
  - Call Chain = GUI_GetClientRect ⇒ WM_GetClientRect ⇒ WM_GetClientRectEx ⇒ WM__GetClientRectEx
  [Calls]
  - >> WM_GetClientRect
  [Called By]
  - >> GUI__DispStringInRect

  GUI_GetDrawMode (Thumb, 8 bytes, Stack size 0 bytes, gui_getdrawmode.o(i.GUI_GetDrawMode))
  [Called By]

  - >> CUSTOM_FillRect

  GUI_GetFontDistY (Thumb, 10 bytes, Stack size 0 bytes, gui_char.o(i.GUI_GetFontDistY))
  [Called By]

  - >> GUI__DispStringInRect

  GUI_GetLayerPosEx (Thumb, 22 bytes, Stack size 16 bytes, gui_selectlayer.o(i.GUI_GetLayerPosEx))
  [Stack]

  - Max Depth = 40
  - Call Chain = GUI_GetLayerPosEx ⇒ LCD_GetPosEx
  [Calls]
  - >> LCD_GetPosEx
  [Called By]
  - >> LCD_X_DisplayDriver

  GUI_GetOrg (Thumb, 4 bytes, Stack size 0 bytes, gui_getorg.o(i.GUI_GetOrg))
  [Calls]

  - >> GUI__GetOrg
  [Called By]
  - >> GUI_MEMDEV_Draw

  GUI_GetpfColor2IndexEx (Thumb, 12 bytes, Stack size 0 bytes, lcd_getex.o(i.GUI_GetpfColor2IndexEx))
  [Called By]

  - >> _WriteToActiveOpaque_8

  GUI_GetpfIndex2ColorEx (Thumb, 12 bytes, Stack size 0 bytes, lcd_getex.o(i.GUI_GetpfIndex2ColorEx))
  [Called By]

  - >> GUI__DoAlphaBlending
  - >> _WriteToActiveOpaque_8

  GUI_GotoXY (Thumb, 20 bytes, Stack size 16 bytes, gui_goto.o(i.GUI_GotoXY))
  [Stack]

  - Max Depth = 16
  - Call Chain = GUI_GotoXY
  [Calls]
  - >> _GotoY
  - >> _GotoX
  [Called By]
  - >> GUI_Clear

  GUI_Init (Thumb, 74 bytes, Stack size 8 bytes, gui_core.o(i.GUI_Init))
  [Stack]

  - Max Depth = 320
  - Call Chain = GUI_Init ⇒ WM_Init ⇒ WM_CreateWindowAsChild ⇒ WM__SendMsgNoData ⇒ WM__SendMessage ⇒ WM_DefaultProc ⇒ WM_InvalidateWindow ⇒ WM_InvalidateRect ⇒ WM__InvalidateRectEx ⇒ WM__InvalidateRect ⇒ WM__InvalidateRect (Cycle)
  [Calls]
  - >> emWin_LCD_Init
  - >> WM_Init
  - >> GUI_SetOrg
  - >> GUI__Config
  - >> _InitContext
  - >> GUI_X_Init
  [Called By]
  - >> main

  GUI_MEMDEV_Clear (Thumb, 54 bytes, Stack size 16 bytes, guidev_clear.o(i.GUI_MEMDEV_Clear))
  [Stack]

  - Max Depth = 16
  - Call Chain = GUI_MEMDEV_Clear
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  [Called By]
  - >> GUI_MEMDEV_Draw

  GUI_MEMDEV_CopyToLCD (Thumb, 8 bytes, Stack size 0 bytes, guidev.o(i.GUI_MEMDEV_CopyToLCD))
  [Stack]

  - Max Depth = 368
  - Call Chain = GUI_MEMDEV_CopyToLCD ⇒ GUI_MEMDEV_CopyToLCDAt ⇒ GUI_MEMDEV__WriteToActiveOpaque ⇒ _WriteToActiveOpaque_8 ⇒ LCD__DrawBitmap_1bpp ⇒ LCD_FillRect
  [Calls]
  - >> GUI_MEMDEV_CopyToLCDAt
  [Called By]
  - >> GUI_MEMDEV_Draw

  GUI_MEMDEV_CopyToLCDAt (Thumb, 156 bytes, Stack size 56 bytes, guidev.o(i.GUI_MEMDEV_CopyToLCDAt))
  [Stack]

  - Max Depth = 368
  - Call Chain = GUI_MEMDEV_CopyToLCDAt ⇒ GUI_MEMDEV__WriteToActiveOpaque ⇒ _WriteToActiveOpaque_8 ⇒ LCD__DrawBitmap_1bpp ⇒ LCD_FillRect
  [Calls]
  - >> WM__InitIVRSearch
  - >> WM__GetNextIVR
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> WM_Activate
  - >> GUI_SelectLayer
  - >> GUI_MEMDEV__WriteToActiveOpaque
  - >> GUI_MEMDEV_Select
  - >> GUI_SetDrawMode
  [Called By]
  - >> GUI_MEMDEV_CopyToLCD

  GUI_MEMDEV_CreateEx (Thumb, 108 bytes, Stack size 48 bytes, guidev.o(i.GUI_MEMDEV_CreateEx))
  [Stack]

  - Max Depth = 304
  - Call Chain = GUI_MEMDEV_CreateEx ⇒ GUI_MEMDEV__CreateFixed ⇒ GUI_DEVICE_Create ⇒ GUI_ALLOC_GetFixedBlock ⇒ _InitOnce ⇒ _EnlargeBlocks ⇒ _Alloc ⇒ _InitOnce (Cycle)
  [Calls]
  - >> GUI_DEVICE__GetpDriver
  - >> GUI_MEMDEV__CreateFixed
  [Called By]
  - >> GUI_MEMDEV_Draw

  GUI_MEMDEV_Delete (Thumb, 58 bytes, Stack size 16 bytes, guidev.o(i.GUI_MEMDEV_Delete))
  [Stack]

  - Max Depth = 72
  - Call Chain = GUI_MEMDEV_Delete ⇒ GUI_USAGE_DecUseCnt ⇒ GUI_ALLOC_Free ⇒ _AddFreeMemory ⇒ _RemoveFreeBlock
  [Calls]
  - >> GUI_DEVICE_Delete
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> GUI_ALLOC_Free
  - >> GUI_SelectLCD
  - >> GUI_USAGE_DecUseCnt
  [Called By]
  - >> WM_DeleteWindow
  - >> GUI_MEMDEV_Draw
  - >> WM__InvalidateDrawAndDescs

  GUI_MEMDEV_Draw (Thumb, 286 bytes, Stack size 64 bytes, guidev_banding.o(i.GUI_MEMDEV_Draw))
  [Stack]

  - Max Depth = 432
  - Call Chain = GUI_MEMDEV_Draw ⇒ GUI_MEMDEV_CopyToLCD ⇒ GUI_MEMDEV_CopyToLCDAt ⇒ GUI_MEMDEV__WriteToActiveOpaque ⇒ _WriteToActiveOpaque_8 ⇒ LCD__DrawBitmap_1bpp ⇒ LCD_FillRect
  [Calls]
  - >> LCD_GetYSizeEx
  - >> LCD_GetXSizeEx
  - >> LCD_GetVYSizeEx
  - >> LCD_GetVXSizeEx
  - >> GUI_MEMDEV_SetOrg
  - >> GUI_MEMDEV_ReduceYSize
  - >> GUI_MEMDEV_GetYSize
  - >> GUI_MEMDEV_Clear
  - >> GUI_GetOrg
  - >> _Min
  - >> GUI_MEMDEV_Select
  - >> GUI_MEMDEV_CreateEx
  - >> GUI_MEMDEV_CopyToLCD
  - >> GUI_MEMDEV_Delete
  [Called By]
  - >> WM__Paint

  GUI_MEMDEV_GetBitsPerPixel (Thumb, 36 bytes, Stack size 16 bytes, guidev.o(i.GUI_MEMDEV_GetBitsPerPixel))
  [Stack]

  - Max Depth = 20
  - Call Chain = GUI_MEMDEV_GetBitsPerPixel ⇒ LCD__GetBPPDevice
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> LCD__GetBPPDevice
  [Called By]
  - >> GUI_MEMDEV__WriteToActiveOpaque

  GUI_MEMDEV_GetDataPtr (Thumb, 26 bytes, Stack size 16 bytes, guidev_getdataptr.o(i.GUI_MEMDEV_GetDataPtr))
  [Stack]

  - Max Depth = 16
  - Call Chain = GUI_MEMDEV_GetDataPtr
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  [Called By]
  - >> GUI_MEMDEV__WriteToActiveAlpha
  - >> _WriteToActiveOpaque_8
  - >> _CreateStaticDevice

  GUI_MEMDEV_GetYSize (Thumb, 34 bytes, Stack size 16 bytes, guidev_getysize.o(i.GUI_MEMDEV_GetYSize))
  [Stack]

  - Max Depth = 16
  - Call Chain = GUI_MEMDEV_GetYSize
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  [Called By]
  - >> GUI_MEMDEV_Draw

  GUI_MEMDEV_Paint1Static (Thumb, 30 bytes, Stack size 16 bytes, guidev_staticdevices.o(i.GUI_MEMDEV_Paint1Static))
  [Stack]

  - Max Depth = 528
  - Call Chain = GUI_MEMDEV_Paint1Static ⇒ _CreateStaticDevice ⇒ WM_SetSize ⇒ WM_ResizeWindow ⇒ WM__UpdateChildPositions ⇒ WM_ResizeWindow (Cycle)
  [Calls]
  - >> GUI_MEMDEV_Write
  - >> _CreateStaticDevice
  [Address Reference Count : 1]
  - wm.o(i._Paint1)

  GUI_MEMDEV_ReduceYSize (Thumb, 40 bytes, Stack size 16 bytes, guidev_reduceysize.o(i.GUI_MEMDEV_ReduceYSize))
  [Stack]

  - Max Depth = 16
  - Call Chain = GUI_MEMDEV_ReduceYSize
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  [Called By]
  - >> GUI_MEMDEV_Draw

  GUI_MEMDEV_Select (Thumb, 64 bytes, Stack size 24 bytes, guidev.o(i.GUI_MEMDEV_Select))
  [Stack]

  - Max Depth = 40
  - Call Chain = GUI_MEMDEV_Select ⇒ GUI_DEVICE_Link
  [Calls]
  - >> GUI_DEVICE_Link
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> WM_Deactivate
  - >> LCD_UpdateColorIndices
  - >> LCD_SetClipRectMax
  - >> GUI_SelectLCD
  [Called By]
  - >> _CreateStaticDevice
  - >> GUI_MEMDEV_CopyToLCDAt
  - >> GUI_MEMDEV_Draw

  GUI_MEMDEV_SetOrg (Thumb, 84 bytes, Stack size 24 bytes, guidev_setorg.o(i.GUI_MEMDEV_SetOrg))
  [Stack]

  - Max Depth = 24
  - Call Chain = GUI_MEMDEV_SetOrg
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> LCD_SetClipRectMax
  [Called By]
  - >> _CreateStaticDevice
  - >> GUI_MEMDEV_Draw

  GUI_MEMDEV_Write (Thumb, 8 bytes, Stack size 0 bytes, guidev_write.o(i.GUI_MEMDEV_Write))
  [Stack]

  - Max Depth = 168
  - Call Chain = GUI_MEMDEV_Write ⇒ GUI_MEMDEV_WriteAt ⇒ WM__InitIVRSearch ⇒ WM__GetNextIVR ⇒ WM__ActivateClipRect ⇒ _SetClipRectUserIntersect ⇒ LCD_SetClipRectEx ⇒ GUI__IntersectRects
  [Calls]
  - >> GUI_MEMDEV_WriteAt
  [Called By]
  - >> GUI_MEMDEV_Paint1Static

  GUI_MEMDEV_WriteAt (Thumb, 94 bytes, Stack size 32 bytes, guidev_write.o(i.GUI_MEMDEV_WriteAt))
  [Stack]

  - Max Depth = 168
  - Call Chain = GUI_MEMDEV_WriteAt ⇒ WM__InitIVRSearch ⇒ WM__GetNextIVR ⇒ WM__ActivateClipRect ⇒ _SetClipRectUserIntersect ⇒ LCD_SetClipRectEx ⇒ GUI__IntersectRects
  [Calls]
  - >> WM__InitIVRSearch
  - >> WM__GetNextIVR
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> GUI_MEMDEV__WriteToActiveAt
  [Called By]
  - >> GUI_MEMDEV_Write

  GUI_MEMDEV__CreateFixed (Thumb, 238 bytes, Stack size 64 bytes, guidev.o(i.GUI_MEMDEV__CreateFixed))
  [Stack]

  - Max Depth = 256
  - Call Chain = GUI_MEMDEV__CreateFixed ⇒ GUI_DEVICE_Create ⇒ GUI_ALLOC_GetFixedBlock ⇒ _InitOnce ⇒ _EnlargeBlocks ⇒ _Alloc ⇒ _InitOnce (Cycle)
  [Calls]
  - >> GUI_DEVICE_Delete
  - >> GUI_DEVICE_Create
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_RequestSize
  - >> GUI_ALLOC_LockH
  - >> GUI_ALLOC_Free
  - >> GUI_ALLOC_AllocNoInit
  - >> LCD__GetBPPDevice
  - >> GUI_USAGE_BM_Create
  - >> GUI_ALLOC_AllocZero
  [Called By]
  - >> _CreateStaticDevice
  - >> GUI_MEMDEV_CreateEx

  GUI_MEMDEV__WriteToActiveAlpha (Thumb, 386 bytes, Stack size 104 bytes, guidev_writetoactivealpha.o(i.GUI_MEMDEV__WriteToActiveAlpha))
  [Stack]

  - Max Depth = 408
  - Call Chain = GUI_MEMDEV__WriteToActiveAlpha ⇒ GUI__DoAlphaBlending ⇒ GUI__GetAlphaBuffer ⇒ GUI_ALLOC_GetFixedBlock ⇒ _InitOnce ⇒ _EnlargeBlocks ⇒ _Alloc ⇒ _InitOnce (Cycle)
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> GUI__DoAlphaBlending
  - >> GUI__AllocAlphaBuffer
  - >> LCD_DrawBitmap
  - >> GUI__CompactPixelIndicesEx
  - >> GUI_MEMDEV_GetDataPtr
  [Address Reference Count : 1]
  - guidev_32.o(i._GetDevFunc)

  GUI_MEMDEV__WriteToActiveAt (Thumb, 48 bytes, Stack size 24 bytes, guidev.o(i.GUI_MEMDEV__WriteToActiveAt))
  [Stack]

  - Max Depth = 24
  - Call Chain = GUI_MEMDEV__WriteToActiveAt
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  [Called By]
  - >> GUI_MEMDEV_WriteAt

  GUI_MEMDEV__WriteToActiveOpaque (Thumb, 60 bytes, Stack size 24 bytes, guidev_writetoactiveopaque.o(i.GUI_MEMDEV__WriteToActiveOpaque))
  [Stack]

  - Max Depth = 312
  - Call Chain = GUI_MEMDEV__WriteToActiveOpaque ⇒ _WriteToActiveOpaque_8 ⇒ LCD__DrawBitmap_1bpp ⇒ LCD_FillRect
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> _WriteToActiveOpaque_HT
  - >> _WriteToActiveOpaque_8
  - >> GUI_MEMDEV_GetBitsPerPixel
  [Called By]
  - >> GUI_MEMDEV_CopyToLCDAt

  GUI_MULTIBUF_ConfirmEx (Thumb, 38 bytes, Stack size 0 bytes, gui_multibuf.o(i.GUI_MULTIBUF_ConfirmEx))
  [Called By]

  - >> HAL_LTDC_LineEventCallback

  GUI_MergeRect (Thumb, 88 bytes, Stack size 8 bytes, gui_mergerect.o(i.GUI_MergeRect))
  [Stack]

  - Max Depth = 8
  - Call Chain = GUI_MergeRect
  [Called By]
  - >> _Invalidate1Abs
  - >> WM_ResizeWindow

  GUI_MoveRect (Thumb, 30 bytes, Stack size 0 bytes, gui_moverect.o(i.GUI_MoveRect))
  [Called By]

  - >> WM__Client2Screen
  - >> WM__MoveWindow
  - >> _MoveDescendents

  GUI_PollKeyMsg (Thumb, 38 bytes, Stack size 16 bytes, gui_onkey.o(i.GUI_PollKeyMsg))
  [Stack]

  - Max Depth = 232
  - Call Chain = GUI_PollKeyMsg ⇒ WM_OnKey ⇒ WM__SendMessage ⇒ WM_DefaultProc ⇒ WM_InvalidateWindow ⇒ WM_InvalidateRect ⇒ WM__InvalidateRectEx ⇒ WM__InvalidateRect ⇒ WM__InvalidateRect (Cycle)
  [Calls]
  - >> WM_OnKey
  - >> _IncReadPointer
  [Called By]
  - >> _Exec1Input

  GUI_ReadRectEx (Thumb, 92 bytes, Stack size 32 bytes, lcd_readrect.o(i.GUI_ReadRectEx))
  [Stack]

  - Max Depth = 96
  - Call Chain = GUI_ReadRectEx ⇒ LCD_ReadRectEx
  [Calls]
  - >> LCD_ReadRectEx
  [Called By]
  - >> GUI__DoAlphaBlending

  GUI_RectsIntersect (Thumb, 56 bytes, Stack size 0 bytes, gui_rectsintersect.o(i.GUI_RectsIntersect))
  [Called By]

  - >> _PaintTransChildren
  - >> _Paint1Trans
  - >> _Findy1
  - >> _Findx1
  - >> _Findx0
  - >> _DispLine

  GUI_RestoreContext (Thumb, 12 bytes, Stack size 0 bytes, gui_savecontext.o(i.GUI_RestoreContext))
  [Stack]

  - Max Depth = 8
  - Call Chain = GUI_RestoreContext ⇒ __aeabi_memcpy4
  [Calls]
  - >> __aeabi_memcpy4
  [Called By]
  - >> _DrawNext

  GUI_SaveContext_W (Thumb, 10 bytes, Stack size 0 bytes, gui_savecontext.o(i.GUI_SaveContext_W))
  [Stack]

  - Max Depth = 8
  - Call Chain = GUI_SaveContext_W ⇒ __aeabi_memcpy4
  [Calls]
  - >> __aeabi_memcpy4
  [Called By]
  - >> _DrawNext

  GUI_SelectLCD (Thumb, 18 bytes, Stack size 8 bytes, gui_selectlcd.o(i.GUI_SelectLCD))
  [Stack]

  - Max Depth = 16
  - Call Chain = GUI_SelectLCD ⇒ LCD_UpdateColorIndices
  [Calls]
  - >> WM_Activate
  - >> LCD_UpdateColorIndices
  - >> LCD_SelectLCD
  [Called By]
  - >> GUI_SelectLayer
  - >> GUI_MEMDEV_Select
  - >> GUI_MEMDEV_Delete

  GUI_SelectLayer (Thumb, 28 bytes, Stack size 16 bytes, gui_selectlayer.o(i.GUI_SelectLayer))
  [Stack]

  - Max Depth = 32
  - Call Chain = GUI_SelectLayer ⇒ GUI_SelectLCD ⇒ LCD_UpdateColorIndices
  [Calls]
  - >> GUI_SelectLCD
  [Called By]
  - >> emWin_LCD_Init
  - >> GUI_MEMDEV_CopyToLCDAt
  - >> WM__SelectTopLevelLayer

  GUI_SetBkColor (Thumb, 4 bytes, Stack size 0 bytes, gui_setcolor.o(i.GUI_SetBkColor))
  [Calls]

  - >> LCD_SetBkColor
  [Called By]
  - >> cbBackWin
  - >> _DrawNext
  - >> GL_SetDefault

  GUI_SetColor (Thumb, 4 bytes, Stack size 0 bytes, gui_setcolor.o(i.GUI_SetColor))
  [Calls]

  - >> LCD_SetColor
  [Called By]
  - >> _DrawNext
  - >> GL_SetDefault

  GUI_SetDefaultFont (Thumb, 6 bytes, Stack size 0 bytes, gui_core.o(i.GUI_SetDefaultFont))
  [Called By]

  - >> GUI_X_Config

  GUI_SetDrawMode (Thumb, 4 bytes, Stack size 0 bytes, gui_setdrawmode.o(i.GUI_SetDrawMode))
  [Calls]

  - >> LCD_SetDrawMode
  [Called By]
  - >> GUI_MEMDEV_CopyToLCDAt
  - >> GL_SetDefault

  GUI_SetFont (Thumb, 14 bytes, Stack size 0 bytes, gui_setfont.o(i.GUI_SetFont))
  [Called By]

  - >> MainTask
  - >> GL_SetDefault

  GUI_SetFuncAlphaBlending (Thumb, 6 bytes, Stack size 0 bytes, gui__alpha.o(i.GUI_SetFuncAlphaBlending))
  [Called By]

  - >> LCD_X_Config

  GUI_SetFuncGetpPalConvTable (Thumb, 6 bytes, Stack size 0 bytes, gui_core.o(i.GUI_SetFuncGetpPalConvTable))
  [Called By]

  - >> LCD_X_Config

  GUI_SetFuncMixColors (Thumb, 6 bytes, Stack size 0 bytes, gui__alpha.o(i.GUI_SetFuncMixColors))
  [Called By]

  - >> LCD_X_Config

  GUI_SetFuncMixColorsBulk (Thumb, 6 bytes, Stack size 0 bytes, gui__alpha.o(i.GUI_SetFuncMixColorsBulk))
  [Called By]

  - >> LCD_X_Config

  GUI_SetLineStyle (Thumb, 12 bytes, Stack size 0 bytes, gui_setlinestyle.o(i.GUI_SetLineStyle))
  [Called By]

  - >> GL_SetDefault

  GUI_SetOrg (Thumb, 38 bytes, Stack size 8 bytes, gui_setorg.o(i.GUI_SetOrg))
  [Stack]

  - Max Depth = 8
  - Call Chain = GUI_SetOrg
  [Called By]
  - >> GUI_Init

  GUI_SetPenSize (Thumb, 12 bytes, Stack size 0 bytes, gui_pen.o(i.GUI_SetPenSize))
  [Called By]

  - >> GL_SetDefault

  GUI_SetTextAlign (Thumb, 14 bytes, Stack size 0 bytes, gui_settextalign.o(i.GUI_SetTextAlign))
  [Called By]

  - >> GL_SetDefault

  GUI_SetTextMode (Thumb, 14 bytes, Stack size 0 bytes, gui_settextmode.o(i.GUI_SetTextMode))
  [Called By]

  - >> Calibration
  - >> MainTask
  - >> GL_SetDefault

  GUI_SignalEvent (Thumb, 12 bytes, Stack size 0 bytes, gui_waitevent.o(i.GUI_SignalEvent))
  [Called By]

  - >> _Invalidate1Abs
  - >> GUI_StoreKey

  GUI_StoreKey (Thumb, 12 bytes, Stack size 0 bytes, gui_onkey.o(i.GUI_StoreKey))
  [Calls]

  - >> GUI_SignalEvent
  [Called By]
  - >> cbBackWin

  GUI_TIMER_Delete (Thumb, 28 bytes, Stack size 8 bytes, gui_timer.o(i.GUI_TIMER_Delete))
  [Stack]

  - Max Depth = 48
  - Call Chain = GUI_TIMER_Delete ⇒ GUI_ALLOC_Free ⇒ _AddFreeMemory ⇒ _RemoveFreeBlock
  [Calls]
  - >> GUI_ALLOC_Free
  - >> _Unlink
  - >> _RemoveFromLinList
  [Called By]
  - >> WM_DeleteTimer

  GUI_TIMER_GetFlag (Thumb, 38 bytes, Stack size 16 bytes, gui_timer.o(i.GUI_TIMER_GetFlag))
  [Stack]

  - Max Depth = 16
  - Call Chain = GUI_TIMER_GetFlag
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  [Called By]
  - >> WM__DeleteAssocTimer

  GUI_TIMER__GetFirstTimer (Thumb, 36 bytes, Stack size 16 bytes, gui_timer.o(i.GUI_TIMER__GetFirstTimer))
  [Stack]

  - Max Depth = 16
  - Call Chain = GUI_TIMER__GetFirstTimer
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  [Called By]
  - >> WM__DeleteAssocTimer

  GUI_TIMER__GetNextTimerLin (Thumb, 54 bytes, Stack size 16 bytes, gui_timer.o(i.GUI_TIMER__GetNextTimerLin))
  [Stack]

  - Max Depth = 16
  - Call Chain = GUI_TIMER__GetNextTimerLin
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  [Called By]
  - >> WM__DeleteAssocTimer

  GUI_UC__GetCharCodeInc (Thumb, 38 bytes, Stack size 24 bytes, gui_uc.o(i.GUI_UC__GetCharCodeInc))
  [Stack]

  - Max Depth = 24
  - Call Chain = GUI_UC__GetCharCodeInc
  [Called By]
  - >> GUI__GetLineNumChars
  - >> GUI__GetLineDistX
  - >> _DispLine

  GUI_UC__NumChars2NumBytes (Thumb, 36 bytes, Stack size 24 bytes, gui_uc.o(i.GUI_UC__NumChars2NumBytes))
  [Stack]

  - Max Depth = 24
  - Call Chain = GUI_UC__NumChars2NumBytes
  [Called By]
  - >> GUI__DispStringInRect

  GUI_USAGE_AddRect (Thumb, 40 bytes, Stack size 24 bytes, guidev_usage.o(i.GUI_USAGE_AddRect))
  [Stack]

  - Max Depth = 24
  - Call Chain = GUI_USAGE_AddRect
  [Called By]
  - >> _FillRect
  - >> _DrawBitmap

  GUI_USAGE_BM_Create (Thumb, 78 bytes, Stack size 32 bytes, guidev_usagebm.o(i.GUI_USAGE_BM_Create))
  [Stack]

  - Max Depth = 144
  - Call Chain = GUI_USAGE_BM_Create ⇒ GUI_ALLOC_AllocZero ⇒ GUI_ALLOC_AllocNoInit ⇒ _Alloc ⇒ _InitOnce (Cycle)
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> GUI_ALLOC_AllocZero
  [Called By]
  - >> GUI_MEMDEV__CreateFixed

  GUI_USAGE_DecUseCnt (Thumb, 36 bytes, Stack size 16 bytes, guidev_usage.o(i.GUI_USAGE_DecUseCnt))
  [Stack]

  - Max Depth = 56
  - Call Chain = GUI_USAGE_DecUseCnt ⇒ GUI_ALLOC_Free ⇒ _AddFreeMemory ⇒ _RemoveFreeBlock
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> GUI_ALLOC_Free
  [Called By]
  - >> GUI_MEMDEV_Delete

  GUI_X_Config (Thumb, 22 bytes, Stack size 8 bytes, guiconf_1.o(i.GUI_X_Config))
  [Stack]

  - Max Depth = 8
  - Call Chain = GUI_X_Config
  [Calls]
  - >> GUI_SetDefaultFont
  - >> GUI_ALLOC_AssignMemory
  [Called By]
  - >> GUI__Config

  GUI_X_Delay (Thumb, 16 bytes, Stack size 0 bytes, gui_x.o(i.GUI_X_Delay))
  [Called By]

  - >> GUI_Delay

  GUI_X_ExecIdle (Thumb, 2 bytes, Stack size 0 bytes, gui_x.o(i.GUI_X_ExecIdle))
  [Address Reference Count : 1]

  - gui_waitevent.o(.data)

  GUI_X_GetTime (Thumb, 6 bytes, Stack size 0 bytes, gui_x.o(i.GUI_X_GetTime))
  [Called By]

  - >> GUI_Delay

  GUI_X_Init (Thumb, 2 bytes, Stack size 0 bytes, gui_x.o(i.GUI_X_Init))
  [Called By]

  - >> GUI_Init

  GUI__AllocAlphaBuffer (Thumb, 22 bytes, Stack size 16 bytes, gui__alpha.o(i.GUI__AllocAlphaBuffer))
  [Stack]

  - Max Depth = 216
  - Call Chain = GUI__AllocAlphaBuffer ⇒ GUI__GetAlphaBuffer ⇒ GUI_ALLOC_GetFixedBlock ⇒ _InitOnce ⇒ _EnlargeBlocks ⇒ _Alloc ⇒ _InitOnce (Cycle)
  [Calls]
  - >> GUI__GetAlphaBuffer
  [Called By]
  - >> GUI_MEMDEV__WriteToActiveAlpha

  GUI__AlphaSuppressMixing (Thumb, 32 bytes, Stack size 8 bytes, gui_setalpha.o(i.GUI__AlphaSuppressMixing))
  [Stack]

  - Max Depth = 8
  - Call Chain = GUI__AlphaSuppressMixing
  [Calls]
  - >> LCD_AA_SetAndMask
  [Called By]
  - >> _CreateStaticDevice

  GUI__CompactPixelIndices (Thumb, 292 bytes, Stack size 8 bytes, gui__compactpixelindices.o(i.GUI__CompactPixelIndices))
  [Stack]

  - Max Depth = 8
  - Call Chain = GUI__CompactPixelIndices
  [Called By]
  - >> _Convert8
  - >> _Convert16

  GUI__CompactPixelIndicesEx (Thumb, 12 bytes, Stack size 16 bytes, gui__compactpixelindices.o(i.GUI__CompactPixelIndicesEx))
  [Stack]

  - Max Depth = 40
  - Call Chain = GUI__CompactPixelIndicesEx ⇒ GUI__ConvertColor2Index
  [Calls]
  - >> GUI__ConvertColor2Index
  [Called By]
  - >> GUI_MEMDEV__WriteToActiveAlpha

  GUI__Config (Thumb, 42 bytes, Stack size 8 bytes, gui_core.o(i.GUI__Config))
  [Stack]

  - Max Depth = 232
  - Call Chain = GUI__Config ⇒ LCD_X_Config ⇒ GUI_DEVICE_CreateAndLink ⇒ GUI_DEVICE_Create ⇒ GUI_ALLOC_GetFixedBlock ⇒ _InitOnce ⇒ _EnlargeBlocks ⇒ _Alloc ⇒ _InitOnce (Cycle)
  [Calls]
  - >> GUI_X_Config
  - >> LCD_X_Config
  - >> GUI__RegisterExit
  [Called By]
  - >> GUI_Init

  GUI__ConvertColor2Index (Thumb, 360 bytes, Stack size 24 bytes, gui__compactpixelindices.o(i.GUI__ConvertColor2Index))
  [Stack]

  - Max Depth = 24
  - Call Chain = GUI__ConvertColor2Index
  [Called By]
  - >> GUI__CompactPixelIndicesEx

  GUI__DispLine (Thumb, 166 bytes, Stack size 24 bytes, gui_charline.o(i.GUI__DispLine))
  [Stack]

  - Max Depth = 160
  - Call Chain = GUI__DispLine ⇒ WM__InitIVRSearch ⇒ WM__GetNextIVR ⇒ WM__ActivateClipRect ⇒ _SetClipRectUserIntersect ⇒ LCD_SetClipRectEx ⇒ GUI__IntersectRects
  [Calls]
  - >> WM__InitIVRSearch
  - >> WM__GetNextIVR
  - >> _DispLine
  [Called By]
  - >> GUI__DispStringInRect

  GUI__DispStringInRect (Thumb, 320 bytes, Stack size 72 bytes, gui_dispstringinrect.o(i.GUI__DispStringInRect))
  [Stack]

  - Max Depth = 232
  - Call Chain = GUI__DispStringInRect ⇒ GUI__DispLine ⇒ WM__InitIVRSearch ⇒ WM__GetNextIVR ⇒ WM__ActivateClipRect ⇒ _SetClipRectUserIntersect ⇒ LCD_SetClipRectEx ⇒ GUI__IntersectRects
  [Calls]
  - >> GUI__HandleEOLine
  - >> GUI__GetLineNumChars
  - >> GUI__GetLineDistX
  - >> GUI__DispLine
  - >> GUI_UC__NumChars2NumBytes
  - >> GUI_GetFontDistY
  - >> GUI_GetClientRect
  [Called By]
  - >> GUI_DispStringInRectEx
  - >> GUI_DispStringInRectMax

  GUI__DoAlphaBlending (Thumb, 442 bytes, Stack size 104 bytes, gui__alpha.o(i.GUI__DoAlphaBlending))
  [Stack]

  - Max Depth = 304
  - Call Chain = GUI__DoAlphaBlending ⇒ GUI__GetAlphaBuffer ⇒ GUI_ALLOC_GetFixedBlock ⇒ _InitOnce ⇒ _EnlargeBlocks ⇒ _Alloc ⇒ _InitOnce (Cycle)
  [Calls]
  - >> GUI__ExpandPixelIndicesEx
  - >> GUI_ReadRectEx
  - >> GUI_GetpfIndex2ColorEx
  - >> GUI_GetBitsPerPixelEx
  - >> GUI__MixColors
  - >> GUI__GetAlphaBuffer
  [Called By]
  - >> GUI_MEMDEV__WriteToActiveAlpha

  GUI__ExpandPixelIndicesEx (Thumb, 322 bytes, Stack size 40 bytes, gui__expandpixelindices.o(i.GUI__ExpandPixelIndicesEx))
  [Stack]

  - Max Depth = 40
  - Call Chain = GUI__ExpandPixelIndicesEx
  [Called By]
  - >> GUI__DoAlphaBlending

  GUI__GetAlphaBuffer (Thumb, 144 bytes, Stack size 32 bytes, gui__alpha.o(i.GUI__GetAlphaBuffer))
  [Stack]

  - Max Depth = 200
  - Call Chain = GUI__GetAlphaBuffer ⇒ GUI_ALLOC_GetFixedBlock ⇒ _InitOnce ⇒ _EnlargeBlocks ⇒ _Alloc ⇒ _InitOnce (Cycle)
  [Calls]
  - >> LCD_GetVXSizeMax
  - >> GUI__RegisterExit
  - >> GUI_ALLOC_GetFixedBlock
  [Called By]
  - >> GUI__DoAlphaBlending
  - >> GUI__AllocAlphaBuffer

  GUI__GetLineDistX (Thumb, 74 bytes, Stack size 24 bytes, gui_charline.o(i.GUI__GetLineDistX))
  [Stack]

  - Max Depth = 48
  - Call Chain = GUI__GetLineDistX ⇒ GUI_UC__GetCharCodeInc
  [Calls]
  - >> GUI_UC__GetCharCodeInc
  - >> GUI__GetOverlap
  - >> GUI_GetCharDistX
  [Called By]
  - >> GUI__DispStringInRect

  GUI__GetLineNumChars (Thumb, 52 bytes, Stack size 24 bytes, gui_charline.o(i.GUI__GetLineNumChars))
  [Stack]

  - Max Depth = 48
  - Call Chain = GUI__GetLineNumChars ⇒ GUI_UC__GetCharCodeInc
  [Calls]
  - >> GUI_UC__GetCharCodeInc
  [Called By]
  - >> GUI__DispStringInRect

  GUI__GetOrg (Thumb, 18 bytes, Stack size 0 bytes, gui_getorg.o(i.GUI__GetOrg))
  [Called By]

  - >> GUI_GetOrg

  GUI__GetOverlap (Thumb, 24 bytes, Stack size 16 bytes, gui_charline.o(i.GUI__GetOverlap))
  [Stack]

  - Max Depth = 16
  - Call Chain = GUI__GetOverlap
  [Calls]
  - >> GUI_GetCharDistXEx
  [Called By]
  - >> GUI__GetLineDistX

  GUI__HandleEOLine (Thumb, 24 bytes, Stack size 0 bytes, gui__handleeoline.o(i.GUI__HandleEOLine))
  [Called By]

  - >> GUI__DispStringInRect

  GUI__IntersectRect (Thumb, 58 bytes, Stack size 0 bytes, gui__intersectrect.o(i.GUI__IntersectRect))
  [Called By]

  - >> WM__InitIVRSearch
  - >> WM__ClipAtParentBorders
  - >> WM_InvalidateRect
  - >> _SetClipRectUserIntersect
  - >> WM_ResizeWindow

  GUI__IntersectRects (Thumb, 82 bytes, Stack size 16 bytes, gui__intersectrects.o(i.GUI__IntersectRects))
  [Stack]

  - Max Depth = 16
  - Call Chain = GUI__IntersectRects
  [Called By]
  - >> GUI_DispStringInRectEx
  - >> GUI_DispStringInRectMax
  - >> WM_InvalidateWindowAndDescsEx
  - >> _Paint1Trans
  - >> _Invalidate1Abs
  - >> _Findy1
  - >> _Findx1
  - >> _Findx0
  - >> LCD_SetClipRectEx
  - >> WM__InvalidateRect

  GUI__ManageCache (Thumb, 12 bytes, Stack size 0 bytes, gui__managecache.o(i.GUI__ManageCache))
  [Stack]

  - Max Depth = 32
  - Call Chain = GUI__ManageCache ⇒ GUI__ManageCacheEx
  [Calls]
  - >> GUI__ManageCacheEx
  [Called By]
  - >> WM_Exec
  - >> _DispLine

  GUI__ManageCacheEx (Thumb, 196 bytes, Stack size 32 bytes, gui__managecache.o(i.GUI__ManageCacheEx))
  [Stack]

  - Max Depth = 32
  - Call Chain = GUI__ManageCacheEx
  [Calls]
  - >> GUI_DEVICE__GetpDriver
  [Called By]
  - >> GUI__ManageCache

  GUI__MixColors (Thumb, 102 bytes, Stack size 16 bytes, gui__alpha.o(i.GUI__MixColors))
  [Stack]

  - Max Depth = 16
  - Call Chain = GUI__MixColors
  [Called By]
  - >> GUI__MixColorsBulk
  - >> GUI__DoAlphaBlending
  - >> _DrawBitLine32BPP_DDB
  [Address Reference Count : 1]
  - gui__alpha.o(.data)

  GUI__MixColorsBulk (Thumb, 78 bytes, Stack size 36 bytes, gui__alpha.o(i.GUI__MixColorsBulk))
  [Stack]

  - Max Depth = 52
  - Call Chain = GUI__MixColorsBulk ⇒ GUI__MixColors
  [Calls]
  - >> GUI__MixColors
  [Address Reference Count : 1]
  - gui__alpha.o(.data)

  GUI__RegisterExit (Thumb, 10 bytes, Stack size 0 bytes, gui_core.o(i.GUI__RegisterExit))
  [Called By]

  - >> WM_Init
  - >> GUI__Config
  - >> _InitOnce
  - >> GUI__GetAlphaBuffer
  - >> LCD_InitColors

  GUI__memset (Thumb, 76 bytes, Stack size 8 bytes, gui__memset.o(i.GUI__memset))
  [Stack]

  - Max Depth = 8
  - Call Chain = GUI__memset
  [Called By]
  - >> _OnExit
  - >> _OnExit
  - >> _InitOnce
  - >> _CreateStaticDevice
  - >> GUI_ALLOC_AllocZero

  HAL_DMA2D_Init (Thumb, 90 bytes, Stack size 16 bytes, stm32f4xx_hal_dma2d.o(i.HAL_DMA2D_Init))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_DMA2D_Init ⇒ HAL_DMA2D_MspInit
  [Calls]
  - >> HAL_DMA2D_MspInit
  [Called By]
  - >> LCD_LL_Init

  HAL_DMA2D_MspInit (Thumb, 22 bytes, Stack size 8 bytes, lcdconf_stm32f429i_disco_mb1075_1.o(i.HAL_DMA2D_MspInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_DMA2D_MspInit
  [Called By]
  - >> HAL_DMA2D_Init

  HAL_DMA_DeInit (Thumb, 86 bytes, Stack size 16 bytes, stm32f4xx_hal_dma.o(i.HAL_DMA_DeInit))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_DMA_DeInit
  [Calls]
  - >> DMA_CalcBaseAndBitshift
  [Called By]
  - >> MspInit

  HAL_DMA_IRQHandler (Thumb, 412 bytes, Stack size 24 bytes, stm32f4xx_hal_dma.o(i.HAL_DMA_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_DMA_IRQHandler
  [Called By]
  - >> DMA2_Stream7_IRQHandler

  HAL_DMA_Init (Thumb, 116 bytes, Stack size 16 bytes, stm32f4xx_hal_dma.o(i.HAL_DMA_Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_DMA_Init
  [Calls]
  - >> DMA_CalcBaseAndBitshift
  [Called By]
  - >> HAL_UART_MspInit
  - >> MspInit

  HAL_DMA_Start_IT (Thumb, 78 bytes, Stack size 16 bytes, stm32f4xx_hal_dma.o(i.HAL_DMA_Start_IT))
  [Stack]

  - Max Depth = 28
  - Call Chain = HAL_DMA_Start_IT ⇒ DMA_SetConfig
  [Calls]
  - >> DMA_SetConfig
  [Called By]
  - >> HAL_UART_Transmit_DMA

  HAL_Delay (Thumb, 22 bytes, Stack size 16 bytes, stm32f4xx_hal.o(i.HAL_Delay))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_Delay
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> ConfigureSPIandGPIO
  - >> ErrorHandler
  - >> MainTask
  - >> BSP_SDRAM_Initialization_sequence
  - >> LCD_Delay
  - >> USB_SetCurrentMode
  - >> USB_DevDisconnect
  - >> USB_DevConnect

  HAL_FLASHEx_Erase (Thumb, 146 bytes, Stack size 32 bytes, stm32f4xx_hal_flash_ex.o(i.HAL_FLASHEx_Erase))
  [Stack]

  - Max Depth = 48
  - Call Chain = HAL_FLASHEx_Erase ⇒ FLASH_WaitForLastOperation
  [Calls]
  - >> FLASH_MassErase
  - >> FLASH_FlushCaches
  - >> FLASH_Erase_Sector
  - >> FLASH_WaitForLastOperation
  [Called By]
  - >> MainTask

  HAL_FLASH_Lock (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_hal_flash.o(i.HAL_FLASH_Lock))
  [Called By]

  - >> MainTask

  HAL_FLASH_Program (Thumb, 116 bytes, Stack size 32 bytes, stm32f4xx_hal_flash.o(i.HAL_FLASH_Program))
  [Stack]

  - Max Depth = 48
  - Call Chain = HAL_FLASH_Program ⇒ FLASH_WaitForLastOperation
  [Calls]
  - >> FLASH_WaitForLastOperation
  - >> FLASH_Program_Word
  - >> FLASH_Program_HalfWord
  - >> FLASH_Program_DoubleWord
  - >> FLASH_Program_Byte
  [Called By]
  - >> MainTask

  HAL_FLASH_Unlock (Thumb, 28 bytes, Stack size 0 bytes, stm32f4xx_hal_flash.o(i.HAL_FLASH_Unlock))
  [Called By]

  - >> MainTask

  HAL_GPIO_DeInit (Thumb, 320 bytes, Stack size 36 bytes, stm32f4xx_hal_gpio.o(i.HAL_GPIO_DeInit))
  [Stack]

  - Max Depth = 36
  - Call Chain = HAL_GPIO_DeInit
  [Called By]
  - >> HAL_UART_MspDeInit

  HAL_GPIO_Init (Thumb, 408 bytes, Stack size 40 bytes, stm32f4xx_hal_gpio.o(i.HAL_GPIO_Init))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_GPIO_Init
  [Called By]
  - >> HAL_UART_MspInit
  - >> HAL_PCD_MspInit
  - >> ConfigureSPIandGPIO
  - >> BSP_LED_Init
  - >> HAL_LTDC_MspInit
  - >> MspInit
  - >> SPIx_MspInit
  - >> LCD_IO_Init

  HAL_GPIO_ReadPin (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_hal_gpio.o(i.HAL_GPIO_ReadPin))
  [Called By]

  - >> Calibration
  - >> MainTask

  HAL_GPIO_TogglePin (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_hal_gpio.o(i.HAL_GPIO_TogglePin))
  [Called By]

  - >> BSP_LED_Toggle

  HAL_GPIO_WritePin (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_hal_gpio.o(i.HAL_GPIO_WritePin))
  [Called By]

  - >> ReadMAX11254Results
  - >> ConfigureSPIandGPIO
  - >> ConfigureMAX11254
  - >> Calibration
  - >> MainTask
  - >> BSP_LED_Init
  - >> LCD_IO_WriteReg
  - >> LCD_IO_WriteData
  - >> LCD_IO_Init

  HAL_GetTick (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_hal.o(i.HAL_GetTick))
  [Called By]

  - >> HAL_Delay
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_ClockConfig
  - >> HAL_RCCEx_PeriphCLKConfig
  - >> FLASH_WaitForLastOperation
  - >> SPI_WaitOnFlagUntilTimeout
  - >> FMC_SDRAM_SendCommand

  HAL_IncTick (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_hal.o(i.HAL_IncTick))
  [Called By]

  - >> SysTick_Handler

  HAL_Init (Thumb, 48 bytes, Stack size 8 bytes, stm32f4xx_hal.o(i.HAL_Init))
  [Stack]

  - Max Depth = 36
  - Call Chain = HAL_Init ⇒ HAL_InitTick ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_MspInit
  - >> HAL_InitTick
  - >> HAL_NVIC_SetPriorityGrouping
  [Called By]
  - >> main

  HAL_InitTick (Thumb, 34 bytes, Stack size 8 bytes, stm32f4xx_hal.o(i.HAL_InitTick))
  [Stack]

  - Max Depth = 28
  - Call Chain = HAL_InitTick ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_SYSTICK_Config
  - >> HAL_RCC_GetHCLKFreq
  [Called By]
  - >> HAL_RCC_ClockConfig
  - >> HAL_Init

  HAL_LTDC_ConfigCLUT (Thumb, 120 bytes, Stack size 20 bytes, stm32f4xx_hal_ltdc.o(i.HAL_LTDC_ConfigCLUT))
  [Stack]

  - Max Depth = 20
  - Call Chain = HAL_LTDC_ConfigCLUT
  [Called By]
  - >> LCD_LL_LayerInit
  - >> LCD_X_DisplayDriver

  HAL_LTDC_ConfigColorKeying (Thumb, 64 bytes, Stack size 12 bytes, stm32f4xx_hal_ltdc.o(i.HAL_LTDC_ConfigColorKeying))
  [Stack]

  - Max Depth = 12
  - Call Chain = HAL_LTDC_ConfigColorKeying
  [Called By]
  - >> LCD_X_DisplayDriver

  HAL_LTDC_ConfigLayer (Thumb, 82 bytes, Stack size 24 bytes, stm32f4xx_hal_ltdc.o(i.HAL_LTDC_ConfigLayer))
  [Stack]

  - Max Depth = 44
  - Call Chain = HAL_LTDC_ConfigLayer ⇒ LTDC_SetConfig
  [Calls]
  - >> LTDC_SetConfig
  - >> __aeabi_memcpy4
  [Called By]
  - >> LCD_LL_LayerInit

  HAL_LTDC_DeInit (Thumb, 24 bytes, Stack size 8 bytes, stm32f4xx_hal_ltdc.o(i.HAL_LTDC_DeInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_LTDC_DeInit
  [Calls]
  - >> HAL_LTDC_MspDeInit
  [Called By]
  - >> LCD_LL_Init

  HAL_LTDC_DisableColorKeying (Thumb, 58 bytes, Stack size 8 bytes, stm32f4xx_hal_ltdc.o(i.HAL_LTDC_DisableColorKeying))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_LTDC_DisableColorKeying
  [Called By]
  - >> LCD_X_DisplayDriver

  HAL_LTDC_EnableCLUT (Thumb, 58 bytes, Stack size 8 bytes, stm32f4xx_hal_ltdc.o(i.HAL_LTDC_EnableCLUT))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_LTDC_EnableCLUT
  [Called By]
  - >> LCD_LL_LayerInit

  HAL_LTDC_EnableColorKeying (Thumb, 58 bytes, Stack size 8 bytes, stm32f4xx_hal_ltdc.o(i.HAL_LTDC_EnableColorKeying))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_LTDC_EnableColorKeying
  [Called By]
  - >> LCD_X_DisplayDriver

  HAL_LTDC_ErrorCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_ltdc.o(i.HAL_LTDC_ErrorCallback))
  [Called By]

  - >> HAL_LTDC_IRQHandler

  HAL_LTDC_IRQHandler (Thumb, 162 bytes, Stack size 16 bytes, stm32f4xx_hal_ltdc.o(i.HAL_LTDC_IRQHandler))
  [Stack]

  - Max Depth = 68
  - Call Chain = HAL_LTDC_IRQHandler ⇒ HAL_LTDC_LineEventCallback ⇒ HAL_LTDC_SetAddress ⇒ LTDC_SetConfig
  [Calls]
  - >> HAL_LTDC_LineEventCallback
  - >> HAL_LTDC_ErrorCallback
  [Called By]
  - >> LTDC_IRQHandler

  HAL_LTDC_Init (Thumb, 248 bytes, Stack size 16 bytes, stm32f4xx_hal_ltdc.o(i.HAL_LTDC_Init))
  [Stack]

  - Max Depth = 96
  - Call Chain = HAL_LTDC_Init ⇒ HAL_LTDC_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_LTDC_MspInit
  [Called By]
  - >> LCD_LL_Init

  HAL_LTDC_LineEventCallback (Thumb, 74 bytes, Stack size 16 bytes, lcdconf_stm32f429i_disco_mb1075_1.o(i.HAL_LTDC_LineEventCallback))
  [Stack]

  - Max Depth = 52
  - Call Chain = HAL_LTDC_LineEventCallback ⇒ HAL_LTDC_SetAddress ⇒ LTDC_SetConfig
  [Calls]
  - >> HAL_LTDC_SetAddress
  - >> HAL_LTDC_ProgramLineEvent
  - >> GUI_MULTIBUF_ConfirmEx
  [Called By]
  - >> HAL_LTDC_IRQHandler

  HAL_LTDC_MspDeInit (Thumb, 20 bytes, Stack size 0 bytes, lcdconf_stm32f429i_disco_mb1075_1.o(i.HAL_LTDC_MspDeInit))
  [Called By]

  - >> HAL_LTDC_DeInit

  HAL_LTDC_MspInit (Thumb, 270 bytes, Stack size 40 bytes, lcdconf_stm32f429i_disco_mb1075_1.o(i.HAL_LTDC_MspInit))
  [Stack]

  - Max Depth = 80
  - Call Chain = HAL_LTDC_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  - >> HAL_GPIO_Init
  [Called By]
  - >> HAL_LTDC_Init

  HAL_LTDC_ProgramLineEvent (Thumb, 50 bytes, Stack size 8 bytes, stm32f4xx_hal_ltdc.o(i.HAL_LTDC_ProgramLineEvent))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_LTDC_ProgramLineEvent
  [Called By]
  - >> LCD_LL_Init
  - >> HAL_LTDC_LineEventCallback

  HAL_LTDC_SetAddress (Thumb, 68 bytes, Stack size 16 bytes, stm32f4xx_hal_ltdc.o(i.HAL_LTDC_SetAddress))
  [Stack]

  - Max Depth = 36
  - Call Chain = HAL_LTDC_SetAddress ⇒ LTDC_SetConfig
  [Calls]
  - >> LTDC_SetConfig
  [Called By]
  - >> LCD_X_DisplayDriver
  - >> HAL_LTDC_LineEventCallback

  HAL_LTDC_SetAlpha (Thumb, 68 bytes, Stack size 16 bytes, stm32f4xx_hal_ltdc.o(i.HAL_LTDC_SetAlpha))
  [Stack]

  - Max Depth = 36
  - Call Chain = HAL_LTDC_SetAlpha ⇒ LTDC_SetConfig
  [Calls]
  - >> LTDC_SetConfig
  [Called By]
  - >> LCD_X_DisplayDriver

  HAL_LTDC_SetWindowPosition (Thumb, 84 bytes, Stack size 16 bytes, stm32f4xx_hal_ltdc.o(i.HAL_LTDC_SetWindowPosition))
  [Stack]

  - Max Depth = 36
  - Call Chain = HAL_LTDC_SetWindowPosition ⇒ LTDC_SetConfig
  [Calls]
  - >> LTDC_SetConfig
  [Called By]
  - >> LCD_X_DisplayDriver

  HAL_MspInit (Thumb, 8 bytes, Stack size 8 bytes, stm32f4xx_hal.o(i.HAL_MspInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_MspInit
  [Called By]
  - >> HAL_Init

  HAL_NVIC_DisableIRQ (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_hal_cortex.o(i.HAL_NVIC_DisableIRQ))
  [Called By]

  - >> HAL_UART_MspDeInit

  HAL_NVIC_EnableIRQ (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_hal_cortex.o(i.HAL_NVIC_EnableIRQ))
  [Called By]

  - >> HAL_UART_MspInit
  - >> HAL_PCD_MspInit
  - >> HAL_LTDC_MspInit
  - >> MspInit

  HAL_NVIC_SetPriority (Thumb, 60 bytes, Stack size 16 bytes, stm32f4xx_hal_cortex.o(i.HAL_NVIC_SetPriority))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_NVIC_SetPriority
  [Calls]
  - >> NVIC_SetPriority
  [Called By]
  - >> HAL_UART_MspInit
  - >> HAL_PCD_MspInit
  - >> HAL_LTDC_MspInit
  - >> MspInit
  - >> HAL_InitTick

  HAL_NVIC_SetPriorityGrouping (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_hal_cortex.o(i.HAL_NVIC_SetPriorityGrouping))
  [Called By]

  - >> HAL_Init

  HAL_PCDEx_SetRxFiFo (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_hal_pcd_ex.o(i.HAL_PCDEx_SetRxFiFo))
  [Called By]

  - >> USBD_LL_Init

  HAL_PCDEx_SetTxFiFo (Thumb, 68 bytes, Stack size 20 bytes, stm32f4xx_hal_pcd_ex.o(i.HAL_PCDEx_SetTxFiFo))
  [Stack]

  - Max Depth = 20
  - Call Chain = HAL_PCDEx_SetTxFiFo
  [Called By]
  - >> USBD_LL_Init

  HAL_PCD_ConnectCallback (Thumb, 8 bytes, Stack size 0 bytes, usbd_conf.o(i.HAL_PCD_ConnectCallback))
  [Calls]

  - >> USBD_LL_DevConnected
  [Called By]
  - >> HAL_PCD_IRQHandler

  HAL_PCD_DataInStageCallback (Thumb, 18 bytes, Stack size 0 bytes, usbd_conf.o(i.HAL_PCD_DataInStageCallback))
  [Stack]

  - Max Depth = 88
  - Call Chain = HAL_PCD_DataInStageCallback ⇒ USBD_LL_DataInStage ⇒ USBD_CtlContinueSendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_DataInStage
  [Called By]
  - >> HAL_PCD_IRQHandler

  HAL_PCD_DataOutStageCallback (Thumb, 20 bytes, Stack size 0 bytes, usbd_conf.o(i.HAL_PCD_DataOutStageCallback))
  [Stack]

  - Max Depth = 80
  - Call Chain = HAL_PCD_DataOutStageCallback ⇒ USBD_LL_DataOutStage ⇒ USBD_CtlSendStatus ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_DataOutStage
  [Called By]
  - >> HAL_PCD_IRQHandler

  HAL_PCD_DisconnectCallback (Thumb, 8 bytes, Stack size 0 bytes, usbd_conf.o(i.HAL_PCD_DisconnectCallback))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_PCD_DisconnectCallback ⇒ USBD_LL_DevDisconnected
  [Calls]
  - >> USBD_LL_DevDisconnected
  [Called By]
  - >> HAL_PCD_IRQHandler

  HAL_PCD_EP_Close (Thumb, 68 bytes, Stack size 8 bytes, stm32f4xx_hal_pcd.o(i.HAL_PCD_EP_Close))
  [Stack]

  - Max Depth = 20
  - Call Chain = HAL_PCD_EP_Close ⇒ USB_DeactivateEndpoint
  [Calls]
  - >> USB_DeactivateEndpoint
  [Called By]
  - >> USBD_LL_CloseEP

  HAL_PCD_EP_ClrStall (Thumb, 80 bytes, Stack size 16 bytes, stm32f4xx_hal_pcd.o(i.HAL_PCD_EP_ClrStall))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_PCD_EP_ClrStall
  [Calls]
  - >> USB_EPClearStall
  [Called By]
  - >> USBD_LL_ClearStallEP

  HAL_PCD_EP_GetRxCount (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_hal_pcd.o(i.HAL_PCD_EP_GetRxCount))
  [Called By]

  - >> USBD_LL_GetRxDataSize

  HAL_PCD_EP_Open (Thumb, 84 bytes, Stack size 16 bytes, stm32f4xx_hal_pcd.o(i.HAL_PCD_EP_Open))
  [Stack]

  - Max Depth = 28
  - Call Chain = HAL_PCD_EP_Open ⇒ USB_ActivateEndpoint
  [Calls]
  - >> USB_ActivateEndpoint
  [Called By]
  - >> USBD_LL_OpenEP

  HAL_PCD_EP_Receive (Thumb, 94 bytes, Stack size 16 bytes, stm32f4xx_hal_pcd.o(i.HAL_PCD_EP_Receive))
  [Stack]

  - Max Depth = 48
  - Call Chain = HAL_PCD_EP_Receive ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USB_EPStartXfer
  - >> USB_EP0StartXfer
  [Called By]
  - >> USBD_LL_PrepareReceive

  HAL_PCD_EP_SetStall (Thumb, 96 bytes, Stack size 16 bytes, stm32f4xx_hal_pcd.o(i.HAL_PCD_EP_SetStall))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_PCD_EP_SetStall
  [Calls]
  - >> USB_EPSetStall
  - >> USB_EP0_OutStart
  [Called By]
  - >> USBD_LL_StallEP

  HAL_PCD_EP_Transmit (Thumb, 86 bytes, Stack size 16 bytes, stm32f4xx_hal_pcd.o(i.HAL_PCD_EP_Transmit))
  [Stack]

  - Max Depth = 48
  - Call Chain = HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USB_EPStartXfer
  - >> USB_EP0StartXfer
  [Called By]
  - >> USBD_LL_Transmit

  HAL_PCD_IRQHandler (Thumb, 1022 bytes, Stack size 40 bytes, stm32f4xx_hal_pcd.o(i.HAL_PCD_IRQHandler))
  [Stack]

  - Max Depth = 168
  - Call Chain = HAL_PCD_IRQHandler ⇒ HAL_PCD_SetupStageCallback ⇒ USBD_LL_SetupStage ⇒ USBD_StdDevReq ⇒ USBD_GetDescriptor ⇒ USBD_CtlSendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> HAL_PCD_SuspendCallback
  - >> HAL_PCD_SetupStageCallback
  - >> HAL_PCD_SOFCallback
  - >> HAL_PCD_ResumeCallback
  - >> HAL_PCD_ResetCallback
  - >> HAL_PCD_ISOOUTIncompleteCallback
  - >> HAL_PCD_ISOINIncompleteCallback
  - >> HAL_PCD_DisconnectCallback
  - >> HAL_PCD_DataOutStageCallback
  - >> HAL_PCD_DataInStageCallback
  - >> HAL_PCD_ConnectCallback
  - >> PCD_WriteEmptyTxFifo
  - >> USB_ReadPacket
  - >> USB_ReadInterrupts
  - >> USB_ReadDevOutEPInterrupt
  - >> USB_ReadDevInEPInterrupt
  - >> USB_ReadDevAllOutEpInterrupt
  - >> USB_ReadDevAllInEpInterrupt
  - >> USB_GetMode
  - >> USB_GetDevSpeed
  - >> USB_FlushTxFifo
  - >> USB_EP0_OutStart
  - >> USB_ActivateSetup
  [Called By]
  - >> OTG_HS_IRQHandler

  HAL_PCD_ISOINIncompleteCallback (Thumb, 8 bytes, Stack size 0 bytes, usbd_conf.o(i.HAL_PCD_ISOINIncompleteCallback))
  [Calls]

  - >> USBD_LL_IsoINIncomplete
  [Called By]
  - >> HAL_PCD_IRQHandler

  HAL_PCD_ISOOUTIncompleteCallback (Thumb, 8 bytes, Stack size 0 bytes, usbd_conf.o(i.HAL_PCD_ISOOUTIncompleteCallback))
  [Calls]

  - >> USBD_LL_IsoOUTIncomplete
  [Called By]
  - >> HAL_PCD_IRQHandler

  HAL_PCD_Init (Thumb, 190 bytes, Stack size 64 bytes, stm32f4xx_hal_pcd.o(i.HAL_PCD_Init))
  [Stack]

  - Max Depth = 144
  - Call Chain = HAL_PCD_Init ⇒ HAL_PCD_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_PCD_MspInit
  - >> USB_SetCurrentMode
  - >> USB_DisableGlobalInt
  - >> USB_DevInit
  - >> USB_DevDisconnect
  - >> USB_CoreInit
  - >> __aeabi_memcpy4
  [Called By]
  - >> USBD_LL_Init

  HAL_PCD_MspInit (Thumb, 250 bytes, Stack size 40 bytes, usbd_conf.o(i.HAL_PCD_MspInit))
  [Stack]

  - Max Depth = 80
  - Call Chain = HAL_PCD_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  - >> HAL_GPIO_Init
  [Called By]
  - >> HAL_PCD_Init

  HAL_PCD_ResetCallback (Thumb, 32 bytes, Stack size 8 bytes, usbd_conf.o(i.HAL_PCD_ResetCallback))
  [Stack]

  - Max Depth = 60
  - Call Chain = HAL_PCD_ResetCallback ⇒ USBD_LL_Reset ⇒ USBD_LL_OpenEP ⇒ HAL_PCD_EP_Open ⇒ USB_ActivateEndpoint
  [Calls]
  - >> USBD_LL_SetSpeed
  - >> USBD_LL_Reset
  [Called By]
  - >> HAL_PCD_IRQHandler

  HAL_PCD_ResumeCallback (Thumb, 8 bytes, Stack size 0 bytes, usbd_conf.o(i.HAL_PCD_ResumeCallback))
  [Calls]

  - >> USBD_LL_Resume
  [Called By]
  - >> HAL_PCD_IRQHandler

  HAL_PCD_SOFCallback (Thumb, 8 bytes, Stack size 0 bytes, usbd_conf.o(i.HAL_PCD_SOFCallback))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_PCD_SOFCallback ⇒ USBD_LL_SOF
  [Calls]
  - >> USBD_LL_SOF
  [Called By]
  - >> HAL_PCD_IRQHandler

  HAL_PCD_SetAddress (Thumb, 36 bytes, Stack size 8 bytes, stm32f4xx_hal_pcd.o(i.HAL_PCD_SetAddress))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_PCD_SetAddress
  [Calls]
  - >> USB_SetDevAddress
  [Called By]
  - >> USBD_LL_SetUSBAddress

  HAL_PCD_SetupStageCallback (Thumb, 14 bytes, Stack size 0 bytes, usbd_conf.o(i.HAL_PCD_SetupStageCallback))
  [Stack]

  - Max Depth = 128
  - Call Chain = HAL_PCD_SetupStageCallback ⇒ USBD_LL_SetupStage ⇒ USBD_StdDevReq ⇒ USBD_GetDescriptor ⇒ USBD_CtlSendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_SetupStage
  [Called By]
  - >> HAL_PCD_IRQHandler

  HAL_PCD_Start (Thumb, 42 bytes, Stack size 8 bytes, stm32f4xx_hal_pcd.o(i.HAL_PCD_Start))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_PCD_Start ⇒ USB_DevConnect ⇒ HAL_Delay
  [Calls]
  - >> USB_EnableGlobalInt
  - >> USB_DevConnect
  [Called By]
  - >> USBD_LL_Start

  HAL_PCD_SuspendCallback (Thumb, 8 bytes, Stack size 0 bytes, usbd_conf.o(i.HAL_PCD_SuspendCallback))
  [Calls]

  - >> USBD_LL_Suspend
  [Called By]
  - >> HAL_PCD_IRQHandler

  HAL_RCCEx_PeriphCLKConfig (Thumb, 644 bytes, Stack size 40 bytes, stm32f4xx_hal_rcc_ex.o(i.HAL_RCCEx_PeriphCLKConfig))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_RCCEx_PeriphCLKConfig
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> LCD_LL_Init

  HAL_RCC_ClockConfig (Thumb, 514 bytes, Stack size 40 bytes, stm32f4xx_hal_rcc.o(i.HAL_RCC_ClockConfig))
  [Stack]

  - Max Depth = 68
  - Call Chain = HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_GetTick
  - >> HAL_InitTick
  [Called By]
  - >> SystemClock_Config

  HAL_RCC_GetHCLKFreq (Thumb, 38 bytes, Stack size 8 bytes, stm32f4xx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq))
  [Stack]

  - Max Depth = 20
  - Call Chain = HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_RCC_GetSysClockFreq
  [Called By]
  - >> HAL_RCC_GetPCLK2Freq
  - >> HAL_InitTick
  - >> HAL_RCC_GetPCLK1Freq

  HAL_RCC_GetPCLK1Freq (Thumb, 36 bytes, Stack size 8 bytes, stm32f4xx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq))
  [Stack]

  - Max Depth = 28
  - Call Chain = HAL_RCC_GetPCLK1Freq ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_RCC_GetHCLKFreq
  [Called By]
  - >> UART_SetConfig

  HAL_RCC_GetPCLK2Freq (Thumb, 36 bytes, Stack size 8 bytes, stm32f4xx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq))
  [Stack]

  - Max Depth = 28
  - Call Chain = HAL_RCC_GetPCLK2Freq ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_RCC_GetHCLKFreq
  [Called By]
  - >> UART_SetConfig

  HAL_RCC_GetSysClockFreq (Thumb, 104 bytes, Stack size 12 bytes, stm32f4xx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq))
  [Stack]

  - Max Depth = 12
  - Call Chain = HAL_RCC_GetSysClockFreq
  [Called By]
  - >> HAL_RCC_GetHCLKFreq

  HAL_RCC_OscConfig (Thumb, 806 bytes, Stack size 40 bytes, stm32f4xx_hal_rcc.o(i.HAL_RCC_OscConfig))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_RCC_OscConfig
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_SDRAM_Init (Thumb, 66 bytes, Stack size 16 bytes, stm32f4xx_hal_sdram.o(i.HAL_SDRAM_Init))
  [Stack]

  - Max Depth = 36
  - Call Chain = HAL_SDRAM_Init ⇒ FMC_SDRAM_Timing_Init
  [Calls]
  - >> HAL_SDRAM_MspInit
  - >> FMC_SDRAM_Timing_Init
  - >> FMC_SDRAM_Init
  [Called By]
  - >> BSP_SDRAM_Init

  HAL_SDRAM_MspInit (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_sdram.o(i.HAL_SDRAM_MspInit))
  [Called By]

  - >> HAL_SDRAM_Init

  HAL_SDRAM_ProgramRefreshRate (Thumb, 34 bytes, Stack size 8 bytes, stm32f4xx_hal_sdram.o(i.HAL_SDRAM_ProgramRefreshRate))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_SDRAM_ProgramRefreshRate
  [Calls]
  - >> FMC_SDRAM_ProgramRefreshRate
  [Called By]
  - >> BSP_SDRAM_Initialization_sequence

  HAL_SDRAM_SendCommand (Thumb, 48 bytes, Stack size 16 bytes, stm32f4xx_hal_sdram.o(i.HAL_SDRAM_SendCommand))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_SDRAM_SendCommand ⇒ FMC_SDRAM_SendCommand
  [Calls]
  - >> FMC_SDRAM_SendCommand
  [Called By]
  - >> BSP_SDRAM_Initialization_sequence

  HAL_SPI_DeInit (Thumb, 40 bytes, Stack size 8 bytes, stm32f4xx_hal_spi.o(i.HAL_SPI_DeInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_SPI_DeInit
  [Calls]
  - >> HAL_SPI_MspDeInit
  [Called By]
  - >> SPIx_Error

  HAL_SPI_GetState (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_hal_spi.o(i.HAL_SPI_GetState))
  [Called By]

  - >> SPIx_Init

  HAL_SPI_Init (Thumb, 132 bytes, Stack size 16 bytes, stm32f4xx_hal_spi.o(i.HAL_SPI_Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_SPI_Init
  [Calls]
  - >> HAL_SPI_MspInit
  [Called By]
  - >> SPIx_Init

  HAL_SPI_MspDeInit (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_spi.o(i.HAL_SPI_MspDeInit))
  [Called By]

  - >> HAL_SPI_DeInit

  HAL_SPI_MspInit (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_spi.o(i.HAL_SPI_MspInit))
  [Called By]

  - >> HAL_SPI_Init

  HAL_SPI_Transmit (Thumb, 324 bytes, Stack size 32 bytes, stm32f4xx_hal_spi.o(i.HAL_SPI_Transmit))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_SPI_Transmit ⇒ SPI_WaitOnFlagUntilTimeout
  [Calls]
  - >> SPI_WaitOnFlagUntilTimeout
  [Called By]
  - >> SPIx_Write_2
  - >> SPIx_Write

  HAL_SPI_TransmitReceive (Thumb, 682 bytes, Stack size 32 bytes, stm32f4xx_hal_spi.o(i.HAL_SPI_TransmitReceive))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_SPI_TransmitReceive ⇒ SPI_WaitOnFlagUntilTimeout
  [Calls]
  - >> SPI_WaitOnFlagUntilTimeout
  [Called By]
  - >> SPIx_WriteRead_2

  HAL_SYSTICK_Config (Thumb, 40 bytes, Stack size 8 bytes, stm32f4xx_hal_cortex.o(i.HAL_SYSTICK_Config))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_SYSTICK_Config
  [Calls]
  - >> NVIC_SetPriority
  [Called By]
  - >> HAL_InitTick

  HAL_TIMEx_BreakCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_tim_ex.o(i.HAL_TIMEx_BreakCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIMEx_CommutationCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_tim_ex.o(i.HAL_TIMEx_CommutationCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIM_Base_Init (Thumb, 54 bytes, Stack size 8 bytes, stm32f4xx_hal_tim.o(i.HAL_TIM_Base_Init))
  [Stack]

  - Max Depth = 28
  - Call Chain = HAL_TIM_Base_Init ⇒ TIM_Base_SetConfig
  [Calls]
  - >> TIM_Base_SetConfig
  - >> HAL_TIM_Base_MspInit
  [Called By]
  - >> CDC_Itf_Init

  HAL_TIM_Base_MspInit (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_tim.o(i.HAL_TIM_Base_MspInit))
  [Called By]

  - >> HAL_TIM_Base_Init

  HAL_TIM_Base_Start_IT (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_hal_tim.o(i.HAL_TIM_Base_Start_IT))
  [Called By]

  - >> CDC_Itf_Init

  HAL_TIM_IC_CaptureCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_tim.o(i.HAL_TIM_IC_CaptureCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIM_IRQHandler (Thumb, 358 bytes, Stack size 16 bytes, stm32f4xx_hal_tim.o(i.HAL_TIM_IRQHandler))
  [Stack]

  - Max Depth = 96
  - Call Chain = HAL_TIM_IRQHandler ⇒ HAL_TIM_PeriodElapsedCallback ⇒ USBD_CDC_TransmitPacket ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> HAL_TIM_PeriodElapsedCallback
  - >> HAL_TIMEx_CommutationCallback
  - >> HAL_TIMEx_BreakCallback
  - >> HAL_TIM_TriggerCallback
  - >> HAL_TIM_PWM_PulseFinishedCallback
  - >> HAL_TIM_OC_DelayElapsedCallback
  - >> HAL_TIM_IC_CaptureCallback
  [Called By]
  - >> TIM3_IRQHandler

  HAL_TIM_OC_DelayElapsedCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_tim.o(i.HAL_TIM_OC_DelayElapsedCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIM_PWM_PulseFinishedCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_tim.o(i.HAL_TIM_PWM_PulseFinishedCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIM_PeriodElapsedCallback (Thumb, 62 bytes, Stack size 16 bytes, usbd_cdc_interface.o(i.HAL_TIM_PeriodElapsedCallback))
  [Stack]

  - Max Depth = 80
  - Call Chain = HAL_TIM_PeriodElapsedCallback ⇒ USBD_CDC_TransmitPacket ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_CDC_TransmitPacket
  - >> USBD_CDC_SetTxBuffer
  [Called By]
  - >> HAL_TIM_IRQHandler

  HAL_TIM_TriggerCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_tim.o(i.HAL_TIM_TriggerCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_UART_DeInit (Thumb, 36 bytes, Stack size 8 bytes, stm32f4xx_hal_uart.o(i.HAL_UART_DeInit))
  [Stack]

  - Max Depth = 52
  - Call Chain = HAL_UART_DeInit ⇒ HAL_UART_MspDeInit ⇒ HAL_GPIO_DeInit
  [Calls]
  - >> HAL_UART_MspDeInit
  [Called By]
  - >> ComPort_Config
  - >> CDC_Itf_DeInit

  HAL_UART_ErrorCallback (Thumb, 2 bytes, Stack size 0 bytes, usbd_cdc_interface.o(i.HAL_UART_ErrorCallback))
  [Called By]

  - >> HAL_UART_IRQHandler
  - >> UART_DMAError

  HAL_UART_IRQHandler (Thumb, 246 bytes, Stack size 16 bytes, stm32f4xx_hal_uart.o(i.HAL_UART_IRQHandler))
  [Stack]

  - Max Depth = 80
  - Call Chain = HAL_UART_IRQHandler ⇒ HAL_UART_TxCpltCallback ⇒ USBD_CDC_ReceivePacket ⇒ USBD_LL_PrepareReceive ⇒ HAL_PCD_EP_Receive ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> HAL_UART_TxCpltCallback
  - >> HAL_UART_ErrorCallback
  - >> UART_Transmit_IT
  - >> UART_Receive_IT
  [Called By]
  - >> USART1_IRQHandler

  HAL_UART_Init (Thumb, 94 bytes, Stack size 16 bytes, stm32f4xx_hal_uart.o(i.HAL_UART_Init))
  [Stack]

  - Max Depth = 104
  - Call Chain = HAL_UART_Init ⇒ HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_UART_MspInit
  - >> UART_SetConfig
  [Called By]
  - >> ComPort_Config
  - >> CDC_Itf_Init

  HAL_UART_MspDeInit (Thumb, 66 bytes, Stack size 8 bytes, stm32f4xx_hal_msp.o(i.HAL_UART_MspDeInit))
  [Stack]

  - Max Depth = 44
  - Call Chain = HAL_UART_MspDeInit ⇒ HAL_GPIO_DeInit
  [Calls]
  - >> HAL_NVIC_DisableIRQ
  - >> HAL_GPIO_DeInit
  [Called By]
  - >> HAL_UART_DeInit

  HAL_UART_MspInit (Thumb, 252 bytes, Stack size 48 bytes, stm32f4xx_hal_msp.o(i.HAL_UART_MspInit))
  [Stack]

  - Max Depth = 88
  - Call Chain = HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_DMA_Init
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  - >> HAL_GPIO_Init
  [Called By]
  - >> HAL_UART_Init

  HAL_UART_Receive_IT (Thumb, 106 bytes, Stack size 0 bytes, stm32f4xx_hal_uart.o(i.HAL_UART_Receive_IT))
  [Called By]

  - >> HAL_UART_RxCpltCallback
  - >> ComPort_Config
  - >> CDC_Itf_Init

  HAL_UART_RxCpltCallback (Thumb, 28 bytes, Stack size 0 bytes, usbd_cdc_interface.o(i.HAL_UART_RxCpltCallback))
  [Calls]

  - >> HAL_UART_Receive_IT
  [Called By]
  - >> UART_Receive_IT

  HAL_UART_Transmit_DMA (Thumb, 130 bytes, Stack size 16 bytes, stm32f4xx_hal_uart.o(i.HAL_UART_Transmit_DMA))
  [Stack]

  - Max Depth = 44
  - Call Chain = HAL_UART_Transmit_DMA ⇒ HAL_DMA_Start_IT ⇒ DMA_SetConfig
  [Calls]
  - >> HAL_DMA_Start_IT
  [Called By]
  - >> CDC_Itf_Receive

  HAL_UART_TxCpltCallback (Thumb, 18 bytes, Stack size 8 bytes, usbd_cdc_interface.o(i.HAL_UART_TxCpltCallback))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_UART_TxCpltCallback ⇒ USBD_CDC_ReceivePacket ⇒ USBD_LL_PrepareReceive ⇒ HAL_PCD_EP_Receive ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_CDC_ReceivePacket
  [Called By]
  - >> HAL_UART_IRQHandler
  - >> UART_DMATransmitCplt

  HAL_UART_TxHalfCpltCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_uart.o(i.HAL_UART_TxHalfCpltCallback))
  [Called By]

  - >> UART_DMATxHalfCplt

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.HardFault_Handler))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f429xx.o(RESET)

  LCD_AA_MixColors16 (Thumb, 50 bytes, Stack size 8 bytes, lcd_aa.o(i.LCD_AA_MixColors16))
  [Stack]

  - Max Depth = 8
  - Call Chain = LCD_AA_MixColors16
  [Called By]
  - >> LCD_SetPixelAA4_Trans
  - >> LCD_SetPixelAA4_NoTrans

  LCD_AA_MixColors256 (Thumb, 16 bytes, Stack size 8 bytes, lcd_aa.o(i.LCD_AA_MixColors256))
  [Stack]

  - Max Depth = 8
  - Call Chain = LCD_AA_MixColors256
  [Called By]
  - >> LCD_SetPixelAA8_Trans
  - >> LCD_SetPixelAA8_NoTrans

  LCD_AA_SetAndMask (Thumb, 10 bytes, Stack size 0 bytes, lcd_aa.o(i.LCD_AA_SetAndMask))
  [Called By]

  - >> GUI__AlphaSuppressMixing

  LCD_Color2Index (Thumb, 18 bytes, Stack size 0 bytes, lcd.o(i.LCD_Color2Index))
  [Called By]

  - >> LCD_SetPixelAA8_Trans
  - >> LCD_SetPixelAA8_NoTrans
  - >> LCD_SetPixelAA4_Trans
  - >> LCD_SetPixelAA4_NoTrans
  - >> LCD_UpdateColorIndices
  - >> LCD_GetpPalConvTableUncached
  - >> _SetColor
  - >> _SetBkColor

  LCD_Color2Index_8666 (Thumb, 86 bytes, Stack size 0 bytes, guicc_8666.o(i.LCD_Color2Index_8666))
  [Address Reference Count : 1]

  - guicc_8666.o(.constdata)

  LCD_Delay (Thumb, 4 bytes, Stack size 0 bytes, stm32f429i_discovery.o(i.LCD_Delay))
  [Stack]

  - Max Depth = 16
  - Call Chain = LCD_Delay ⇒ HAL_Delay
  [Calls]
  - >> HAL_Delay
  [Called By]
  - >> ili9341_Init

  LCD_DrawBitmap (Thumb, 504 bytes, Stack size 88 bytes, lcd.o(i.LCD_DrawBitmap))
  [Stack]

  - Max Depth = 104
  - Call Chain = LCD_DrawBitmap ⇒ LCD_FillRect
  [Calls]
  - >> LCD_FillRect
  [Called By]
  - >> GUI_MEMDEV__WriteToActiveAlpha
  - >> GUIMONO_DispChar
  - >> _WriteToActiveOpaque_HT
  - >> _WriteToActiveOpaque_8

  LCD_DrawHLine (Thumb, 78 bytes, Stack size 16 bytes, lcd.o(i.LCD_DrawHLine))
  [Stack]

  - Max Depth = 16
  - Call Chain = LCD_DrawHLine
  [Address Reference Count : 1]
  - gui_core.o(.constdata)

  LCD_DrawPixel (Thumb, 96 bytes, Stack size 8 bytes, lcd.o(i.LCD_DrawPixel))
  [Stack]

  - Max Depth = 8
  - Call Chain = LCD_DrawPixel
  [Address Reference Count : 1]
  - gui_core.o(.constdata)

  LCD_FillRect (Thumb, 80 bytes, Stack size 16 bytes, lcd.o(i.LCD_FillRect))
  [Stack]

  - Max Depth = 16
  - Call Chain = LCD_FillRect
  [Called By]
  - >> CUSTOM_FillRect
  - >> GUI_ClearRect
  - >> GUI_FillRect
  - >> emWin_LCD_Init
  - >> GUIMONO_DispChar
  - >> _DrawBitmapCW
  - >> LCD__DrawBitmap_1bpp
  - >> LCD_DrawBitmap

  LCD_GetBitsPerPixelEx (Thumb, 6 bytes, Stack size 0 bytes, lcd_getex.o(i.LCD_GetBitsPerPixelEx))
  [Stack]

  - Max Depth = 16
  - Call Chain = LCD_GetBitsPerPixelEx ⇒ _GetDevProp
  [Calls]
  - >> _GetDevProp
  [Called By]
  - >> LCD_LL_LayerInit
  - >> LCD_X_Config
  - >> LCD_InitLUT

  LCD_GetDevFunc (Thumb, 18 bytes, Stack size 0 bytes, lcd_getex.o(i.LCD_GetDevFunc))
  [Called By]

  - >> _LCD_GetpPalConvTable

  LCD_GetMirrorXEx (Thumb, 6 bytes, Stack size 0 bytes, lcd_getex.o(i.LCD_GetMirrorXEx))
  [Stack]

  - Max Depth = 16
  - Call Chain = LCD_GetMirrorXEx ⇒ _GetDevProp
  [Calls]
  - >> _GetDevProp
  [Called By]
  - >> _SetOrg

  LCD_GetMirrorYEx (Thumb, 6 bytes, Stack size 0 bytes, lcd_getex.o(i.LCD_GetMirrorYEx))
  [Stack]

  - Max Depth = 16
  - Call Chain = LCD_GetMirrorYEx ⇒ _GetDevProp
  [Calls]
  - >> _GetDevProp
  [Called By]
  - >> _SetOrg

  LCD_GetNumColors (Thumb, 12 bytes, Stack size 0 bytes, lcd_getex.o(i.LCD_GetNumColors))
  [Stack]

  - Max Depth = 16
  - Call Chain = LCD_GetNumColors ⇒ _GetDevProp
  [Calls]
  - >> _GetDevProp
  [Called By]
  - >> _Index2Color_0
  - >> _GetIndexMask_0
  - >> _Color2Index_0

  LCD_GetNumColorsEx (Thumb, 6 bytes, Stack size 0 bytes, lcd_getex.o(i.LCD_GetNumColorsEx))
  [Stack]

  - Max Depth = 16
  - Call Chain = LCD_GetNumColorsEx ⇒ _GetDevProp
  [Calls]
  - >> _GetDevProp
  [Called By]
  - >> LCD_InitLUT

  LCD_GetNumLayers (Thumb, 26 bytes, Stack size 16 bytes, lcd_getnumdisplays.o(i.LCD_GetNumLayers))
  [Stack]

  - Max Depth = 16
  - Call Chain = LCD_GetNumLayers
  [Calls]
  - >> GUI_DEVICE__GetpDriver
  [Called By]
  - >> LCD_InitLUT

  LCD_GetPalette (Thumb, 10 bytes, Stack size 0 bytes, lcd_getex.o(i.LCD_GetPalette))
  [Stack]

  - Max Depth = 8
  - Call Chain = LCD_GetPalette ⇒ LCD_GetPaletteEx
  [Calls]
  - >> LCD_GetPaletteEx
  [Called By]
  - >> _Index2Color_0
  - >> _Color2Index_0

  LCD_GetPaletteEx (Thumb, 24 bytes, Stack size 8 bytes, lcd_getex.o(i.LCD_GetPaletteEx))
  [Stack]

  - Max Depth = 8
  - Call Chain = LCD_GetPaletteEx
  [Calls]
  - >> GUI_DEVICE__GetpDriver
  [Called By]
  - >> LCD_GetPalette

  LCD_GetPixelColor (Thumb, 14 bytes, Stack size 8 bytes, lcd_getpixelcolor.o(i.LCD_GetPixelColor))
  [Stack]

  - Max Depth = 40
  - Call Chain = LCD_GetPixelColor ⇒ LCD_GetPixelIndex
  [Calls]
  - >> LCD_Index2Color
  - >> LCD_GetPixelIndex
  [Called By]
  - >> LCD_SetPixelAA8_Trans
  - >> LCD_SetPixelAA4_Trans

  LCD_GetPixelIndex (Thumb, 86 bytes, Stack size 32 bytes, lcd_getp.o(i.LCD_GetPixelIndex))
  [Stack]

  - Max Depth = 32
  - Call Chain = LCD_GetPixelIndex
  [Called By]
  - >> LCD_GetPixelColor

  LCD_GetPosEx (Thumb, 44 bytes, Stack size 24 bytes, lcd_set.o(i.LCD_GetPosEx))
  [Stack]

  - Max Depth = 24
  - Call Chain = LCD_GetPosEx
  [Calls]
  - >> GUI_DEVICE__GetpDriver
  [Called By]
  - >> GUI_GetLayerPosEx

  LCD_GetSwapXYEx (Thumb, 6 bytes, Stack size 0 bytes, lcd_getex.o(i.LCD_GetSwapXYEx))
  [Stack]

  - Max Depth = 16
  - Call Chain = LCD_GetSwapXYEx ⇒ _GetDevProp
  [Calls]
  - >> _GetDevProp
  [Called By]
  - >> LCD_X_Config
  - >> _SetVSize
  - >> _SetSize
  - >> _SetOrg

  LCD_GetVXSizeEx (Thumb, 6 bytes, Stack size 0 bytes, lcd_getex.o(i.LCD_GetVXSizeEx))
  [Stack]

  - Max Depth = 16
  - Call Chain = LCD_GetVXSizeEx ⇒ _GetDevProp
  [Calls]
  - >> _GetDevProp
  [Called By]
  - >> GUI_MEMDEV_Draw

  LCD_GetVXSizeMax (Thumb, 6 bytes, Stack size 0 bytes, lcd_getex.o(i.LCD_GetVXSizeMax))
  [Stack]

  - Max Depth = 32
  - Call Chain = LCD_GetVXSizeMax ⇒ _GetMaxValue ⇒ _GetDevProp
  [Calls]
  - >> _GetMaxValue
  [Called By]
  - >> GUI__GetAlphaBuffer

  LCD_GetVYSizeEx (Thumb, 6 bytes, Stack size 0 bytes, lcd_getex.o(i.LCD_GetVYSizeEx))
  [Stack]

  - Max Depth = 16
  - Call Chain = LCD_GetVYSizeEx ⇒ _GetDevProp
  [Calls]
  - >> _GetDevProp
  [Called By]
  - >> GUI_MEMDEV_Draw

  LCD_GetXSize (Thumb, 12 bytes, Stack size 0 bytes, lcd_getex.o(i.LCD_GetXSize))
  [Stack]

  - Max Depth = 16
  - Call Chain = LCD_GetXSize ⇒ _GetDevProp
  [Calls]
  - >> _GetDevProp
  [Called By]
  - >> _TransformPoint
  - >> _CreateStaticDevice

  LCD_GetXSizeEx (Thumb, 6 bytes, Stack size 0 bytes, lcd_getex.o(i.LCD_GetXSizeEx))
  [Stack]

  - Max Depth = 16
  - Call Chain = LCD_GetXSizeEx ⇒ _GetDevProp
  [Calls]
  - >> _GetDevProp
  [Called By]
  - >> GUI_MEMDEV_Draw

  LCD_GetYSize (Thumb, 12 bytes, Stack size 0 bytes, lcd_getex.o(i.LCD_GetYSize))
  [Stack]

  - Max Depth = 16
  - Call Chain = LCD_GetYSize ⇒ _GetDevProp
  [Calls]
  - >> _GetDevProp
  [Called By]
  - >> _TransformPoint
  - >> _CreateStaticDevice

  LCD_GetYSizeEx (Thumb, 6 bytes, Stack size 0 bytes, lcd_getex.o(i.LCD_GetYSizeEx))
  [Stack]

  - Max Depth = 16
  - Call Chain = LCD_GetYSizeEx ⇒ _GetDevProp
  [Calls]
  - >> _GetDevProp
  [Called By]
  - >> GUI_MEMDEV_Draw

  LCD_GetpPalConvTable (Thumb, 4 bytes, Stack size 0 bytes, lcd_color.o(i.LCD_GetpPalConvTable))
  [Stack]

  - Max Depth = 24
  - Call Chain = LCD_GetpPalConvTable ⇒ LCD_GetpPalConvTableUncached
  [Calls]
  - >> LCD_GetpPalConvTableUncached
  [Called By]
  - >> _LCD_GetpPalConvTable

  LCD_GetpPalConvTableBM (Thumb, 4 bytes, Stack size 0 bytes, lcd_color.o(i.LCD_GetpPalConvTableBM))
  [Stack]

  - Max Depth = 24
  - Call Chain = LCD_GetpPalConvTableBM ⇒ LCD_GetpPalConvTableUncached
  [Calls]
  - >> LCD_GetpPalConvTableUncached
  [Address Reference Count : 1]
  - gui_core.o(.data)

  LCD_GetpPalConvTableUncached (Thumb, 68 bytes, Stack size 24 bytes, lcd_color.o(i.LCD_GetpPalConvTableUncached))
  [Stack]

  - Max Depth = 24
  - Call Chain = LCD_GetpPalConvTableUncached
  [Calls]
  - >> LCD_Color2Index
  [Called By]
  - >> LCD_GetpPalConvTable
  - >> LCD_GetpPalConvTableBM

  LCD_IO_Init (Thumb, 150 bytes, Stack size 48 bytes, stm32f429i_discovery.o(i.LCD_IO_Init))
  [Stack]

  - Max Depth = 136
  - Call Chain = LCD_IO_Init ⇒ SPIx_Init ⇒ SPIx_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  - >> SPIx_Init
  - >> HAL_GPIO_WritePin
  [Called By]
  - >> ili9341_Init

  LCD_IO_WriteData (Thumb, 46 bytes, Stack size 16 bytes, stm32f429i_discovery.o(i.LCD_IO_WriteData))
  [Stack]

  - Max Depth = 120
  - Call Chain = LCD_IO_WriteData ⇒ SPIx_Write ⇒ SPIx_Error ⇒ SPIx_Init ⇒ SPIx_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> SPIx_Write
  [Called By]
  - >> ili9341_Init

  LCD_IO_WriteReg (Thumb, 48 bytes, Stack size 16 bytes, stm32f429i_discovery.o(i.LCD_IO_WriteReg))
  [Stack]

  - Max Depth = 120
  - Call Chain = LCD_IO_WriteReg ⇒ SPIx_Write ⇒ SPIx_Error ⇒ SPIx_Init ⇒ SPIx_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> SPIx_Write
  [Called By]
  - >> ili9341_Init

  LCD_Index2Color (Thumb, 18 bytes, Stack size 0 bytes, lcd.o(i.LCD_Index2Color))
  [Called By]

  - >> LCD_GetPixelColor
  - >> LCD_SetPixelAA8_Trans
  - >> LCD_SetPixelAA8_NoTrans
  - >> LCD_SetPixelAA4_Trans
  - >> LCD_SetPixelAA4_NoTrans
  - >> LCD_InitLUT

  LCD_Index2Color_8666 (Thumb, 100 bytes, Stack size 8 bytes, guicc_8666.o(i.LCD_Index2Color_8666))
  [Stack]

  - Max Depth = 8
  - Call Chain = LCD_Index2Color_8666
  [Address Reference Count : 1]
  - guicc_8666.o(.constdata)

  LCD_Index2Color_888 (Thumb, 2 bytes, Stack size 0 bytes, guicc_888_index2color.o(i.LCD_Index2Color_888))
  [Address Reference Count : 1]

  - gui__alpha.o(i.GUI__DoAlphaBlending)

  LCD_Index2Color_8888 (Thumb, 2 bytes, Stack size 0 bytes, guicc_8888_index2color.o(i.LCD_Index2Color_8888))
  [Address Reference Count : 3]

  - gui__alpha.o(i.GUI__DoAlphaBlending)
  - guidev_writetoactivealpha.o(i.GUI_MEMDEV__WriteToActiveAlpha)
  - guicc_8888.o(.constdata)

  LCD_Index2Color_M565 (Thumb, 34 bytes, Stack size 8 bytes, guicc_m565.o(i.LCD_Index2Color_M565))
  [Stack]

  - Max Depth = 8
  - Call Chain = LCD_Index2Color_M565
  [Address Reference Count : 1]
  - guicc_m565.o(.constdata)

  LCD_Index2Color_M888 (Thumb, 20 bytes, Stack size 0 bytes, guicc_m888_index2color.o(i.LCD_Index2Color_M888))
  [Address Reference Count : 1]

  - guicc_m888.o(.constdata)

  LCD_InitColors (Thumb, 42 bytes, Stack size 8 bytes, lcd_color.o(i.LCD_InitColors))
  [Stack]

  - Max Depth = 176
  - Call Chain = LCD_InitColors ⇒ GUI_ALLOC_GetFixedBlock ⇒ _InitOnce ⇒ _EnlargeBlocks ⇒ _Alloc ⇒ _InitOnce (Cycle)
  [Calls]
  - >> GUI__RegisterExit
  - >> GUI_ALLOC_GetFixedBlock
  [Called By]
  - >> emWin_LCD_Init

  LCD_InitLUT (Thumb, 112 bytes, Stack size 32 bytes, lcd_color.o(i.LCD_InitLUT))
  [Stack]

  - Max Depth = 56
  - Call Chain = LCD_InitLUT ⇒ LCD_SetLUTEntryEx
  [Calls]
  - >> LCD_GetBitsPerPixelEx
  - >> GUI_DEVICE__GetpDriver
  - >> LCD_SetLUTEntryEx
  - >> LCD_GetNumLayers
  - >> LCD_GetNumColorsEx
  - >> LCD_Index2Color
  [Called By]
  - >> emWin_LCD_Init

  LCD_SelectLCD (Thumb, 54 bytes, Stack size 8 bytes, lcd_selectlcd.o(i.LCD_SelectLCD))
  [Stack]

  - Max Depth = 8
  - Call Chain = LCD_SelectLCD
  [Calls]
  - >> GUI_DEVICE_Unlink
  - >> LCD_SetClipRectMax
  [Called By]
  - >> GUI_SelectLCD

  LCD_SetBkColor (Thumb, 8 bytes, Stack size 0 bytes, lcd.o(i.LCD_SetBkColor))
  [Called By]

  - >> _InitContext
  - >> GUI_SetBkColor

  LCD_SetBkColorIndex (Thumb, 20 bytes, Stack size 0 bytes, lcd.o(i.LCD_SetBkColorIndex))
  [Called By]

  - >> LCD_UpdateColorIndices
  - >> _SetBkColor

  LCD_SetClipRectEx (Thumb, 38 bytes, Stack size 24 bytes, lcd_setcliprectex.o(i.LCD_SetClipRectEx))
  [Stack]

  - Max Depth = 40
  - Call Chain = LCD_SetClipRectEx ⇒ GUI__IntersectRects
  [Calls]
  - >> GUI__IntersectRects
  [Called By]
  - >> _SetClipRectUserIntersect

  LCD_SetClipRectMax (Thumb, 20 bytes, Stack size 0 bytes, lcd.o(i.LCD_SetClipRectMax))
  [Called By]

  - >> emWin_LCD_Init
  - >> WM_SelectWindow
  - >> WM_Deactivate
  - >> LCD_SelectLCD
  - >> GUI_MEMDEV_SetOrg
  - >> GUI_MEMDEV_Select

  LCD_SetColor (Thumb, 8 bytes, Stack size 0 bytes, lcd.o(i.LCD_SetColor))
  [Called By]

  - >> GUI_SetColor
  - >> _InitContext

  LCD_SetColorIndex (Thumb, 20 bytes, Stack size 0 bytes, lcd.o(i.LCD_SetColorIndex))
  [Called By]

  - >> LCD_UpdateColorIndices
  - >> _SetColor

  LCD_SetDevFunc (Thumb, 44 bytes, Stack size 24 bytes, lcd_set.o(i.LCD_SetDevFunc))
  [Stack]

  - Max Depth = 24
  - Call Chain = LCD_SetDevFunc
  [Calls]
  - >> GUI_DEVICE__GetpDriver
  [Called By]
  - >> CUSTOM_FillRect
  - >> LCD_X_Config

  LCD_SetDrawMode (Thumb, 8 bytes, Stack size 0 bytes, lcd.o(i.LCD_SetDrawMode))
  [Called By]

  - >> GUI_ClearRect
  - >> emWin_LCD_Init
  - >> GUIMONO_DispChar
  - >> GUI_SetDrawMode

  LCD_SetLUTEntryEx (Thumb, 44 bytes, Stack size 24 bytes, lcd_set.o(i.LCD_SetLUTEntryEx))
  [Stack]

  - Max Depth = 24
  - Call Chain = LCD_SetLUTEntryEx
  [Calls]
  - >> GUI_DEVICE__GetpDriver
  [Called By]
  - >> LCD_InitLUT

  LCD_SetPixelAA4_NoTrans (Thumb, 134 bytes, Stack size 32 bytes, lcd_aa.o(i.LCD_SetPixelAA4_NoTrans))
  [Stack]

  - Max Depth = 40
  - Call Chain = LCD_SetPixelAA4_NoTrans ⇒ LCD_AA_MixColors16
  [Calls]
  - >> LCD_AA_MixColors16
  - >> LCD_Index2Color
  - >> LCD_Color2Index
  [Address Reference Count : 1]
  - lcd_aa.o(i.LCD__GetPfSetPixel)

  LCD_SetPixelAA4_Trans (Thumb, 126 bytes, Stack size 32 bytes, lcd_aa.o(i.LCD_SetPixelAA4_Trans))
  [Stack]

  - Max Depth = 72
  - Call Chain = LCD_SetPixelAA4_Trans ⇒ LCD_GetPixelColor ⇒ LCD_GetPixelIndex
  [Calls]
  - >> LCD_GetPixelColor
  - >> LCD_AA_MixColors16
  - >> LCD_Index2Color
  - >> LCD_Color2Index
  [Address Reference Count : 1]
  - lcd_aa.o(i.LCD__GetPfSetPixel)

  LCD_SetPixelAA8_NoTrans (Thumb, 134 bytes, Stack size 32 bytes, lcd_aa.o(i.LCD_SetPixelAA8_NoTrans))
  [Stack]

  - Max Depth = 40
  - Call Chain = LCD_SetPixelAA8_NoTrans ⇒ LCD_AA_MixColors256
  [Calls]
  - >> LCD_AA_MixColors256
  - >> LCD_Index2Color
  - >> LCD_Color2Index
  [Address Reference Count : 1]
  - lcd_aa.o(i.LCD__GetPfSetPixel)

  LCD_SetPixelAA8_Trans (Thumb, 126 bytes, Stack size 32 bytes, lcd_aa.o(i.LCD_SetPixelAA8_Trans))
  [Stack]

  - Max Depth = 72
  - Call Chain = LCD_SetPixelAA8_Trans ⇒ LCD_GetPixelColor ⇒ LCD_GetPixelIndex
  [Calls]
  - >> LCD_GetPixelColor
  - >> LCD_AA_MixColors256
  - >> LCD_Index2Color
  - >> LCD_Color2Index
  [Address Reference Count : 1]
  - lcd_aa.o(i.LCD__GetPfSetPixel)

  LCD_SetSizeEx (Thumb, 44 bytes, Stack size 24 bytes, lcd_set.o(i.LCD_SetSizeEx))
  [Stack]

  - Max Depth = 24
  - Call Chain = LCD_SetSizeEx
  [Calls]
  - >> GUI_DEVICE__GetpDriver
  [Called By]
  - >> LCD_X_Config

  LCD_SetVRAMAddrEx (Thumb, 40 bytes, Stack size 16 bytes, lcd_set.o(i.LCD_SetVRAMAddrEx))
  [Stack]

  - Max Depth = 16
  - Call Chain = LCD_SetVRAMAddrEx
  [Calls]
  - >> GUI_DEVICE__GetpDriver
  [Called By]
  - >> LCD_X_Config

  LCD_SetVSizeEx (Thumb, 44 bytes, Stack size 24 bytes, lcd_set.o(i.LCD_SetVSizeEx))
  [Stack]

  - Max Depth = 24
  - Call Chain = LCD_SetVSizeEx
  [Calls]
  - >> GUI_DEVICE__GetpDriver
  [Called By]
  - >> LCD_X_Config

  LCD_UpdateColorIndices (Thumb, 32 bytes, Stack size 8 bytes, lcd_updatecolorindices.o(i.LCD_UpdateColorIndices))
  [Stack]

  - Max Depth = 8
  - Call Chain = LCD_UpdateColorIndices
  [Calls]
  - >> LCD_SetColorIndex
  - >> LCD_SetBkColorIndex
  - >> LCD_Color2Index
  [Called By]
  - >> GUI_SelectLCD
  - >> GUI_MEMDEV_Select

  LCD_X_Config (Thumb, 240 bytes, Stack size 16 bytes, lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config))
  [Stack]

  - Max Depth = 224
  - Call Chain = LCD_X_Config ⇒ GUI_DEVICE_CreateAndLink ⇒ GUI_DEVICE_Create ⇒ GUI_ALLOC_GetFixedBlock ⇒ _InitOnce ⇒ _EnlargeBlocks ⇒ _Alloc ⇒ _InitOnce (Cycle)
  [Calls]
  - >> LCD_LL_Init
  - >> LCD_LL_GetPixelformat
  - >> LCD_SetVSizeEx
  - >> LCD_SetVRAMAddrEx
  - >> LCD_SetSizeEx
  - >> LCD_SetDevFunc
  - >> LCD_GetSwapXYEx
  - >> LCD_GetBitsPerPixelEx
  - >> GUI_SetFuncMixColorsBulk
  - >> GUI_SetFuncMixColors
  - >> GUI_SetFuncGetpPalConvTable
  - >> GUI_SetFuncAlphaBlending
  - >> GUI_DEVICE_CreateAndLink
  - >> GUICC_M888_SetCustColorConv
  - >> GUICC_M8888I_SetCustColorConv
  - >> GUICC_M565_SetCustColorConv
  - >> GUICC_M4444I_SetCustColorConv
  - >> GUICC_M1555I_SetCustColorConv
  [Called By]
  - >> GUI__Config

  LCD_X_DisplayDriver (Thumb, 294 bytes, Stack size 32 bytes, lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_DisplayDriver))
  [Stack]

  - Max Depth = 156
  - Call Chain = LCD_X_DisplayDriver ⇒ LCD_LL_LayerInit ⇒ HAL_LTDC_ConfigLayer ⇒ LTDC_SetConfig
  [Calls]
  - >> LCD_LL_LayerInit
  - >> HAL_LTDC_SetWindowPosition
  - >> HAL_LTDC_SetAlpha
  - >> HAL_LTDC_SetAddress
  - >> HAL_LTDC_EnableColorKeying
  - >> HAL_LTDC_DisableColorKeying
  - >> HAL_LTDC_ConfigColorKeying
  - >> HAL_LTDC_ConfigCLUT
  - >> GUI_GetLayerPosEx
  [Called By]
  - >> _ShowBuffer
  - >> _SetVis
  - >> _SetVRAMAddr
  - >> _SetSize
  - >> _SetPos
  - >> _SetOrg
  - >> _SetChromaMode
  - >> _SetChroma
  - >> _SetAlphaMode
  - >> _SetAlpha
  - >> _On
  - >> _Off
  - >> _Init

  LCD__DrawBitmap_1bpp (Thumb, 424 bytes, Stack size 104 bytes, lcd.o(i.LCD__DrawBitmap_1bpp))
  [Stack]

  - Max Depth = 120
  - Call Chain = LCD__DrawBitmap_1bpp ⇒ LCD_FillRect
  [Calls]
  - >> LCD_FillRect
  [Called By]
  - >> _WriteToActiveOpaque_8

  LCD__GetBPP (Thumb, 92 bytes, Stack size 0 bytes, lcd_getex.o(i.LCD__GetBPP))
  [Called By]

  - >> LCD__GetBPPDevice

  LCD__GetBPPDevice (Thumb, 50 bytes, Stack size 4 bytes, lcd_getex.o(i.LCD__GetBPPDevice))
  [Stack]

  - Max Depth = 4
  - Call Chain = LCD__GetBPPDevice
  [Calls]
  - >> LCD__GetBPP
  [Called By]
  - >> GUI_MEMDEV__CreateFixed
  - >> GUI_MEMDEV_GetBitsPerPixel

  LCD__GetPfSetPixel (Thumb, 48 bytes, Stack size 0 bytes, lcd_aa.o(i.LCD__GetPfSetPixel))
  [Called By]

  - >> _DrawBitmap

  LTDC_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.LTDC_IRQHandler))
  [Stack]

  - Max Depth = 68
  - Call Chain = LTDC_IRQHandler ⇒ HAL_LTDC_IRQHandler ⇒ HAL_LTDC_LineEventCallback ⇒ HAL_LTDC_SetAddress ⇒ LTDC_SetConfig
  [Calls]
  - >> HAL_LTDC_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f429xx.o(RESET)

  MainTask (Thumb, 2984 bytes, Stack size 432 bytes, maintask.o(i.MainTask))
  [Stack]

  - Max Depth = 2824
  - Call Chain = MainTask ⇒ Calibration ⇒ GUI_Delay ⇒ GUI_Exec ⇒ GUI_Exec1 ⇒ WM_Exec ⇒ _DrawNext ⇒ WM__Paint ⇒ GUI_MEMDEV_Draw ⇒ GUI_MEMDEV_CopyToLCD ⇒ GUI_MEMDEV_CopyToLCDAt ⇒ GUI_MEMDEV__WriteToActiveOpaque ⇒ _WriteToActiveOpaque_8 ⇒ LCD__DrawBitmap_1bpp ⇒ LCD_FillRect
  [Calls]
  - >> USBD_CDC_TransmitPacket
  - >> USBD_CDC_SetTxBuffer
  - >> HAL_Delay
  - >> __aeabi_ui2d
  - >> __aeabi_i2d
  - >> __aeabi_dsub
  - >> __aeabi_drsub
  - >> __aeabi_dmul
  - >> __aeabi_ddiv
  - >> __aeabi_dadd
  - >> __aeabi_d2iz
  - >> __aeabi_cdrcmple
  - >> __aeabi_cdcmple
  - >> SPIx_Write_2
  - >> HAL_GPIO_WritePin
  - >> HAL_GPIO_ReadPin
  - >> HAL_FLASH_Unlock
  - >> HAL_FLASH_Program
  - >> HAL_FLASH_Lock
  - >> HAL_FLASHEx_Erase
  - >> GUI_SetTextMode
  - >> GUI_SetFont
  - >> GUI_FillRectEx
  - >> GUI_FillCircle
  - >> GUI_DispStringInRectEx
  - >> GUI_ClearRect
  - >> GUI_Clear
  - >> BSP_LED_Toggle
  - >> ReadMAX11254Results
  - >> ConfigureSPIandGPIO
  - >> ConfigureMAX11254
  - >> Calibration
  - >> ErrorHandler
  - >> __2sprintf
  - >> strlen
  - >> __aeabi_memcpy4
  [Called By]
  - >> main

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.MemManage_Handler))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f429xx.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.NMI_Handler))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  OTG_HS_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.OTG_HS_IRQHandler))
  [Stack]

  - Max Depth = 168
  - Call Chain = OTG_HS_IRQHandler ⇒ HAL_PCD_IRQHandler ⇒ HAL_PCD_SetupStageCallback ⇒ USBD_LL_SetupStage ⇒ USBD_StdDevReq ⇒ USBD_GetDescriptor ⇒ USBD_CtlSendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> HAL_PCD_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f429xx.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.PendSV_Handler))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  ReadMAX11254Results (Thumb, 264 bytes, Stack size 24 bytes, maintask.o(i.ReadMAX11254Results))
  [Stack]

  - Max Depth = 136
  - Call Chain = ReadMAX11254Results ⇒ SPIx_WriteRead_2 ⇒ SPIx_Error ⇒ SPIx_Init ⇒ SPIx_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> SPIx_WriteRead_2
  - >> HAL_GPIO_WritePin
  [Called By]
  - >> Calibration
  - >> MainTask

  SPIx_Error (Thumb, 16 bytes, Stack size 8 bytes, stm32f429i_discovery.o(i.SPIx_Error))
  [Stack]

  - Max Depth = 96
  - Call Chain = SPIx_Error ⇒ SPIx_Init ⇒ SPIx_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> SPIx_Init
  - >> HAL_SPI_DeInit
  [Called By]
  - >> SPIx_Write_2
  - >> SPIx_WriteRead_2
  - >> SPIx_Write

  SPIx_Init (Thumb, 70 bytes, Stack size 8 bytes, stm32f429i_discovery.o(i.SPIx_Init))
  [Stack]

  - Max Depth = 88
  - Call Chain = SPIx_Init ⇒ SPIx_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_SPI_Init
  - >> HAL_SPI_GetState
  - >> SPIx_MspInit
  [Called By]
  - >> ConfigureSPIandGPIO
  - >> SPIx_Error
  - >> LCD_IO_Init

  SPIx_MspInit (Thumb, 106 bytes, Stack size 40 bytes, stm32f429i_discovery.o(i.SPIx_MspInit))
  [Stack]

  - Max Depth = 80
  - Call Chain = SPIx_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> SPIx_Init

  SPIx_Write (Thumb, 26 bytes, Stack size 8 bytes, stm32f429i_discovery.o(i.SPIx_Write))
  [Stack]

  - Max Depth = 104
  - Call Chain = SPIx_Write ⇒ SPIx_Error ⇒ SPIx_Init ⇒ SPIx_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_SPI_Transmit
  - >> SPIx_Error
  [Called By]
  - >> LCD_IO_WriteReg
  - >> LCD_IO_WriteData

  SPIx_WriteRead_2 (Thumb, 32 bytes, Stack size 16 bytes, stm32f429i_discovery.o(i.SPIx_WriteRead_2))
  [Stack]

  - Max Depth = 112
  - Call Chain = SPIx_WriteRead_2 ⇒ SPIx_Error ⇒ SPIx_Init ⇒ SPIx_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_SPI_TransmitReceive
  - >> SPIx_Error
  [Called By]
  - >> ReadMAX11254Results

  SPIx_Write_2 (Thumb, 30 bytes, Stack size 8 bytes, stm32f429i_discovery.o(i.SPIx_Write_2))
  [Stack]

  - Max Depth = 104
  - Call Chain = SPIx_Write_2 ⇒ SPIx_Error ⇒ SPIx_Init ⇒ SPIx_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_SPI_Transmit
  - >> SPIx_Error
  [Called By]
  - >> ConfigureMAX11254
  - >> Calibration
  - >> MainTask

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  SysTick_Handler (Thumb, 16 bytes, Stack size 8 bytes, stm32f4xx_it.o(i.SysTick_Handler))
  [Stack]

  - Max Depth = 8
  - Call Chain = SysTick_Handler
  [Calls]
  - >> HAL_IncTick
  [Address Reference Count : 1]
  - startup_stm32f429xx.o(RESET)

  SystemInit (Thumb, 66 bytes, Stack size 0 bytes, system_stm32f4xx.o(i.SystemInit))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(.text)

  TIM3_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.TIM3_IRQHandler))
  [Stack]

  - Max Depth = 96
  - Call Chain = TIM3_IRQHandler ⇒ HAL_TIM_IRQHandler ⇒ HAL_TIM_PeriodElapsedCallback ⇒ USBD_CDC_TransmitPacket ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> HAL_TIM_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f429xx.o(RESET)

  TIM_Base_SetConfig (Thumb, 148 bytes, Stack size 20 bytes, stm32f4xx_hal_tim.o(i.TIM_Base_SetConfig))
  [Stack]

  - Max Depth = 20
  - Call Chain = TIM_Base_SetConfig
  [Called By]
  - >> HAL_TIM_Base_Init

  USART1_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.USART1_IRQHandler))
  [Stack]

  - Max Depth = 80
  - Call Chain = USART1_IRQHandler ⇒ HAL_UART_IRQHandler ⇒ HAL_UART_TxCpltCallback ⇒ USBD_CDC_ReceivePacket ⇒ USBD_LL_PrepareReceive ⇒ HAL_PCD_EP_Receive ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> HAL_UART_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f429xx.o(RESET)

  USBD_CDC_GetDeviceQualifierDescriptor (Thumb, 8 bytes, Stack size 0 bytes, usbd_cdc.o(i.USBD_CDC_GetDeviceQualifierDescriptor))
  [Address Reference Count : 1]

  - usbd_cdc.o(.data)

  USBD_CDC_ReceivePacket (Thumb, 40 bytes, Stack size 8 bytes, usbd_cdc.o(i.USBD_CDC_ReceivePacket))
  [Stack]

  - Max Depth = 56
  - Call Chain = USBD_CDC_ReceivePacket ⇒ USBD_LL_PrepareReceive ⇒ HAL_PCD_EP_Receive ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_PrepareReceive
  [Called By]
  - >> HAL_UART_TxCpltCallback

  USBD_CDC_RegisterInterface (Thumb, 16 bytes, Stack size 0 bytes, usbd_cdc.o(i.USBD_CDC_RegisterInterface))
  [Called By]

  - >> main

  USBD_CDC_SetRxBuffer (Thumb, 12 bytes, Stack size 0 bytes, usbd_cdc.o(i.USBD_CDC_SetRxBuffer))
  [Called By]

  - >> CDC_Itf_Init

  USBD_CDC_SetTxBuffer (Thumb, 16 bytes, Stack size 0 bytes, usbd_cdc.o(i.USBD_CDC_SetTxBuffer))
  [Called By]

  - >> HAL_TIM_PeriodElapsedCallback
  - >> CDC_Itf_Init
  - >> MainTask

  USBD_CDC_TransmitPacket (Thumb, 48 bytes, Stack size 8 bytes, usbd_cdc.o(i.USBD_CDC_TransmitPacket))
  [Stack]

  - Max Depth = 64
  - Call Chain = USBD_CDC_TransmitPacket ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_Transmit
  [Called By]
  - >> HAL_TIM_PeriodElapsedCallback
  - >> MainTask

  USBD_ClrClassConfig (Thumb, 14 bytes, Stack size 8 bytes, usbd_core.o(i.USBD_ClrClassConfig))
  [Stack]

  - Max Depth = 8
  - Call Chain = USBD_ClrClassConfig
  [Called By]
  - >> USBD_SetConfig

  USBD_CtlContinueRx (Thumb, 16 bytes, Stack size 8 bytes, usbd_ioreq.o(i.USBD_CtlContinueRx))
  [Stack]

  - Max Depth = 56
  - Call Chain = USBD_CtlContinueRx ⇒ USBD_LL_PrepareReceive ⇒ HAL_PCD_EP_Receive ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_PrepareReceive
  [Called By]
  - >> USBD_LL_DataOutStage

  USBD_CtlContinueSendData (Thumb, 16 bytes, Stack size 8 bytes, usbd_ioreq.o(i.USBD_CtlContinueSendData))
  [Stack]

  - Max Depth = 64
  - Call Chain = USBD_CtlContinueSendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_Transmit
  [Called By]
  - >> USBD_LL_DataInStage

  USBD_CtlError (Thumb, 22 bytes, Stack size 8 bytes, usbd_ctlreq.o(i.USBD_CtlError))
  [Stack]

  - Max Depth = 32
  - Call Chain = USBD_CtlError ⇒ USBD_LL_StallEP ⇒ HAL_PCD_EP_SetStall
  [Calls]
  - >> USBD_LL_StallEP
  [Called By]
  - >> USBD_StdItfReq
  - >> USBD_StdEPReq
  - >> USBD_StdDevReq
  - >> USBD_SetConfig
  - >> USBD_GetDescriptor

  USBD_CtlPrepareRx (Thumb, 30 bytes, Stack size 8 bytes, usbd_ioreq.o(i.USBD_CtlPrepareRx))
  [Stack]

  - Max Depth = 56
  - Call Chain = USBD_CtlPrepareRx ⇒ USBD_LL_PrepareReceive ⇒ HAL_PCD_EP_Receive ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_PrepareReceive
  [Called By]
  - >> USBD_CDC_Setup

  USBD_CtlReceiveStatus (Thumb, 22 bytes, Stack size 8 bytes, usbd_ioreq.o(i.USBD_CtlReceiveStatus))
  [Stack]

  - Max Depth = 56
  - Call Chain = USBD_CtlReceiveStatus ⇒ USBD_LL_PrepareReceive ⇒ HAL_PCD_EP_Receive ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_PrepareReceive
  [Called By]
  - >> USBD_LL_DataInStage

  USBD_CtlSendData (Thumb, 26 bytes, Stack size 8 bytes, usbd_ioreq.o(i.USBD_CtlSendData))
  [Stack]

  - Max Depth = 64
  - Call Chain = USBD_CtlSendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_Transmit
  [Called By]
  - >> USBD_CDC_Setup
  - >> USBD_StdEPReq
  - >> USBD_StdDevReq
  - >> USBD_GetDescriptor

  USBD_CtlSendStatus (Thumb, 22 bytes, Stack size 8 bytes, usbd_ioreq.o(i.USBD_CtlSendStatus))
  [Stack]

  - Max Depth = 64
  - Call Chain = USBD_CtlSendStatus ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_Transmit
  [Called By]
  - >> USBD_LL_DataOutStage
  - >> USBD_StdItfReq
  - >> USBD_StdEPReq
  - >> USBD_StdDevReq
  - >> USBD_SetConfig

  USBD_GetString (Thumb, 70 bytes, Stack size 16 bytes, usbd_ctlreq.o(i.USBD_GetString))
  [Stack]

  - Max Depth = 16
  - Call Chain = USBD_GetString
  [Called By]
  - >> USBD_VCP_ProductStrDescriptor
  - >> USBD_VCP_ManufacturerStrDescriptor
  - >> USBD_VCP_InterfaceStrDescriptor
  - >> USBD_VCP_ConfigStrDescriptor

  USBD_Init (Thumb, 42 bytes, Stack size 8 bytes, usbd_core.o(i.USBD_Init))
  [Stack]

  - Max Depth = 160
  - Call Chain = USBD_Init ⇒ USBD_LL_Init ⇒ HAL_PCD_Init ⇒ HAL_PCD_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> USBD_LL_Init
  [Called By]
  - >> main

  USBD_LL_ClearStallEP (Thumb, 14 bytes, Stack size 8 bytes, usbd_conf.o(i.USBD_LL_ClearStallEP))
  [Stack]

  - Max Depth = 24
  - Call Chain = USBD_LL_ClearStallEP ⇒ HAL_PCD_EP_ClrStall
  [Calls]
  - >> HAL_PCD_EP_ClrStall
  [Called By]
  - >> USBD_StdEPReq

  USBD_LL_CloseEP (Thumb, 14 bytes, Stack size 8 bytes, usbd_conf.o(i.USBD_LL_CloseEP))
  [Stack]

  - Max Depth = 28
  - Call Chain = USBD_LL_CloseEP ⇒ HAL_PCD_EP_Close ⇒ USB_DeactivateEndpoint
  [Calls]
  - >> HAL_PCD_EP_Close
  [Called By]
  - >> USBD_CDC_DeInit

  USBD_LL_DataInStage (Thumb, 170 bytes, Stack size 24 bytes, usbd_core.o(i.USBD_LL_DataInStage))
  [Stack]

  - Max Depth = 88
  - Call Chain = USBD_LL_DataInStage ⇒ USBD_CtlContinueSendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_PrepareReceive
  - >> USBD_CtlReceiveStatus
  - >> USBD_CtlContinueSendData
  [Called By]
  - >> HAL_PCD_DataInStageCallback

  USBD_LL_DataOutStage (Thumb, 106 bytes, Stack size 16 bytes, usbd_core.o(i.USBD_LL_DataOutStage))
  [Stack]

  - Max Depth = 80
  - Call Chain = USBD_LL_DataOutStage ⇒ USBD_CtlSendStatus ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_CtlContinueRx
  - >> USBD_CtlSendStatus
  [Called By]
  - >> HAL_PCD_DataOutStageCallback

  USBD_LL_DevConnected (Thumb, 4 bytes, Stack size 0 bytes, usbd_core.o(i.USBD_LL_DevConnected))
  [Called By]

  - >> HAL_PCD_ConnectCallback

  USBD_LL_DevDisconnected (Thumb, 22 bytes, Stack size 8 bytes, usbd_core.o(i.USBD_LL_DevDisconnected))
  [Stack]

  - Max Depth = 8
  - Call Chain = USBD_LL_DevDisconnected
  [Called By]
  - >> HAL_PCD_DisconnectCallback

  USBD_LL_GetRxDataSize (Thumb, 8 bytes, Stack size 0 bytes, usbd_conf.o(i.USBD_LL_GetRxDataSize))
  [Calls]

  - >> HAL_PCD_EP_GetRxCount
  [Called By]
  - >> USBD_CDC_DataOut

  USBD_LL_Init (Thumb, 92 bytes, Stack size 8 bytes, usbd_conf.o(i.USBD_LL_Init))
  [Stack]

  - Max Depth = 152
  - Call Chain = USBD_LL_Init ⇒ HAL_PCD_Init ⇒ HAL_PCD_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_PCD_Init
  - >> HAL_PCDEx_SetTxFiFo
  - >> HAL_PCDEx_SetRxFiFo
  [Called By]
  - >> USBD_Init

  USBD_LL_IsStallEP (Thumb, 32 bytes, Stack size 0 bytes, usbd_conf.o(i.USBD_LL_IsStallEP))
  [Called By]

  - >> USBD_StdEPReq

  USBD_LL_IsoINIncomplete (Thumb, 4 bytes, Stack size 0 bytes, usbd_core.o(i.USBD_LL_IsoINIncomplete))
  [Called By]

  - >> HAL_PCD_ISOINIncompleteCallback

  USBD_LL_IsoOUTIncomplete (Thumb, 4 bytes, Stack size 0 bytes, usbd_core.o(i.USBD_LL_IsoOUTIncomplete))
  [Called By]

  - >> HAL_PCD_ISOOUTIncompleteCallback

  USBD_LL_OpenEP (Thumb, 20 bytes, Stack size 8 bytes, usbd_conf.o(i.USBD_LL_OpenEP))
  [Stack]

  - Max Depth = 36
  - Call Chain = USBD_LL_OpenEP ⇒ HAL_PCD_EP_Open ⇒ USB_ActivateEndpoint
  [Calls]
  - >> HAL_PCD_EP_Open
  [Called By]
  - >> USBD_LL_Reset
  - >> USBD_CDC_Init

  USBD_LL_PrepareReceive (Thumb, 8 bytes, Stack size 0 bytes, usbd_conf.o(i.USBD_LL_PrepareReceive))
  [Stack]

  - Max Depth = 48
  - Call Chain = USBD_LL_PrepareReceive ⇒ HAL_PCD_EP_Receive ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> HAL_PCD_EP_Receive
  [Called By]
  - >> USBD_CDC_ReceivePacket
  - >> USBD_LL_DataInStage
  - >> USBD_CtlPrepareRx
  - >> USBD_CDC_Init
  - >> USBD_CtlReceiveStatus
  - >> USBD_CtlContinueRx

  USBD_LL_Reset (Thumb, 62 bytes, Stack size 16 bytes, usbd_core.o(i.USBD_LL_Reset))
  [Stack]

  - Max Depth = 52
  - Call Chain = USBD_LL_Reset ⇒ USBD_LL_OpenEP ⇒ HAL_PCD_EP_Open ⇒ USB_ActivateEndpoint
  [Calls]
  - >> USBD_LL_OpenEP
  [Called By]
  - >> HAL_PCD_ResetCallback

  USBD_LL_Resume (Thumb, 12 bytes, Stack size 0 bytes, usbd_core.o(i.USBD_LL_Resume))
  [Called By]

  - >> HAL_PCD_ResumeCallback

  USBD_LL_SOF (Thumb, 24 bytes, Stack size 8 bytes, usbd_core.o(i.USBD_LL_SOF))
  [Stack]

  - Max Depth = 8
  - Call Chain = USBD_LL_SOF
  [Called By]
  - >> HAL_PCD_SOFCallback

  USBD_LL_SetSpeed (Thumb, 6 bytes, Stack size 0 bytes, usbd_core.o(i.USBD_LL_SetSpeed))
  [Called By]

  - >> HAL_PCD_ResetCallback

  USBD_LL_SetUSBAddress (Thumb, 14 bytes, Stack size 8 bytes, usbd_conf.o(i.USBD_LL_SetUSBAddress))
  [Stack]

  - Max Depth = 16
  - Call Chain = USBD_LL_SetUSBAddress ⇒ HAL_PCD_SetAddress
  [Calls]
  - >> HAL_PCD_SetAddress
  [Called By]
  - >> USBD_StdDevReq

  USBD_LL_SetupStage (Thumb, 90 bytes, Stack size 16 bytes, usbd_core.o(i.USBD_LL_SetupStage))
  [Stack]

  - Max Depth = 128
  - Call Chain = USBD_LL_SetupStage ⇒ USBD_StdDevReq ⇒ USBD_GetDescriptor ⇒ USBD_CtlSendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_StallEP
  - >> USBD_StdItfReq
  - >> USBD_StdEPReq
  - >> USBD_StdDevReq
  - >> USBD_ParseSetupRequest
  [Called By]
  - >> HAL_PCD_SetupStageCallback

  USBD_LL_StallEP (Thumb, 14 bytes, Stack size 8 bytes, usbd_conf.o(i.USBD_LL_StallEP))
  [Stack]

  - Max Depth = 24
  - Call Chain = USBD_LL_StallEP ⇒ HAL_PCD_EP_SetStall
  [Calls]
  - >> HAL_PCD_EP_SetStall
  [Called By]
  - >> USBD_LL_SetupStage
  - >> USBD_StdEPReq
  - >> USBD_CtlError

  USBD_LL_Start (Thumb, 14 bytes, Stack size 8 bytes, usbd_conf.o(i.USBD_LL_Start))
  [Stack]

  - Max Depth = 40
  - Call Chain = USBD_LL_Start ⇒ HAL_PCD_Start ⇒ USB_DevConnect ⇒ HAL_Delay
  [Calls]
  - >> HAL_PCD_Start
  [Called By]
  - >> USBD_Start

  USBD_LL_Suspend (Thumb, 18 bytes, Stack size 0 bytes, usbd_core.o(i.USBD_LL_Suspend))
  [Called By]

  - >> HAL_PCD_SuspendCallback

  USBD_LL_Transmit (Thumb, 14 bytes, Stack size 8 bytes, usbd_conf.o(i.USBD_LL_Transmit))
  [Stack]

  - Max Depth = 56
  - Call Chain = USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> HAL_PCD_EP_Transmit
  [Called By]
  - >> USBD_CDC_TransmitPacket
  - >> USBD_CtlSendData
  - >> USBD_CtlContinueSendData
  - >> USBD_CtlSendStatus

  USBD_ParseSetupRequest (Thumb, 40 bytes, Stack size 0 bytes, usbd_ctlreq.o(i.USBD_ParseSetupRequest))
  [Called By]

  - >> USBD_LL_SetupStage

  USBD_RegisterClass (Thumb, 16 bytes, Stack size 0 bytes, usbd_core.o(i.USBD_RegisterClass))
  [Called By]

  - >> main

  USBD_SetClassConfig (Thumb, 22 bytes, Stack size 8 bytes, usbd_core.o(i.USBD_SetClassConfig))
  [Stack]

  - Max Depth = 8
  - Call Chain = USBD_SetClassConfig
  [Called By]
  - >> USBD_SetConfig

  USBD_Start (Thumb, 10 bytes, Stack size 8 bytes, usbd_core.o(i.USBD_Start))
  [Stack]

  - Max Depth = 48
  - Call Chain = USBD_Start ⇒ USBD_LL_Start ⇒ HAL_PCD_Start ⇒ USB_DevConnect ⇒ HAL_Delay
  [Calls]
  - >> USBD_LL_Start
  [Called By]
  - >> main

  USBD_StdDevReq (Thumb, 242 bytes, Stack size 24 bytes, usbd_ctlreq.o(i.USBD_StdDevReq))
  [Stack]

  - Max Depth = 112
  - Call Chain = USBD_StdDevReq ⇒ USBD_GetDescriptor ⇒ USBD_CtlSendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_SetUSBAddress
  - >> USBD_CtlSendData
  - >> USBD_CtlSendStatus
  - >> USBD_CtlError
  - >> USBD_SetConfig
  - >> USBD_GetDescriptor
  [Called By]
  - >> USBD_LL_SetupStage

  USBD_StdEPReq (Thumb, 220 bytes, Stack size 16 bytes, usbd_ctlreq.o(i.USBD_StdEPReq))
  [Stack]

  - Max Depth = 80
  - Call Chain = USBD_StdEPReq ⇒ USBD_CtlSendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_StallEP
  - >> USBD_LL_IsStallEP
  - >> USBD_LL_ClearStallEP
  - >> USBD_CtlSendData
  - >> USBD_CtlSendStatus
  - >> USBD_CtlError
  [Called By]
  - >> USBD_LL_SetupStage

  USBD_StdItfReq (Thumb, 52 bytes, Stack size 16 bytes, usbd_ctlreq.o(i.USBD_StdItfReq))
  [Stack]

  - Max Depth = 80
  - Call Chain = USBD_StdItfReq ⇒ USBD_CtlSendStatus ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_CtlSendStatus
  - >> USBD_CtlError
  [Called By]
  - >> USBD_LL_SetupStage

  USBD_VCP_ConfigStrDescriptor (Thumb, 16 bytes, Stack size 8 bytes, usbd_desc.o(i.USBD_VCP_ConfigStrDescriptor))
  [Stack]

  - Max Depth = 24
  - Call Chain = USBD_VCP_ConfigStrDescriptor ⇒ USBD_GetString
  [Calls]
  - >> USBD_GetString
  [Address Reference Count : 1]
  - usbd_desc.o(.data)

  USBD_VCP_DeviceDescriptor (Thumb, 8 bytes, Stack size 0 bytes, usbd_desc.o(i.USBD_VCP_DeviceDescriptor))
  [Address Reference Count : 1]

  - usbd_desc.o(.data)

  USBD_VCP_InterfaceStrDescriptor (Thumb, 16 bytes, Stack size 8 bytes, usbd_desc.o(i.USBD_VCP_InterfaceStrDescriptor))
  [Stack]

  - Max Depth = 24
  - Call Chain = USBD_VCP_InterfaceStrDescriptor ⇒ USBD_GetString
  [Calls]
  - >> USBD_GetString
  [Address Reference Count : 1]
  - usbd_desc.o(.data)

  USBD_VCP_LangIDStrDescriptor (Thumb, 8 bytes, Stack size 0 bytes, usbd_desc.o(i.USBD_VCP_LangIDStrDescriptor))
  [Address Reference Count : 1]

  - usbd_desc.o(.data)

  USBD_VCP_ManufacturerStrDescriptor (Thumb, 16 bytes, Stack size 8 bytes, usbd_desc.o(i.USBD_VCP_ManufacturerStrDescriptor))
  [Stack]

  - Max Depth = 24
  - Call Chain = USBD_VCP_ManufacturerStrDescriptor ⇒ USBD_GetString
  [Calls]
  - >> USBD_GetString
  [Address Reference Count : 1]
  - usbd_desc.o(.data)

  USBD_VCP_ProductStrDescriptor (Thumb, 24 bytes, Stack size 8 bytes, usbd_desc.o(i.USBD_VCP_ProductStrDescriptor))
  [Stack]

  - Max Depth = 24
  - Call Chain = USBD_VCP_ProductStrDescriptor ⇒ USBD_GetString
  [Calls]
  - >> USBD_GetString
  [Address Reference Count : 1]
  - usbd_desc.o(.data)

  USBD_VCP_SerialStrDescriptor (Thumb, 48 bytes, Stack size 8 bytes, usbd_desc.o(i.USBD_VCP_SerialStrDescriptor))
  [Stack]

  - Max Depth = 28
  - Call Chain = USBD_VCP_SerialStrDescriptor ⇒ IntToUnicode
  [Calls]
  - >> IntToUnicode
  [Address Reference Count : 1]
  - usbd_desc.o(.data)

  USB_ActivateEndpoint (Thumb, 122 bytes, Stack size 12 bytes, stm32f4xx_ll_usb.o(i.USB_ActivateEndpoint))
  [Stack]

  - Max Depth = 12
  - Call Chain = USB_ActivateEndpoint
  [Called By]
  - >> HAL_PCD_EP_Open

  USB_ActivateSetup (Thumb, 52 bytes, Stack size 0 bytes, stm32f4xx_ll_usb.o(i.USB_ActivateSetup))
  [Called By]

  - >> HAL_PCD_IRQHandler

  USB_CoreInit (Thumb, 104 bytes, Stack size 16 bytes, stm32f4xx_ll_usb.o(i.USB_CoreInit))
  [Stack]

  - Max Depth = 16
  - Call Chain = USB_CoreInit
  [Calls]
  - >> USB_CoreReset
  [Called By]
  - >> HAL_PCD_Init

  USB_DeactivateEndpoint (Thumb, 110 bytes, Stack size 12 bytes, stm32f4xx_ll_usb.o(i.USB_DeactivateEndpoint))
  [Stack]

  - Max Depth = 12
  - Call Chain = USB_DeactivateEndpoint
  [Called By]
  - >> HAL_PCD_EP_Close

  USB_DevConnect (Thumb, 24 bytes, Stack size 8 bytes, stm32f4xx_ll_usb.o(i.USB_DevConnect))
  [Stack]

  - Max Depth = 24
  - Call Chain = USB_DevConnect ⇒ HAL_Delay
  [Calls]
  - >> HAL_Delay
  [Called By]
  - >> HAL_PCD_Start

  USB_DevDisconnect (Thumb, 24 bytes, Stack size 8 bytes, stm32f4xx_ll_usb.o(i.USB_DevDisconnect))
  [Stack]

  - Max Depth = 24
  - Call Chain = USB_DevDisconnect ⇒ HAL_Delay
  [Calls]
  - >> HAL_Delay
  [Called By]
  - >> HAL_PCD_Init

  USB_DevInit (Thumb, 306 bytes, Stack size 32 bytes, stm32f4xx_ll_usb.o(i.USB_DevInit))
  [Stack]

  - Max Depth = 32
  - Call Chain = USB_DevInit
  [Calls]
  - >> USB_FlushTxFifo
  - >> USB_FlushRxFifo
  [Called By]
  - >> HAL_PCD_Init

  USB_DisableGlobalInt (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_ll_usb.o(i.USB_DisableGlobalInt))
  [Called By]

  - >> HAL_PCD_Init

  USB_EP0StartXfer (Thumb, 316 bytes, Stack size 12 bytes, stm32f4xx_ll_usb.o(i.USB_EP0StartXfer))
  [Stack]

  - Max Depth = 12
  - Call Chain = USB_EP0StartXfer
  [Called By]
  - >> HAL_PCD_EP_Transmit
  - >> HAL_PCD_EP_Receive

  USB_EP0_OutStart (Thumb, 62 bytes, Stack size 0 bytes, stm32f4xx_ll_usb.o(i.USB_EP0_OutStart))
  [Called By]

  - >> HAL_PCD_IRQHandler
  - >> HAL_PCD_EP_SetStall

  USB_EPClearStall (Thumb, 100 bytes, Stack size 0 bytes, stm32f4xx_ll_usb.o(i.USB_EPClearStall))
  [Called By]

  - >> HAL_PCD_EP_ClrStall

  USB_EPSetStall (Thumb, 94 bytes, Stack size 0 bytes, stm32f4xx_ll_usb.o(i.USB_EPSetStall))
  [Called By]

  - >> HAL_PCD_EP_SetStall

  USB_EPStartXfer (Thumb, 534 bytes, Stack size 20 bytes, stm32f4xx_ll_usb.o(i.USB_EPStartXfer))
  [Stack]

  - Max Depth = 32
  - Call Chain = USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USB_WritePacket
  [Called By]
  - >> HAL_PCD_EP_Transmit
  - >> HAL_PCD_EP_Receive

  USB_EnableGlobalInt (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_ll_usb.o(i.USB_EnableGlobalInt))
  [Called By]

  - >> HAL_PCD_Start

  USB_FlushRxFifo (Thumb, 28 bytes, Stack size 0 bytes, stm32f4xx_ll_usb.o(i.USB_FlushRxFifo))
  [Called By]

  - >> USB_DevInit

  USB_FlushTxFifo (Thumb, 32 bytes, Stack size 0 bytes, stm32f4xx_ll_usb.o(i.USB_FlushTxFifo))
  [Called By]

  - >> HAL_PCD_IRQHandler
  - >> USB_DevInit

  USB_GetDevSpeed (Thumb, 60 bytes, Stack size 0 bytes, stm32f4xx_ll_usb.o(i.USB_GetDevSpeed))
  [Called By]

  - >> HAL_PCD_IRQHandler

  USB_GetMode (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_ll_usb.o(i.USB_GetMode))
  [Called By]

  - >> HAL_PCD_IRQHandler

  USB_ReadDevAllInEpInterrupt (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_ll_usb.o(i.USB_ReadDevAllInEpInterrupt))
  [Called By]

  - >> HAL_PCD_IRQHandler

  USB_ReadDevAllOutEpInterrupt (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_ll_usb.o(i.USB_ReadDevAllOutEpInterrupt))
  [Called By]

  - >> HAL_PCD_IRQHandler

  USB_ReadDevInEPInterrupt (Thumb, 30 bytes, Stack size 0 bytes, stm32f4xx_ll_usb.o(i.USB_ReadDevInEPInterrupt))
  [Called By]

  - >> HAL_PCD_IRQHandler

  USB_ReadDevOutEPInterrupt (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_ll_usb.o(i.USB_ReadDevOutEPInterrupt))
  [Called By]

  - >> HAL_PCD_IRQHandler

  USB_ReadInterrupts (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_ll_usb.o(i.USB_ReadInterrupts))
  [Called By]

  - >> HAL_PCD_IRQHandler

  USB_ReadPacket (Thumb, 32 bytes, Stack size 8 bytes, stm32f4xx_ll_usb.o(i.USB_ReadPacket))
  [Stack]

  - Max Depth = 8
  - Call Chain = USB_ReadPacket
  [Called By]
  - >> HAL_PCD_IRQHandler

  USB_SetCurrentMode (Thumb, 44 bytes, Stack size 8 bytes, stm32f4xx_ll_usb.o(i.USB_SetCurrentMode))
  [Stack]

  - Max Depth = 24
  - Call Chain = USB_SetCurrentMode ⇒ HAL_Delay
  [Calls]
  - >> HAL_Delay
  [Called By]
  - >> HAL_PCD_Init

  USB_SetDevAddress (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_ll_usb.o(i.USB_SetDevAddress))
  [Called By]

  - >> HAL_PCD_SetAddress

  USB_WritePacket (Thumb, 40 bytes, Stack size 12 bytes, stm32f4xx_ll_usb.o(i.USB_WritePacket))
  [Stack]

  - Max Depth = 12
  - Call Chain = USB_WritePacket
  [Called By]
  - >> PCD_WriteEmptyTxFifo
  - >> USB_EPStartXfer

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.UsageFault_Handler))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f429xx.o(RESET)

  WM_Activate (Thumb, 12 bytes, Stack size 0 bytes, wm.o(i.WM_Activate))
  [Called By]

  - >> WM_Init
  - >> GUI_SelectLCD
  - >> GUI_MEMDEV_CopyToLCDAt

  WM_BringToBottom (Thumb, 126 bytes, Stack size 64 bytes, wm_bringtobottom.o(i.WM_BringToBottom))
  [Stack]

  - Max Depth = 184
  - Call Chain = WM_BringToBottom ⇒ WM__InvalidateRectEx ⇒ WM__InvalidateRect ⇒ WM__InvalidateRect (Cycle)
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> WM__GetPrevSibling
  - >> WM_GetParent
  - >> WM__InvalidateRectEx
  [Called By]
  - >> WM_CreateWindowAsChild

  WM_CreateWindowAsChild (Thumb, 316 bytes, Stack size 48 bytes, wm.o(i.WM_CreateWindowAsChild))
  [Stack]

  - Max Depth = 256
  - Call Chain = WM_CreateWindowAsChild ⇒ WM__SendMsgNoData ⇒ WM__SendMessage ⇒ WM_DefaultProc ⇒ WM_InvalidateWindow ⇒ WM_InvalidateRect ⇒ WM__InvalidateRectEx ⇒ WM__InvalidateRect ⇒ WM__InvalidateRect (Cycle)
  [Calls]
  - >> GUI_ALLOC_h2p
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> WM_SelectWindow
  - >> WM_InvalidateWindow
  - >> WM_BringToBottom
  - >> GUI_ALLOC_AllocZero
  - >> WM__SendMsgNoData
  - >> WM__InsertWindowIntoList
  [Called By]
  - >> WM_Init

  WM_Deactivate (Thumb, 14 bytes, Stack size 0 bytes, wm.o(i.WM_Deactivate))
  [Calls]

  - >> LCD_SetClipRectMax
  [Called By]
  - >> GUI_MEMDEV_Select

  WM_DefaultProc (Thumb, 70 bytes, Stack size 8 bytes, wm.o(i.WM_DefaultProc))
  [Stack]

  - Max Depth = 168
  - Call Chain = WM_DefaultProc ⇒ WM_InvalidateWindow ⇒ WM_InvalidateRect ⇒ WM__InvalidateRectEx ⇒ WM__InvalidateRect ⇒ WM__InvalidateRect (Cycle)
  [Calls]
  - >> WM_InvalidateWindow
  - >> WM__GetClientRectEx
  - >> WM_SendToParent
  [Called By]
  - >> cbBackWin
  - >> WM__SendMessage

  WM_DeleteTimer (Thumb, 32 bytes, Stack size 16 bytes, wm_timer.o(i.WM_DeleteTimer))
  [Stack]

  - Max Depth = 64
  - Call Chain = WM_DeleteTimer ⇒ GUI_TIMER_Delete ⇒ GUI_ALLOC_Free ⇒ _AddFreeMemory ⇒ _RemoveFreeBlock
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> GUI_ALLOC_Free
  - >> GUI_TIMER_Delete
  [Called By]
  - >> WM__DeleteAssocTimer

  WM_DeleteWindow (Thumb, 222 bytes, Stack size 24 bytes, wm.o(i.WM_DeleteWindow))
  [Stack]

  - Max Depth = 232
  - Call Chain = WM_DeleteWindow ⇒ WM__SendMsgNoData ⇒ WM__SendMessage ⇒ WM_DefaultProc ⇒ WM_InvalidateWindow ⇒ WM_InvalidateRect ⇒ WM__InvalidateRectEx ⇒ WM__InvalidateRect ⇒ WM__InvalidateRect (Cycle)
  [Calls]
  - >> GUI_ALLOC_h2p
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> GUI_ALLOC_Free
  - >> WM__DetachWindow
  - >> WM_SelectWindow
  - >> _DeleteAllChildren
  - >> WM__DeleteAssocTimer
  - >> WM_NotifyParent
  - >> GUI_MEMDEV_Delete
  - >> WM__SendMsgNoData
  - >> WM__IsWindow
  - >> WM__GetTopLevelLayer
  [Called By]
  - >> _Exec1Input
  - >> _DeleteAllChildren

  WM_Exec (Thumb, 110 bytes, Stack size 24 bytes, wm.o(i.WM_Exec))
  [Stack]

  - Max Depth = 648
  - Call Chain = WM_Exec ⇒ _DrawNext ⇒ WM__Paint ⇒ GUI_MEMDEV_Draw ⇒ GUI_MEMDEV_CopyToLCD ⇒ GUI_MEMDEV_CopyToLCDAt ⇒ GUI_MEMDEV__WriteToActiveOpaque ⇒ _WriteToActiveOpaque_8 ⇒ LCD__DrawBitmap_1bpp ⇒ LCD_FillRect
  [Calls]
  - >> _Exec1Input
  - >> _DrawNext
  - >> GUI__ManageCache
  [Called By]
  - >> GUI_Exec1

  WM_GetClientRect (Thumb, 18 bytes, Stack size 0 bytes, wm_getclientrect.o(i.WM_GetClientRect))
  [Stack]

  - Max Depth = 16
  - Call Chain = WM_GetClientRect ⇒ WM_GetClientRectEx ⇒ WM__GetClientRectEx
  [Calls]
  - >> WM_GetClientRectEx
  [Called By]
  - >> GUI_GetClientRect

  WM_GetClientRectEx (Thumb, 4 bytes, Stack size 0 bytes, wm_getclientrect.o(i.WM_GetClientRectEx))
  [Stack]

  - Max Depth = 16
  - Call Chain = WM_GetClientRectEx ⇒ WM__GetClientRectEx
  [Calls]
  - >> WM__GetClientRectEx
  [Called By]
  - >> WM_GetClientRect

  WM_GetDesktopWindow (Thumb, 14 bytes, Stack size 0 bytes, wm_getdesktopwindow.o(i.WM_GetDesktopWindow))
  [Called By]

  - >> _InitContext
  - >> _CreateStaticDevice

  WM_GetFirstChild (Thumb, 14 bytes, Stack size 8 bytes, wm_getfirstchild.o(i.WM_GetFirstChild))
  [Stack]

  - Max Depth = 8
  - Call Chain = WM_GetFirstChild
  [Calls]
  - >> GUI_ALLOC_h2p
  [Called By]
  - >> WM_InvalidateWindowAndDescsEx
  - >> WM__InvalidateDrawAndDescs

  WM_GetParent (Thumb, 14 bytes, Stack size 8 bytes, wm_getparent.o(i.WM_GetParent))
  [Stack]

  - Max Depth = 8
  - Call Chain = WM_GetParent
  [Calls]
  - >> GUI_ALLOC_h2p
  [Called By]
  - >> WM__GetFirstSibling
  - >> WM_SendToParent
  - >> WM_BringToBottom

  WM_GetWindowOrgX (Thumb, 22 bytes, Stack size 8 bytes, wm_getorg.o(i.WM_GetWindowOrgX))
  [Stack]

  - Max Depth = 8
  - Call Chain = WM_GetWindowOrgX
  [Calls]
  - >> GUI_ALLOC_h2p
  [Called By]
  - >> _CreateStaticDevice

  WM_GetWindowRect (Thumb, 32 bytes, Stack size 8 bytes, wm_getwindowrect.o(i.WM_GetWindowRect))
  [Stack]

  - Max Depth = 8
  - Call Chain = WM_GetWindowRect
  [Calls]
  - >> GUI_ALLOC_h2p
  [Called By]
  - >> _TransformPoint

  WM_Init (Thumb, 184 bytes, Stack size 56 bytes, wm.o(i.WM_Init))
  [Stack]

  - Max Depth = 312
  - Call Chain = WM_Init ⇒ WM_CreateWindowAsChild ⇒ WM__SendMsgNoData ⇒ WM__SendMessage ⇒ WM_DefaultProc ⇒ WM_InvalidateWindow ⇒ WM_InvalidateRect ⇒ WM__InvalidateRectEx ⇒ WM__InvalidateRect ⇒ WM__InvalidateRect (Cycle)
  [Calls]
  - >> GUI_DEVICE__GetpDriver
  - >> GUI__RegisterExit
  - >> WM_SelectWindow
  - >> WM_InvalidateWindow
  - >> WM_CreateWindowAsChild
  - >> WM_Activate
  - >> WM__AddCriticalHandle
  [Called By]
  - >> GUI_Init

  WM_InvalidateRect (Thumb, 118 bytes, Stack size 40 bytes, wm.o(i.WM_InvalidateRect))
  [Stack]

  - Max Depth = 160
  - Call Chain = WM_InvalidateRect ⇒ WM__InvalidateRectEx ⇒ WM__InvalidateRect ⇒ WM__InvalidateRect (Cycle)
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> WM__ClipAtParentBorders
  - >> WM__Client2Screen
  - >> GUI__IntersectRect
  - >> WM__InvalidateRectEx
  - >> WM__InvalidateDrawAndDescs
  - >> WM__Invalidate1Abs
  [Called By]
  - >> WM_InvalidateWindow

  WM_InvalidateWindow (Thumb, 6 bytes, Stack size 0 bytes, wm.o(i.WM_InvalidateWindow))
  [Stack]

  - Max Depth = 160
  - Call Chain = WM_InvalidateWindow ⇒ WM_InvalidateRect ⇒ WM__InvalidateRectEx ⇒ WM__InvalidateRect ⇒ WM__InvalidateRect (Cycle)
  [Calls]
  - >> WM_InvalidateRect
  [Called By]
  - >> WM_Init
  - >> WM_DefaultProc
  - >> WM_CreateWindowAsChild

  WM_InvalidateWindowAndDescsEx (Thumb, 94 bytes, Stack size 32 bytes, wm.o(i.WM_InvalidateWindowAndDescsEx))
  [Stack]

  - Max Depth = 80 + In Cycle
  - Call Chain = WM_InvalidateWindowAndDescsEx ⇒ WM_InvalidateWindowAndDescsEx (Cycle)
  [Calls]
  - >> GUI__IntersectRects
  - >> GUI_ALLOC_h2p
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> WM_InvalidateWindowAndDescsEx
  - >> _Invalidate1Abs
  - >> WM_GetFirstChild
  [Called By]
  - >> WM_InvalidateWindowAndDescsEx
  - >> WM__InvalidateRect

  WM_MoveWindow (Thumb, 4 bytes, Stack size 0 bytes, wm_move.o(i.WM_MoveWindow))
  [Stack]

  - Max Depth = 320
  - Call Chain = WM_MoveWindow ⇒ WM__MoveWindow ⇒ _MoveDescendents ⇒ _MoveDescendents (Cycle)
  [Calls]
  - >> WM__MoveWindow
  [Called By]
  - >> WM__UpdateChildPositions

  WM_NotifyParent (Thumb, 16 bytes, Stack size 24 bytes, wm_notifyparent.o(i.WM_NotifyParent))
  [Stack]

  - Max Depth = 48
  - Call Chain = WM_NotifyParent ⇒ WM_SendToParent ⇒ WM__SendMessage (Cycle)
  [Calls]
  - >> WM_SendToParent
  [Called By]
  - >> WM_DeleteWindow

  WM_OnKey (Thumb, 48 bytes, Stack size 32 bytes, wm_onkey.o(i.WM_OnKey))
  [Stack]

  - Max Depth = 216
  - Call Chain = WM_OnKey ⇒ WM__SendMessage ⇒ WM_DefaultProc ⇒ WM_InvalidateWindow ⇒ WM_InvalidateRect ⇒ WM__InvalidateRectEx ⇒ WM__InvalidateRect ⇒ WM__InvalidateRect (Cycle)
  [Calls]
  - >> WM__SendMessage
  [Called By]
  - >> GUI_PollKeyMsg

  WM_ResizeWindow (Thumb, 236 bytes, Stack size 56 bytes, wm_resizewindow.o(i.WM_ResizeWindow))
  [Stack]

  - Max Depth = 432
  - Call Chain = WM_ResizeWindow ⇒ WM__UpdateChildPositions ⇒ WM_ResizeWindow (Cycle)
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> GUI__IntersectRect
  - >> GUI_MergeRect
  - >> WM__SendMsgNoData
  - >> WM__InvalidateRectEx
  - >> WM__InvalidateDrawAndDescs
  - >> WM__UpdateChildPositions
  [Called By]
  - >> WM_SetSize
  - >> WM__UpdateChildPositions

  WM_SelectWindow (Thumb, 52 bytes, Stack size 16 bytes, wm.o(i.WM_SelectWindow))
  [Stack]

  - Max Depth = 56
  - Call Chain = WM_SelectWindow ⇒ WM__SelectTopLevelLayer ⇒ GUI_SelectLayer ⇒ GUI_SelectLCD ⇒ LCD_UpdateColorIndices
  [Calls]
  - >> GUI_ALLOC_h2p
  - >> LCD_SetClipRectMax
  - >> WM__SelectTopLevelLayer
  [Called By]
  - >> WM_Init
  - >> WM_DeleteWindow
  - >> WM_CreateWindowAsChild
  - >> WM__Paint

  WM_SendMessageNoPara (Thumb, 4 bytes, Stack size 0 bytes, wm_sendmessagenopara.o(i.WM_SendMessageNoPara))
  [Stack]

  - Max Depth = 32
  - Call Chain = WM_SendMessageNoPara ⇒ WM__SendMessageNoPara
  [Calls]
  - >> WM__SendMessageNoPara
  [Called By]
  - >> WM__Paint1

  WM_SendToParent (Thumb, 30 bytes, Stack size 16 bytes, wm_sendtoparent.o(i.WM_SendToParent))
  [Stack]

  - Max Depth = 24 + In Cycle
  - Call Chain = WM_SendToParent ⇒ WM__SendMessage (Cycle)
  [Calls]
  - >> WM_GetParent
  - >> WM__SendMessage
  [Called By]
  - >> WM_DefaultProc
  - >> WM_NotifyParent

  WM_SetDefault (Thumb, 16 bytes, Stack size 8 bytes, wm.o(i.WM_SetDefault))
  [Stack]

  - Max Depth = 16
  - Call Chain = WM_SetDefault ⇒ GL_SetDefault
  [Calls]
  - >> GL_SetDefault
  [Called By]
  - >> WM__Paint1

  WM_SetSize (Thumb, 62 bytes, Stack size 24 bytes, wm_setsize.o(i.WM_SetSize))
  [Stack]

  - Max Depth = 456
  - Call Chain = WM_SetSize ⇒ WM_ResizeWindow ⇒ WM__UpdateChildPositions ⇒ WM_ResizeWindow (Cycle)
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> WM_ResizeWindow
  [Called By]
  - >> _CreateStaticDevice

  WM_SetUserClipRect (Thumb, 18 bytes, Stack size 8 bytes, wm_setusercliprect.o(i.WM_SetUserClipRect))
  [Stack]

  - Max Depth = 88
  - Call Chain = WM_SetUserClipRect ⇒ WM__ActivateClipRect ⇒ _SetClipRectUserIntersect ⇒ LCD_SetClipRectEx ⇒ GUI__IntersectRects
  [Calls]
  - >> WM__ActivateClipRect
  [Called By]
  - >> GUI_DispStringInRectEx
  - >> GUI_DispStringInRectMax

  WM__ActivateClipRect (Thumb, 58 bytes, Stack size 16 bytes, wm.o(i.WM__ActivateClipRect))
  [Stack]

  - Max Depth = 80
  - Call Chain = WM__ActivateClipRect ⇒ _SetClipRectUserIntersect ⇒ LCD_SetClipRectEx ⇒ GUI__IntersectRects
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> WM__ClipAtParentBorders
  - >> _SetClipRectUserIntersect
  [Called By]
  - >> WM_SetUserClipRect
  - >> WM__InitIVRSearch
  - >> WM__GetNextIVR

  WM__AddCriticalHandle (Thumb, 10 bytes, Stack size 0 bytes, wm_criticalhandle.o(i.WM__AddCriticalHandle))
  [Called By]

  - >> WM_Init

  WM__Client2Screen (Thumb, 16 bytes, Stack size 0 bytes, wm.o(i.WM__Client2Screen))
  [Calls]

  - >> GUI_MoveRect
  [Called By]
  - >> WM__InitIVRSearch
  - >> WM_InvalidateRect
  - >> _SetClipRectUserIntersect

  WM__ClipAtParentBorders (Thumb, 78 bytes, Stack size 16 bytes, wm.o(i.WM__ClipAtParentBorders))
  [Stack]

  - Max Depth = 16
  - Call Chain = WM__ClipAtParentBorders
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> _DesktopHandle2Index
  - >> GUI__IntersectRect
  [Called By]
  - >> WM__InitIVRSearch
  - >> WM__ActivateClipRect
  - >> WM_InvalidateRect
  - >> WM__Paint

  WM__DeleteAssocTimer (Thumb, 74 bytes, Stack size 24 bytes, wm_timer.o(i.WM__DeleteAssocTimer))
  [Stack]

  - Max Depth = 88
  - Call Chain = WM__DeleteAssocTimer ⇒ WM_DeleteTimer ⇒ GUI_TIMER_Delete ⇒ GUI_ALLOC_Free ⇒ _AddFreeMemory ⇒ _RemoveFreeBlock
  [Calls]
  - >> GUI_ALLOC_h2p
  - >> GUI_TIMER__GetNextTimerLin
  - >> GUI_TIMER__GetFirstTimer
  - >> GUI_TIMER_GetFlag
  - >> WM_DeleteTimer
  [Called By]
  - >> WM_DeleteWindow

  WM__DetachWindow (Thumb, 40 bytes, Stack size 16 bytes, wm.o(i.WM__DetachWindow))
  [Stack]

  - Max Depth = 136
  - Call Chain = WM__DetachWindow ⇒ WM__InvalidateRectEx ⇒ WM__InvalidateRect ⇒ WM__InvalidateRect (Cycle)
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> WM__RemoveWindowFromList
  - >> WM__InvalidateRectEx
  [Called By]
  - >> WM_DeleteWindow

  WM__GetClientRectEx (Thumb, 32 bytes, Stack size 16 bytes, wm_getclientrect.o(i.WM__GetClientRectEx))
  [Stack]

  - Max Depth = 16
  - Call Chain = WM__GetClientRectEx
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> WM__GetClientRectWin
  [Called By]
  - >> WM_DefaultProc
  - >> WM_GetClientRectEx

  WM__GetClientRectWin (Thumb, 24 bytes, Stack size 0 bytes, wm.o(i.WM__GetClientRectWin))
  [Called By]

  - >> WM__GetClientRectEx

  WM__GetFirstSibling (Thumb, 18 bytes, Stack size 8 bytes, wm__getfirstsibling.o(i.WM__GetFirstSibling))
  [Stack]

  - Max Depth = 16
  - Call Chain = WM__GetFirstSibling ⇒ WM_GetParent
  [Calls]
  - >> GUI_ALLOC_h2p
  - >> WM_GetParent
  [Called By]
  - >> WM__GetPrevSibling

  WM__GetNextIVR (Thumb, 54 bytes, Stack size 8 bytes, wm.o(i.WM__GetNextIVR))
  [Stack]

  - Max Depth = 88
  - Call Chain = WM__GetNextIVR ⇒ WM__ActivateClipRect ⇒ _SetClipRectUserIntersect ⇒ LCD_SetClipRectEx ⇒ GUI__IntersectRects
  [Calls]
  - >> WM__ActivateClipRect
  - >> _FindNext_IVR
  [Called By]
  - >> GUI_FillCircle
  - >> GUI_ClearRect
  - >> GUI_FillRect
  - >> WM__InitIVRSearch
  - >> GUI__DispLine
  - >> GUI_MEMDEV_WriteAt
  - >> GUI_MEMDEV_CopyToLCDAt
  - >> WM__Paint1

  WM__GetPrevSibling (Thumb, 36 bytes, Stack size 16 bytes, wm__getprevsibling.o(i.WM__GetPrevSibling))
  [Stack]

  - Max Depth = 32
  - Call Chain = WM__GetPrevSibling ⇒ WM__GetFirstSibling ⇒ WM_GetParent
  [Calls]
  - >> GUI_ALLOC_h2p
  - >> WM__GetFirstSibling
  [Called By]
  - >> WM_BringToBottom

  WM__GetTopLevelLayer (Thumb, 24 bytes, Stack size 8 bytes, wm.o(i.WM__GetTopLevelLayer))
  [Stack]

  - Max Depth = 8
  - Call Chain = WM__GetTopLevelLayer
  [Calls]
  - >> GUI_ALLOC_h2p
  - >> _DesktopHandle2Index
  [Called By]
  - >> WM_DeleteWindow
  - >> WM__SelectTopLevelLayer

  WM__InitIVRSearch (Thumb, 228 bytes, Stack size 48 bytes, wm.o(i.WM__InitIVRSearch))
  [Stack]

  - Max Depth = 136
  - Call Chain = WM__InitIVRSearch ⇒ WM__GetNextIVR ⇒ WM__ActivateClipRect ⇒ _SetClipRectUserIntersect ⇒ LCD_SetClipRectEx ⇒ GUI__IntersectRects
  [Calls]
  - >> WM__GetNextIVR
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> WM__ClipAtParentBorders
  - >> WM__Client2Screen
  - >> WM__ActivateClipRect
  - >> GUI__IntersectRect
  [Called By]
  - >> GUI_FillCircle
  - >> GUI_ClearRect
  - >> GUI_FillRect
  - >> GUI__DispLine
  - >> GUI_MEMDEV_WriteAt
  - >> GUI_MEMDEV_CopyToLCDAt
  - >> WM__Paint1

  WM__InsertWindowIntoList (Thumb, 164 bytes, Stack size 32 bytes, wm.o(i.WM__InsertWindowIntoList))
  [Stack]

  - Max Depth = 32
  - Call Chain = WM__InsertWindowIntoList
  [Calls]
  - >> GUI_ALLOC_h2p
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  [Called By]
  - >> WM_CreateWindowAsChild

  WM__Invalidate1Abs (Thumb, 6 bytes, Stack size 0 bytes, wm.o(i.WM__Invalidate1Abs))
  [Stack]

  - Max Depth = 48
  - Call Chain = WM__Invalidate1Abs ⇒ _Invalidate1Abs ⇒ GUI__IntersectRects
  [Calls]
  - >> _Invalidate1Abs
  [Called By]
  - >> WM_InvalidateRect

  WM__InvalidateDrawAndDescs (Thumb, 78 bytes, Stack size 16 bytes, wm.o(i.WM__InvalidateDrawAndDescs))
  [Stack]

  - Max Depth = 88 + In Cycle
  - Call Chain = WM__InvalidateDrawAndDescs ⇒ WM__InvalidateDrawAndDescs (Cycle)
  [Calls]
  - >> GUI_ALLOC_h2p
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> WM_GetFirstChild
  - >> GUI_MEMDEV_Delete
  - >> WM__InvalidateDrawAndDescs
  [Called By]
  - >> WM_InvalidateRect
  - >> WM_ResizeWindow
  - >> WM__InvalidateDrawAndDescs

  WM__InvalidateParent (Thumb, 42 bytes, Stack size 16 bytes, wm.o(i.WM__InvalidateParent))
  [Stack]

  - Max Depth = 16
  - Call Chain = WM__InvalidateParent
  [Calls]
  - >> GUI_ALLOC_h2p
  [Called By]
  - >> WM__MoveWindow

  WM__InvalidateRect (Thumb, 118 bytes, Stack size 40 bytes, wm.o(i.WM__InvalidateRect))
  [Stack]

  - Max Depth = 120 + In Cycle
  - Call Chain = WM__InvalidateRect ⇒ WM__InvalidateRect (Cycle)
  [Calls]
  - >> GUI__IntersectRects
  - >> GUI_ALLOC_h2p
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> WM_InvalidateWindowAndDescsEx
  - >> _Invalidate1Abs
  - >> WM__InvalidateRect
  [Called By]
  - >> WM__InvalidateRectEx
  - >> WM__InvalidateRect

  WM__InvalidateRectEx (Thumb, 6 bytes, Stack size 0 bytes, wm.o(i.WM__InvalidateRectEx))
  [Stack]

  - Max Depth = 120
  - Call Chain = WM__InvalidateRectEx ⇒ WM__InvalidateRect ⇒ WM__InvalidateRect (Cycle)
  [Calls]
  - >> WM__InvalidateRect
  [Called By]
  - >> WM__DetachWindow
  - >> WM_InvalidateRect
  - >> WM_ResizeWindow
  - >> WM_BringToBottom

  WM__IsWindow (Thumb, 30 bytes, Stack size 8 bytes, wm.o(i.WM__IsWindow))
  [Stack]

  - Max Depth = 8
  - Call Chain = WM__IsWindow
  [Calls]
  - >> GUI_ALLOC_h2p
  [Called By]
  - >> WM_DeleteWindow

  WM__MoveWindow (Thumb, 154 bytes, Stack size 64 bytes, wm_move.o(i.WM__MoveWindow))
  [Stack]

  - Max Depth = 320
  - Call Chain = WM__MoveWindow ⇒ _MoveDescendents ⇒ _MoveDescendents (Cycle)
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> WM__SendMessage
  - >> GUI_MoveRect
  - >> WM__InvalidateParent
  - >> _MoveDescendents
  [Called By]
  - >> WM_MoveWindow

  WM__Paint (Thumb, 152 bytes, Stack size 56 bytes, wm.o(i.WM__Paint))
  [Stack]

  - Max Depth = 488
  - Call Chain = WM__Paint ⇒ GUI_MEMDEV_Draw ⇒ GUI_MEMDEV_CopyToLCD ⇒ GUI_MEMDEV_CopyToLCDAt ⇒ GUI_MEMDEV__WriteToActiveOpaque ⇒ _WriteToActiveOpaque_8 ⇒ LCD__DrawBitmap_1bpp ⇒ LCD_FillRect
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> WM__ClipAtParentBorders
  - >> WM_SelectWindow
  - >> WM__PaintWinAndOverlays
  - >> GUI_MEMDEV_Draw
  [Called By]
  - >> _DrawNext

  WM__Paint1 (Thumb, 136 bytes, Stack size 56 bytes, wm.o(i.WM__Paint1))
  [Stack]

  - Max Depth = 240
  - Call Chain = WM__Paint1 ⇒ WM__SendMessage ⇒ WM_DefaultProc ⇒ WM_InvalidateWindow ⇒ WM_InvalidateRect ⇒ WM__InvalidateRectEx ⇒ WM__InvalidateRect ⇒ WM__InvalidateRect (Cycle)
  [Calls]
  - >> WM__InitIVRSearch
  - >> WM__GetNextIVR
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> WM_SetDefault
  - >> WM__SendMessage
  - >> WM_SendMessageNoPara
  [Called By]
  - >> _CreateStaticDevice
  [Address Reference Count : 1]
  - wm.o(i._Paint1)

  WM__RectIsNZ (Thumb, 32 bytes, Stack size 0 bytes, wm.o(i.WM__RectIsNZ))
  [Called By]

  - >> _Invalidate1Abs

  WM__RemoveWindowFromList (Thumb, 64 bytes, Stack size 16 bytes, wm.o(i.WM__RemoveWindowFromList))
  [Stack]

  - Max Depth = 16
  - Call Chain = WM__RemoveWindowFromList
  [Calls]
  - >> GUI_ALLOC_h2p
  [Called By]
  - >> WM__DetachWindow

  WM__SelectTopLevelLayer (Thumb, 20 bytes, Stack size 8 bytes, wm.o(i.WM__SelectTopLevelLayer))
  [Stack]

  - Max Depth = 40
  - Call Chain = WM__SelectTopLevelLayer ⇒ GUI_SelectLayer ⇒ GUI_SelectLCD ⇒ LCD_UpdateColorIndices
  [Calls]
  - >> GUI_SelectLayer
  - >> WM__GetTopLevelLayer
  [Called By]
  - >> WM_SelectWindow

  WM__SendMessage (Thumb, 54 bytes, Stack size 16 bytes, wm__sendmessage.o(i.WM__SendMessage))
  [Stack]

  - Max Depth = 184
  - Call Chain = WM__SendMessage ⇒ WM_DefaultProc ⇒ WM_InvalidateWindow ⇒ WM_InvalidateRect ⇒ WM__InvalidateRectEx ⇒ WM__InvalidateRect ⇒ WM__InvalidateRect (Cycle)
  [Calls]
  - >> GUI_ALLOC_h2p
  - >> WM_DefaultProc
  [Called By]
  - >> WM_OnKey
  - >> WM_SendToParent
  - >> WM__SendMsgNoData
  - >> WM__Paint1
  - >> WM__MoveWindow
  - >> _MoveDescendents

  WM__SendMessageNoPara (Thumb, 38 bytes, Stack size 32 bytes, wm__sendmessagenopara.o(i.WM__SendMessageNoPara))
  [Stack]

  - Max Depth = 32
  - Call Chain = WM__SendMessageNoPara
  [Calls]
  - >> GUI_ALLOC_h2p
  [Called By]
  - >> WM_SendMessageNoPara

  WM__SendMsgNoData (Thumb, 14 bytes, Stack size 24 bytes, wm.o(i.WM__SendMsgNoData))
  [Stack]

  - Max Depth = 208
  - Call Chain = WM__SendMsgNoData ⇒ WM__SendMessage ⇒ WM_DefaultProc ⇒ WM_InvalidateWindow ⇒ WM_InvalidateRect ⇒ WM__InvalidateRectEx ⇒ WM__InvalidateRect ⇒ WM__InvalidateRect (Cycle)
  [Calls]
  - >> WM__SendMessage
  [Called By]
  - >> WM_DeleteWindow
  - >> WM_CreateWindowAsChild
  - >> WM_ResizeWindow

  WM__UpdateChildPositions (Thumb, 220 bytes, Stack size 56 bytes, wm__updatechildpositions.o(i.WM__UpdateChildPositions))
  [Stack]

  - Max Depth = 376 + In Cycle
  - Call Chain = WM__UpdateChildPositions ⇒ WM_ResizeWindow (Cycle)
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> WM_ResizeWindow
  - >> WM_MoveWindow
  [Called By]
  - >> WM_ResizeWindow

  __0sprintf (Thumb, 34 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)
  [Calls]

  - >> _sputc
  - >> _printf_core

  __1sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)

  __2sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2sprintf
  [Called By]
  - >> MainTask

  __c89sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)

  sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  emWin_LCD_Init (Thumb, 138 bytes, Stack size 24 bytes, lcd.o(i.emWin_LCD_Init))
  [Stack]

  - Max Depth = 200
  - Call Chain = emWin_LCD_Init ⇒ LCD_InitColors ⇒ GUI_ALLOC_GetFixedBlock ⇒ _InitOnce ⇒ _EnlargeBlocks ⇒ _Alloc ⇒ _InitOnce (Cycle)
  [Calls]
  - >> LCD_FillRect
  - >> GUI_DEVICE__GetpDriver
  - >> LCD_SetDrawMode
  - >> LCD_InitLUT
  - >> LCD_InitColors
  - >> LCD_SetClipRectMax
  - >> GUI_SelectLayer
  [Called By]
  - >> GUI_Init

  free (Thumb, 76 bytes, Stack size 8 bytes, malloc.o(i.free))
  [Stack]

  - Max Depth = 8
  - Call Chain = free
  [Called By]
  - >> USBD_CDC_DeInit

  ili9341_Init (Thumb, 658 bytes, Stack size 8 bytes, ili9341.o(i.ili9341_Init))
  [Stack]

  - Max Depth = 144
  - Call Chain = ili9341_Init ⇒ LCD_IO_Init ⇒ SPIx_Init ⇒ SPIx_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> LCD_IO_WriteReg
  - >> LCD_IO_WriteData
  - >> LCD_IO_Init
  - >> LCD_Delay
  [Called By]
  - >> LCD_LL_Init

  main (Thumb, 92 bytes, Stack size 8 bytes, maxrefdes82.o(i.main))
  [Stack]

  - Max Depth = 2832
  - Call Chain = main ⇒ MainTask ⇒ Calibration ⇒ GUI_Delay ⇒ GUI_Exec ⇒ GUI_Exec1 ⇒ WM_Exec ⇒ _DrawNext ⇒ WM__Paint ⇒ GUI_MEMDEV_Draw ⇒ GUI_MEMDEV_CopyToLCD ⇒ GUI_MEMDEV_CopyToLCDAt ⇒ GUI_MEMDEV__WriteToActiveOpaque ⇒ _WriteToActiveOpaque_8 ⇒ LCD__DrawBitmap_1bpp ⇒ LCD_FillRect
  [Calls]
  - >> USBD_Start
  - >> USBD_RegisterClass
  - >> USBD_Init
  - >> USBD_CDC_RegisterInterface
  - >> MainTask
  - >> HAL_Init
  - >> GUI_Init
  - >> BSP_SDRAM_Init
  - >> BSP_LED_Init
  - >> SystemClock_Config
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  malloc (Thumb, 92 bytes, Stack size 20 bytes, malloc.o(i.malloc))
  [Stack]

  - Max Depth = 20
  - Call Chain = malloc
  [Called By]
  - >> USBD_CDC_Init

  ### Local Symbols

  IntToUnicode (Thumb, 56 bytes, Stack size 20 bytes, usbd_desc.o(i.IntToUnicode))
  [Stack]

  - Max Depth = 20
  - Call Chain = IntToUnicode
  [Called By]
  - >> USBD_VCP_SerialStrDescriptor

  CDC_Itf_Control (Thumb, 84 bytes, Stack size 8 bytes, usbd_cdc_interface.o(i.CDC_Itf_Control))
  [Stack]

  - Max Depth = 120
  - Call Chain = CDC_Itf_Control ⇒ ComPort_Config ⇒ HAL_UART_Init ⇒ HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> ComPort_Config
  [Address Reference Count : 1]
  - usbd_cdc_interface.o(.data)

  CDC_Itf_DeInit (Thumb, 12 bytes, Stack size 8 bytes, usbd_cdc_interface.o(i.CDC_Itf_DeInit))
  [Stack]

  - Max Depth = 60
  - Call Chain = CDC_Itf_DeInit ⇒ HAL_UART_DeInit ⇒ HAL_UART_MspDeInit ⇒ HAL_GPIO_DeInit
  [Calls]
  - >> HAL_UART_DeInit
  [Address Reference Count : 1]
  - usbd_cdc_interface.o(.data)

  CDC_Itf_Init (Thumb, 106 bytes, Stack size 8 bytes, usbd_cdc_interface.o(i.CDC_Itf_Init))
  [Stack]

  - Max Depth = 112
  - Call Chain = CDC_Itf_Init ⇒ HAL_UART_Init ⇒ HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> USBD_CDC_SetTxBuffer
  - >> USBD_CDC_SetRxBuffer
  - >> HAL_UART_Receive_IT
  - >> HAL_UART_Init
  - >> HAL_TIM_Base_Start_IT
  - >> HAL_TIM_Base_Init
  [Address Reference Count : 1]
  - usbd_cdc_interface.o(.data)

  CDC_Itf_Receive (Thumb, 18 bytes, Stack size 8 bytes, usbd_cdc_interface.o(i.CDC_Itf_Receive))
  [Stack]

  - Max Depth = 52
  - Call Chain = CDC_Itf_Receive ⇒ HAL_UART_Transmit_DMA ⇒ HAL_DMA_Start_IT ⇒ DMA_SetConfig
  [Calls]
  - >> HAL_UART_Transmit_DMA
  [Address Reference Count : 1]
  - usbd_cdc_interface.o(.data)

  ComPort_Config (Thumb, 126 bytes, Stack size 8 bytes, usbd_cdc_interface.o(i.ComPort_Config))
  [Stack]

  - Max Depth = 112
  - Call Chain = ComPort_Config ⇒ HAL_UART_Init ⇒ HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_UART_Receive_IT
  - >> HAL_UART_Init
  - >> HAL_UART_DeInit
  [Called By]
  - >> CDC_Itf_Control

  BSP_LCD_DrawBitmap16bpp (Thumb, 86 bytes, Stack size 48 bytes, lcdconf_stm32f429i_disco_mb1075_1.o(i.BSP_LCD_DrawBitmap16bpp))
  [Stack]

  - Max Depth = 80
  - Call Chain = BSP_LCD_DrawBitmap16bpp ⇒ DMA2D_CopyBuffer
  [Calls]
  - >> GetBufferSize
  - >> DMA2D_CopyBuffer
  [Address Reference Count : 1]
  - lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)

  BSP_LCD_DrawBitmap8bpp (Thumb, 116 bytes, Stack size 40 bytes, lcdconf_stm32f429i_disco_mb1075_1.o(i.BSP_LCD_DrawBitmap8bpp))
  [Stack]

  - Max Depth = 40
  - Call Chain = BSP_LCD_DrawBitmap8bpp
  [Calls]
  - >> LCD_LL_GetPixelformat
  - >> GetBufferSize
  [Address Reference Count : 1]
  - lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)

  CUSTOM_CopyBuffer (Thumb, 56 bytes, Stack size 32 bytes, lcdconf_stm32f429i_disco_mb1075_1.o(i.CUSTOM_CopyBuffer))
  [Stack]

  - Max Depth = 64
  - Call Chain = CUSTOM_CopyBuffer ⇒ DMA2D_CopyBuffer
  [Calls]
  - >> GetBufferSize
  - >> DMA2D_CopyBuffer
  [Address Reference Count : 1]
  - lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)

  CUSTOM_CopyRect (Thumb, 60 bytes, Stack size 32 bytes, lcdconf_stm32f429i_disco_mb1075_1.o(i.CUSTOM_CopyRect))
  [Stack]

  - Max Depth = 64
  - Call Chain = CUSTOM_CopyRect ⇒ DMA2D_CopyBuffer
  [Calls]
  - >> DMA2D_CopyBuffer
  [Address Reference Count : 1]
  - lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)

  CUSTOM_FillRect (Thumb, 160 bytes, Stack size 32 bytes, lcdconf_stm32f429i_disco_mb1075_1.o(i.CUSTOM_FillRect))
  [Stack]

  - Max Depth = 56
  - Call Chain = CUSTOM_FillRect ⇒ LCD_SetDevFunc
  [Calls]
  - >> LCD_LL_GetPixelformat
  - >> GetBufferSize
  - >> LCD_SetDevFunc
  - >> LCD_FillRect
  - >> GUI_GetDrawMode
  [Address Reference Count : 2]
  - lcdconf_stm32f429i_disco_mb1075_1.o(i.CUSTOM_FillRect)
  - lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)

  Color2IndexBulk_M1555IDMA2D (Thumb, 12 bytes, Stack size 16 bytes, lcdconf_stm32f429i_disco_mb1075_1.o(i.Color2IndexBulk_M1555IDMA2D))
  [Stack]

  - Max Depth = 56
  - Call Chain = Color2IndexBulk_M1555IDMA2D ⇒ DMA2D_Color2IndexBulk ⇒ InvertAlpha_SwapRB
  [Calls]
  - >> DMA2D_Color2IndexBulk
  [Address Reference Count : 1]
  - lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)

  Color2IndexBulk_M4444IDMA2D (Thumb, 12 bytes, Stack size 16 bytes, lcdconf_stm32f429i_disco_mb1075_1.o(i.Color2IndexBulk_M4444IDMA2D))
  [Stack]

  - Max Depth = 56
  - Call Chain = Color2IndexBulk_M4444IDMA2D ⇒ DMA2D_Color2IndexBulk ⇒ InvertAlpha_SwapRB
  [Calls]
  - >> DMA2D_Color2IndexBulk
  [Address Reference Count : 1]
  - lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)

  Color2IndexBulk_M565DMA2D (Thumb, 12 bytes, Stack size 16 bytes, lcdconf_stm32f429i_disco_mb1075_1.o(i.Color2IndexBulk_M565DMA2D))
  [Stack]

  - Max Depth = 56
  - Call Chain = Color2IndexBulk_M565DMA2D ⇒ DMA2D_Color2IndexBulk ⇒ InvertAlpha_SwapRB
  [Calls]
  - >> DMA2D_Color2IndexBulk
  [Address Reference Count : 1]
  - lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)

  Color2IndexBulk_M8888IDMA2D (Thumb, 12 bytes, Stack size 16 bytes, lcdconf_stm32f429i_disco_mb1075_1.o(i.Color2IndexBulk_M8888IDMA2D))
  [Stack]

  - Max Depth = 56
  - Call Chain = Color2IndexBulk_M8888IDMA2D ⇒ DMA2D_Color2IndexBulk ⇒ InvertAlpha_SwapRB
  [Calls]
  - >> DMA2D_Color2IndexBulk
  [Address Reference Count : 1]
  - lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)

  Color2IndexBulk_M888DMA2D (Thumb, 12 bytes, Stack size 16 bytes, lcdconf_stm32f429i_disco_mb1075_1.o(i.Color2IndexBulk_M888DMA2D))
  [Stack]

  - Max Depth = 56
  - Call Chain = Color2IndexBulk_M888DMA2D ⇒ DMA2D_Color2IndexBulk ⇒ InvertAlpha_SwapRB
  [Calls]
  - >> DMA2D_Color2IndexBulk
  [Address Reference Count : 1]
  - lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)

  DMA2D_AlphaBlending (Thumb, 96 bytes, Stack size 16 bytes, lcdconf_stm32f429i_disco_mb1075_1.o(i.DMA2D_AlphaBlending))
  [Stack]

  - Max Depth = 16
  - Call Chain = DMA2D_AlphaBlending
  [Calls]
  - >> InvertAlpha
  [Address Reference Count : 1]
  - lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)

  DMA2D_Color2IndexBulk (Thumb, 30 bytes, Stack size 24 bytes, lcdconf_stm32f429i_disco_mb1075_1.o(i.DMA2D_Color2IndexBulk))
  [Stack]

  - Max Depth = 40
  - Call Chain = DMA2D_Color2IndexBulk ⇒ InvertAlpha_SwapRB
  [Calls]
  - >> InvertAlpha_SwapRB
  - >> DMA2D_ConvertColor
  [Called By]
  - >> Color2IndexBulk_M888DMA2D
  - >> Color2IndexBulk_M8888IDMA2D
  - >> Color2IndexBulk_M565DMA2D
  - >> Color2IndexBulk_M4444IDMA2D
  - >> Color2IndexBulk_M1555IDMA2D

  DMA2D_ConvertColor (Thumb, 50 bytes, Stack size 16 bytes, lcdconf_stm32f429i_disco_mb1075_1.o(i.DMA2D_ConvertColor))
  [Stack]

  - Max Depth = 16
  - Call Chain = DMA2D_ConvertColor
  [Called By]
  - >> DMA2D_Index2ColorBulk
  - >> DMA2D_Color2IndexBulk

  DMA2D_CopyBuffer (Thumb, 68 bytes, Stack size 32 bytes, lcdconf_stm32f429i_disco_mb1075_1.o(i.DMA2D_CopyBuffer))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA2D_CopyBuffer
  [Calls]
  - >> LCD_LL_GetPixelformat
  [Called By]
  - >> CUSTOM_CopyRect
  - >> CUSTOM_CopyBuffer
  - >> BSP_LCD_DrawBitmap16bpp

  DMA2D_Index2ColorBulk (Thumb, 32 bytes, Stack size 16 bytes, lcdconf_stm32f429i_disco_mb1075_1.o(i.DMA2D_Index2ColorBulk))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA2D_Index2ColorBulk ⇒ InvertAlpha_SwapRB
  [Calls]
  - >> InvertAlpha_SwapRB
  - >> DMA2D_ConvertColor
  [Called By]
  - >> Index2ColorBulk_M888DMA2D
  - >> Index2ColorBulk_M8888IDMA2D
  - >> Index2ColorBulk_M565DMA2D
  - >> Index2ColorBulk_M4444IDMA2D
  - >> Index2ColorBulk_M1555IDMA2D

  DMA2D_MixColors (Thumb, 90 bytes, Stack size 16 bytes, lcdconf_stm32f429i_disco_mb1075_1.o(i.DMA2D_MixColors))
  [Stack]

  - Max Depth = 16
  - Call Chain = DMA2D_MixColors
  [Address Reference Count : 1]
  - lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)

  GetBufferSize (Thumb, 22 bytes, Stack size 0 bytes, lcdconf_stm32f429i_disco_mb1075_1.o(i.GetBufferSize))
  [Called By]

  - >> CUSTOM_FillRect
  - >> CUSTOM_CopyBuffer
  - >> BSP_LCD_DrawBitmap8bpp
  - >> BSP_LCD_DrawBitmap16bpp

  Index2ColorBulk_M1555IDMA2D (Thumb, 12 bytes, Stack size 16 bytes, lcdconf_stm32f429i_disco_mb1075_1.o(i.Index2ColorBulk_M1555IDMA2D))
  [Stack]

  - Max Depth = 48
  - Call Chain = Index2ColorBulk_M1555IDMA2D ⇒ DMA2D_Index2ColorBulk ⇒ InvertAlpha_SwapRB
  [Calls]
  - >> DMA2D_Index2ColorBulk
  [Address Reference Count : 1]
  - lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)

  Index2ColorBulk_M4444IDMA2D (Thumb, 12 bytes, Stack size 16 bytes, lcdconf_stm32f429i_disco_mb1075_1.o(i.Index2ColorBulk_M4444IDMA2D))
  [Stack]

  - Max Depth = 48
  - Call Chain = Index2ColorBulk_M4444IDMA2D ⇒ DMA2D_Index2ColorBulk ⇒ InvertAlpha_SwapRB
  [Calls]
  - >> DMA2D_Index2ColorBulk
  [Address Reference Count : 1]
  - lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)

  Index2ColorBulk_M565DMA2D (Thumb, 12 bytes, Stack size 16 bytes, lcdconf_stm32f429i_disco_mb1075_1.o(i.Index2ColorBulk_M565DMA2D))
  [Stack]

  - Max Depth = 48
  - Call Chain = Index2ColorBulk_M565DMA2D ⇒ DMA2D_Index2ColorBulk ⇒ InvertAlpha_SwapRB
  [Calls]
  - >> DMA2D_Index2ColorBulk
  [Address Reference Count : 1]
  - lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)

  Index2ColorBulk_M8888IDMA2D (Thumb, 12 bytes, Stack size 16 bytes, lcdconf_stm32f429i_disco_mb1075_1.o(i.Index2ColorBulk_M8888IDMA2D))
  [Stack]

  - Max Depth = 48
  - Call Chain = Index2ColorBulk_M8888IDMA2D ⇒ DMA2D_Index2ColorBulk ⇒ InvertAlpha_SwapRB
  [Calls]
  - >> DMA2D_Index2ColorBulk
  [Address Reference Count : 1]
  - lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)

  Index2ColorBulk_M888DMA2D (Thumb, 12 bytes, Stack size 16 bytes, lcdconf_stm32f429i_disco_mb1075_1.o(i.Index2ColorBulk_M888DMA2D))
  [Stack]

  - Max Depth = 48
  - Call Chain = Index2ColorBulk_M888DMA2D ⇒ DMA2D_Index2ColorBulk ⇒ InvertAlpha_SwapRB
  [Calls]
  - >> DMA2D_Index2ColorBulk
  [Address Reference Count : 1]
  - lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)

  InvertAlpha (Thumb, 14 bytes, Stack size 0 bytes, lcdconf_stm32f429i_disco_mb1075_1.o(i.InvertAlpha))
  [Calls]

  - >> InvertAlpha
  [Called By]
  - >> LCD_MixColorsBulk
  - >> InvertAlpha
  - >> DMA2D_AlphaBlending

  InvertAlpha_SwapRB (Thumb, 38 bytes, Stack size 16 bytes, lcdconf_stm32f429i_disco_mb1075_1.o(i.InvertAlpha_SwapRB))
  [Stack]

  - Max Depth = 16
  - Call Chain = InvertAlpha_SwapRB
  [Called By]
  - >> _LCD_GetpPalConvTable
  - >> DMA2D_Index2ColorBulk
  - >> DMA2D_Color2IndexBulk

  LCD_LL_GetPixelformat (Thumb, 88 bytes, Stack size 0 bytes, lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_LL_GetPixelformat))
  [Called By]

  - >> LCD_LL_LayerInit
  - >> DMA2D_CopyBuffer
  - >> CUSTOM_FillRect
  - >> BSP_LCD_DrawBitmap8bpp
  - >> LCD_X_Config

  LCD_LL_Init (Thumb, 144 bytes, Stack size 24 bytes, lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_LL_Init))
  [Stack]

  - Max Depth = 168
  - Call Chain = LCD_LL_Init ⇒ ili9341_Init ⇒ LCD_IO_Init ⇒ SPIx_Init ⇒ SPIx_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> ili9341_Init
  - >> HAL_RCCEx_PeriphCLKConfig
  - >> HAL_LTDC_ProgramLineEvent
  - >> HAL_LTDC_Init
  - >> HAL_LTDC_DeInit
  - >> HAL_DMA2D_Init
  [Called By]
  - >> LCD_X_Config

  LCD_LL_LayerInit (Thumb, 170 bytes, Stack size 80 bytes, lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_LL_LayerInit))
  [Stack]

  - Max Depth = 124
  - Call Chain = LCD_LL_LayerInit ⇒ HAL_LTDC_ConfigLayer ⇒ LTDC_SetConfig
  [Calls]
  - >> LCD_LL_GetPixelformat
  - >> LCD_GetBitsPerPixelEx
  - >> HAL_LTDC_EnableCLUT
  - >> HAL_LTDC_ConfigLayer
  - >> HAL_LTDC_ConfigCLUT
  [Called By]
  - >> LCD_X_DisplayDriver

  LCD_MixColorsBulk (Thumb, 174 bytes, Stack size 56 bytes, lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_MixColorsBulk))
  [Stack]

  - Max Depth = 56
  - Call Chain = LCD_MixColorsBulk
  [Calls]
  - >> InvertAlpha
  [Address Reference Count : 1]
  - lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)

  _LCD_GetpPalConvTable (Thumb, 82 bytes, Stack size 16 bytes, lcdconf_stm32f429i_disco_mb1075_1.o(i._LCD_GetpPalConvTable))
  [Stack]

  - Max Depth = 40
  - Call Chain = _LCD_GetpPalConvTable ⇒ LCD_GetpPalConvTable ⇒ LCD_GetpPalConvTableUncached
  [Calls]
  - >> InvertAlpha_SwapRB
  - >> LCD_GetpPalConvTable
  - >> LCD_GetDevFunc
  [Address Reference Count : 1]
  - lcdconf_stm32f429i_disco_mb1075_1.o(i.LCD_X_Config)

  SystemClock_Config (Thumb, 104 bytes, Stack size 88 bytes, maxrefdes82.o(i.SystemClock_Config))
  [Stack]

  - Max Depth = 156
  - Call Chain = SystemClock_Config ⇒ HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_ClockConfig
  [Called By]
  - >> main

  ErrorHandler (Thumb, 14 bytes, Stack size 0 bytes, maintask.o(i.ErrorHandler))
  [Stack]

  - Max Depth = 16 + In Cycle
  - Call Chain = ErrorHandler ⇒ ErrorHandler (Cycle)
  [Calls]
  - >> HAL_Delay
  - >> BSP_LED_Toggle
  - >> ErrorHandler
  [Called By]
  - >> ErrorHandler
  - >> MainTask

  USBD_CDC_DataIn (Thumb, 20 bytes, Stack size 0 bytes, usbd_cdc.o(i.USBD_CDC_DataIn))
  [Address Reference Count : 1]

  - usbd_cdc.o(.data)

  USBD_CDC_DataOut (Thumb, 46 bytes, Stack size 16 bytes, usbd_cdc.o(i.USBD_CDC_DataOut))
  [Stack]

  - Max Depth = 16
  - Call Chain = USBD_CDC_DataOut
  [Calls]
  - >> USBD_LL_GetRxDataSize
  [Address Reference Count : 1]
  - usbd_cdc.o(.data)

  USBD_CDC_DeInit (Thumb, 60 bytes, Stack size 16 bytes, usbd_cdc.o(i.USBD_CDC_DeInit))
  [Stack]

  - Max Depth = 44
  - Call Chain = USBD_CDC_DeInit ⇒ USBD_LL_CloseEP ⇒ HAL_PCD_EP_Close ⇒ USB_DeactivateEndpoint
  [Calls]
  - >> USBD_LL_CloseEP
  - >> free
  [Address Reference Count : 1]
  - usbd_cdc.o(.data)

  USBD_CDC_EP0_RxReady (Thumb, 36 bytes, Stack size 8 bytes, usbd_cdc.o(i.USBD_CDC_EP0_RxReady))
  [Stack]

  - Max Depth = 8
  - Call Chain = USBD_CDC_EP0_RxReady
  [Address Reference Count : 1]
  - usbd_cdc.o(.data)

  USBD_CDC_GetFSCfgDesc (Thumb, 8 bytes, Stack size 0 bytes, usbd_cdc.o(i.USBD_CDC_GetFSCfgDesc))
  [Address Reference Count : 1]

  - usbd_cdc.o(.data)

  USBD_CDC_GetHSCfgDesc (Thumb, 8 bytes, Stack size 0 bytes, usbd_cdc.o(i.USBD_CDC_GetHSCfgDesc))
  [Address Reference Count : 1]

  - usbd_cdc.o(.data)

  USBD_CDC_GetOtherSpeedCfgDesc (Thumb, 8 bytes, Stack size 0 bytes, usbd_cdc.o(i.USBD_CDC_GetOtherSpeedCfgDesc))
  [Address Reference Count : 1]

  - usbd_cdc.o(.data)

  USBD_CDC_Init (Thumb, 136 bytes, Stack size 24 bytes, usbd_cdc.o(i.USBD_CDC_Init))
  [Stack]

  - Max Depth = 72
  - Call Chain = USBD_CDC_Init ⇒ USBD_LL_PrepareReceive ⇒ HAL_PCD_EP_Receive ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_PrepareReceive
  - >> USBD_LL_OpenEP
  - >> malloc
  [Address Reference Count : 1]
  - usbd_cdc.o(.data)

  USBD_CDC_Setup (Thumb, 106 bytes, Stack size 16 bytes, usbd_cdc.o(i.USBD_CDC_Setup))
  [Stack]

  - Max Depth = 80
  - Call Chain = USBD_CDC_Setup ⇒ USBD_CtlSendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_CtlSendData
  - >> USBD_CtlPrepareRx
  [Address Reference Count : 1]
  - usbd_cdc.o(.data)

  MspInit (Thumb, 316 bytes, Stack size 40 bytes, stm32f429i_discovery_sdram.o(i.MspInit))
  [Stack]

  - Max Depth = 80
  - Call Chain = MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_DMA_Init
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  - >> HAL_GPIO_Init
  - >> HAL_DMA_DeInit
  [Called By]
  - >> BSP_SDRAM_Init

  USBD_GetDescriptor (Thumb, 224 bytes, Stack size 24 bytes, usbd_ctlreq.o(i.USBD_GetDescriptor))
  [Stack]

  - Max Depth = 88
  - Call Chain = USBD_GetDescriptor ⇒ USBD_CtlSendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_CtlSendData
  - >> USBD_CtlError
  [Called By]
  - >> USBD_StdDevReq

  USBD_SetConfig (Thumb, 110 bytes, Stack size 16 bytes, usbd_ctlreq.o(i.USBD_SetConfig))
  [Stack]

  - Max Depth = 80
  - Call Chain = USBD_SetConfig ⇒ USBD_CtlSendStatus ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_SetClassConfig
  - >> USBD_CtlSendStatus
  - >> USBD_ClrClassConfig
  - >> USBD_CtlError
  [Called By]
  - >> USBD_StdDevReq

  DMA_CalcBaseAndBitshift (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_hal_dma.o(i.DMA_CalcBaseAndBitshift))
  [Called By]

  - >> HAL_DMA_Init
  - >> HAL_DMA_DeInit

  DMA_SetConfig (Thumb, 40 bytes, Stack size 12 bytes, stm32f4xx_hal_dma.o(i.DMA_SetConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = DMA_SetConfig
  [Called By]
  - >> HAL_DMA_Start_IT

  FLASH_Program_Byte (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_hal_flash.o(i.FLASH_Program_Byte))
  [Called By]

  - >> HAL_FLASH_Program

  FLASH_Program_DoubleWord (Thumb, 34 bytes, Stack size 8 bytes, stm32f4xx_hal_flash.o(i.FLASH_Program_DoubleWord))
  [Stack]

  - Max Depth = 8
  - Call Chain = FLASH_Program_DoubleWord
  [Called By]
  - >> HAL_FLASH_Program

  FLASH_Program_HalfWord (Thumb, 30 bytes, Stack size 0 bytes, stm32f4xx_hal_flash.o(i.FLASH_Program_HalfWord))
  [Called By]

  - >> HAL_FLASH_Program

  FLASH_Program_Word (Thumb, 30 bytes, Stack size 0 bytes, stm32f4xx_hal_flash.o(i.FLASH_Program_Word))
  [Called By]

  - >> HAL_FLASH_Program

  FLASH_SetErrorCode (Thumb, 128 bytes, Stack size 0 bytes, stm32f4xx_hal_flash.o(i.FLASH_SetErrorCode))
  [Called By]

  - >> FLASH_WaitForLastOperation

  FLASH_MassErase (Thumb, 56 bytes, Stack size 0 bytes, stm32f4xx_hal_flash_ex.o(i.FLASH_MassErase))
  [Called By]

  - >> HAL_FLASHEx_Erase

  NVIC_SetPriority (Thumb, 32 bytes, Stack size 0 bytes, stm32f4xx_hal_cortex.o(i.NVIC_SetPriority))
  [Called By]

  - >> HAL_NVIC_SetPriority
  - >> HAL_SYSTICK_Config

  PCD_WriteEmptyTxFifo (Thumb, 150 bytes, Stack size 40 bytes, stm32f4xx_hal_pcd.o(i.PCD_WriteEmptyTxFifo))
  [Stack]

  - Max Depth = 52
  - Call Chain = PCD_WriteEmptyTxFifo ⇒ USB_WritePacket
  [Calls]
  - >> USB_WritePacket
  [Called By]
  - >> HAL_PCD_IRQHandler

  USB_CoreReset (Thumb, 50 bytes, Stack size 0 bytes, stm32f4xx_ll_usb.o(i.USB_CoreReset))
  [Called By]

  - >> USB_CoreInit

  UART_DMAError (Thumb, 30 bytes, Stack size 8 bytes, stm32f4xx_hal_uart.o(i.UART_DMAError))
  [Stack]

  - Max Depth = 8
  - Call Chain = UART_DMAError
  [Calls]
  - >> HAL_UART_ErrorCallback
  [Address Reference Count : 1]
  - stm32f4xx_hal_uart.o(i.HAL_UART_Transmit_DMA)

  UART_DMATransmitCplt (Thumb, 46 bytes, Stack size 8 bytes, stm32f4xx_hal_uart.o(i.UART_DMATransmitCplt))
  [Stack]

  - Max Depth = 72
  - Call Chain = UART_DMATransmitCplt ⇒ HAL_UART_TxCpltCallback ⇒ USBD_CDC_ReceivePacket ⇒ USBD_LL_PrepareReceive ⇒ HAL_PCD_EP_Receive ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> HAL_UART_TxCpltCallback
  [Address Reference Count : 1]
  - stm32f4xx_hal_uart.o(i.HAL_UART_Transmit_DMA)

  UART_DMATxHalfCplt (Thumb, 10 bytes, Stack size 8 bytes, stm32f4xx_hal_uart.o(i.UART_DMATxHalfCplt))
  [Stack]

  - Max Depth = 8
  - Call Chain = UART_DMATxHalfCplt
  [Calls]
  - >> HAL_UART_TxHalfCpltCallback
  [Address Reference Count : 1]
  - stm32f4xx_hal_uart.o(i.HAL_UART_Transmit_DMA)

  UART_Receive_IT (Thumb, 168 bytes, Stack size 8 bytes, stm32f4xx_hal_uart.o(i.UART_Receive_IT))
  [Stack]

  - Max Depth = 8
  - Call Chain = UART_Receive_IT
  [Calls]
  - >> HAL_UART_RxCpltCallback
  [Called By]
  - >> HAL_UART_IRQHandler

  UART_SetConfig (Thumb, 366 bytes, Stack size 24 bytes, stm32f4xx_hal_uart.o(i.UART_SetConfig))
  [Stack]

  - Max Depth = 52
  - Call Chain = UART_SetConfig ⇒ HAL_RCC_GetPCLK2Freq ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_RCC_GetPCLK2Freq
  - >> HAL_RCC_GetPCLK1Freq
  [Called By]
  - >> HAL_UART_Init

  UART_Transmit_IT (Thumb, 102 bytes, Stack size 0 bytes, stm32f4xx_hal_uart.o(i.UART_Transmit_IT))
  [Called By]

  - >> HAL_UART_IRQHandler

  LTDC_SetConfig (Thumb, 354 bytes, Stack size 20 bytes, stm32f4xx_hal_ltdc.o(i.LTDC_SetConfig))
  [Stack]

  - Max Depth = 20
  - Call Chain = LTDC_SetConfig
  [Called By]
  - >> HAL_LTDC_SetWindowPosition
  - >> HAL_LTDC_SetAlpha
  - >> HAL_LTDC_SetAddress
  - >> HAL_LTDC_ConfigLayer

  SPI_WaitOnFlagUntilTimeout (Thumb, 158 bytes, Stack size 32 bytes, stm32f4xx_hal_spi.o(i.SPI_WaitOnFlagUntilTimeout))
  [Stack]

  - Max Depth = 32
  - Call Chain = SPI_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_SPI_TransmitReceive
  - >> HAL_SPI_Transmit

  _Color2IndexBulk_1616I (Thumb, 58 bytes, Stack size 32 bytes, guicc_1616i.o(i._Color2IndexBulk_1616I))
  [Stack]

  - Max Depth = 32
  - Call Chain = _Color2IndexBulk_1616I
  [Address Reference Count : 1]
  - guicc_1616i.o(.constdata)

  _Color2Index_1616I (Thumb, 32 bytes, Stack size 8 bytes, guicc_1616i.o(i._Color2Index_1616I))
  [Stack]

  - Max Depth = 8
  - Call Chain = _Color2Index_1616I
  [Address Reference Count : 1]
  - guicc_1616i.o(.constdata)

  _GetIndexMask_1616I (Thumb, 4 bytes, Stack size 0 bytes, guicc_1616i.o(i._GetIndexMask_1616I))
  [Address Reference Count : 1]

  - guicc_1616i.o(.constdata)

  _Index2ColorBulk_1616I (Thumb, 68 bytes, Stack size 32 bytes, guicc_1616i.o(i._Index2ColorBulk_1616I))
  [Stack]

  - Max Depth = 32
  - Call Chain = _Index2ColorBulk_1616I
  [Address Reference Count : 1]
  - guicc_1616i.o(.constdata)

  _Index2Color_1616I (Thumb, 30 bytes, Stack size 8 bytes, guicc_1616i.o(i._Index2Color_1616I))
  [Stack]

  - Max Depth = 8
  - Call Chain = _Index2Color_1616I
  [Address Reference Count : 1]
  - guicc_1616i.o(.constdata)

  _GetIndexMask_8666 (Thumb, 4 bytes, Stack size 0 bytes, guicc_8666.o(i._GetIndexMask_8666))
  [Address Reference Count : 1]

  - guicc_8666.o(.constdata)

  _Color2IndexBulk_88666I (Thumb, 52 bytes, Stack size 32 bytes, guicc_88666i.o(i._Color2IndexBulk_88666I))
  [Stack]

  - Max Depth = 32
  - Call Chain = _Color2IndexBulk_88666I
  [Address Reference Count : 1]
  - guicc_88666i.o(.constdata)

  _Color2Index_88666I (Thumb, 26 bytes, Stack size 8 bytes, guicc_88666i.o(i._Color2Index_88666I))
  [Stack]

  - Max Depth = 8
  - Call Chain = _Color2Index_88666I
  [Address Reference Count : 1]
  - guicc_88666i.o(.constdata)

  _GetIndexMask_88666I (Thumb, 6 bytes, Stack size 0 bytes, guicc_88666i.o(i._GetIndexMask_88666I))
  [Address Reference Count : 1]

  - guicc_88666i.o(.constdata)

  _Index2ColorBulk_88666I (Thumb, 64 bytes, Stack size 32 bytes, guicc_88666i.o(i._Index2ColorBulk_88666I))
  [Stack]

  - Max Depth = 32
  - Call Chain = _Index2ColorBulk_88666I
  [Address Reference Count : 1]
  - guicc_88666i.o(.constdata)

  _Index2Color_88666I (Thumb, 28 bytes, Stack size 8 bytes, guicc_88666i.o(i._Index2Color_88666I))
  [Stack]

  - Max Depth = 8
  - Call Chain = _Index2Color_88666I
  [Address Reference Count : 1]
  - guicc_88666i.o(.constdata)

  _Color2IndexBulk_M1555I (Thumb, 82 bytes, Stack size 24 bytes, guicc_m1555i.o(i._Color2IndexBulk_M1555I))
  [Stack]

  - Max Depth = 24
  - Call Chain = _Color2IndexBulk_M1555I
  [Address Reference Count : 1]
  - guicc_m1555i.o(.constdata)

  _Color2Index_M1555I (Thumb, 50 bytes, Stack size 8 bytes, guicc_m1555i.o(i._Color2Index_M1555I))
  [Stack]

  - Max Depth = 8
  - Call Chain = _Color2Index_M1555I
  [Address Reference Count : 1]
  - guicc_m1555i.o(.constdata)

  _GetIndexMask_M1555I (Thumb, 6 bytes, Stack size 0 bytes, guicc_m1555i.o(i._GetIndexMask_M1555I))
  [Address Reference Count : 1]

  - guicc_m1555i.o(.constdata)

  _Index2ColorBulk_M1555I (Thumb, 84 bytes, Stack size 16 bytes, guicc_m1555i.o(i._Index2ColorBulk_M1555I))
  [Stack]

  - Max Depth = 16
  - Call Chain = _Index2ColorBulk_M1555I
  [Address Reference Count : 1]
  - guicc_m1555i.o(.constdata)

  _Index2Color_M1555I (Thumb, 44 bytes, Stack size 8 bytes, guicc_m1555i.o(i._Index2Color_M1555I))
  [Stack]

  - Max Depth = 8
  - Call Chain = _Index2Color_M1555I
  [Address Reference Count : 1]
  - guicc_m1555i.o(.constdata)

  _Color2IndexBulk_M4444I (Thumb, 84 bytes, Stack size 16 bytes, guicc_m4444i.o(i._Color2IndexBulk_M4444I))
  [Stack]

  - Max Depth = 16
  - Call Chain = _Color2IndexBulk_M4444I
  [Address Reference Count : 1]
  - guicc_m4444i.o(.constdata)

  _Color2Index_M4444I (Thumb, 58 bytes, Stack size 8 bytes, guicc_m4444i.o(i._Color2Index_M4444I))
  [Stack]

  - Max Depth = 8
  - Call Chain = _Color2Index_M4444I
  [Address Reference Count : 1]
  - guicc_m4444i.o(.constdata)

  _GetIndexMask_M4444I (Thumb, 6 bytes, Stack size 0 bytes, guicc_m4444i.o(i._GetIndexMask_M4444I))
  [Address Reference Count : 1]

  - guicc_m4444i.o(.constdata)

  _Index2ColorBulk_M4444I (Thumb, 84 bytes, Stack size 16 bytes, guicc_m4444i.o(i._Index2ColorBulk_M4444I))
  [Stack]

  - Max Depth = 16
  - Call Chain = _Index2ColorBulk_M4444I
  [Address Reference Count : 1]
  - guicc_m4444i.o(.constdata)

  _Index2Color_M4444I (Thumb, 44 bytes, Stack size 8 bytes, guicc_m4444i.o(i._Index2Color_M4444I))
  [Stack]

  - Max Depth = 8
  - Call Chain = _Index2Color_M4444I
  [Address Reference Count : 1]
  - guicc_m4444i.o(.constdata)

  _Color2IndexBulk_M8888I (Thumb, 64 bytes, Stack size 24 bytes, guicc_m8888i.o(i._Color2IndexBulk_M8888I))
  [Stack]

  - Max Depth = 24
  - Call Chain = _Color2IndexBulk_M8888I
  [Address Reference Count : 1]
  - guicc_m8888i.o(.constdata)

  _Color2Index_M8888I (Thumb, 32 bytes, Stack size 8 bytes, guicc_m8888i.o(i._Color2Index_M8888I))
  [Stack]

  - Max Depth = 8
  - Call Chain = _Color2Index_M8888I
  [Address Reference Count : 1]
  - guicc_m8888i.o(.constdata)

  _GetIndexMask_M8888I (Thumb, 6 bytes, Stack size 0 bytes, guicc_m8888i.o(i._GetIndexMask_M8888I))
  [Address Reference Count : 1]

  - guicc_m8888i.o(.constdata)

  _Index2ColorBulk_M8888I (Thumb, 64 bytes, Stack size 24 bytes, guicc_m8888i.o(i._Index2ColorBulk_M8888I))
  [Stack]

  - Max Depth = 24
  - Call Chain = _Index2ColorBulk_M8888I
  [Address Reference Count : 1]
  - guicc_m8888i.o(.constdata)

  _Index2Color_M8888I (Thumb, 32 bytes, Stack size 8 bytes, guicc_m8888i.o(i._Index2Color_M8888I))
  [Stack]

  - Max Depth = 8
  - Call Chain = _Index2Color_M8888I
  [Address Reference Count : 1]
  - guicc_m8888i.o(.constdata)

  _OnExit (Thumb, 36 bytes, Stack size 8 bytes, gui__alpha.o(i._OnExit))
  [Stack]

  - Max Depth = 8
  - Call Chain = _OnExit
  [Calls]
  - >> GUI_ALLOC_FreeFixedBlock
  [Address Reference Count : 1]
  - gui__alpha.o(i.GUI__GetAlphaBuffer)

  _AddFreeMemory (Thumb, 134 bytes, Stack size 24 bytes, gui_alloc.o(i._AddFreeMemory))
  [Stack]

  - Max Depth = 32
  - Call Chain = _AddFreeMemory ⇒ _RemoveFreeBlock
  [Calls]
  - >> _WriteTagData
  - >> _RemoveFreeBlock
  - >> _GetMinIndex
  [Called By]
  - >> GUI_ALLOC_Free
  - >> _RemoveHoles
  - >> _InitOnce
  - >> _Alloc
  - >> GUI_ALLOC_GetFixedBlock

  _Alloc (Thumb, 184 bytes, Stack size 24 bytes, gui_alloc.o(i._Alloc))
  [Stack]

  - Max Depth = 96 + In Cycle
  - Call Chain = _Alloc ⇒ _InitOnce (Cycle)
  [Calls]
  - >> _WriteTagData
  - >> _RemoveHoles
  - >> _RemoveFreeBlock
  - >> _PushFreeBlock
  - >> _PopFreeBlock
  - >> _InitOnce
  - >> _GetMinIndex
  - >> _AddFreeMemory
  [Called By]
  - >> GUI_ALLOC_AllocNoInit
  - >> _EnlargeBlocks

  _EnlargeBlocks (Thumb, 146 bytes, Stack size 32 bytes, gui_alloc.o(i._EnlargeBlocks))
  [Stack]

  - Max Depth = 128
  - Call Chain = _EnlargeBlocks ⇒ _Alloc ⇒ _InitOnce (Cycle)
  [Calls]
  - >> GUI_ALLOC_Free
  - >> _Alloc
  - >> __aeabi_memcpy4
  [Called By]
  - >> _PopFreeBlock
  - >> _InitOnce

  _GetMinIndex (Thumb, 24 bytes, Stack size 0 bytes, gui_alloc.o(i._GetMinIndex))
  [Called By]

  - >> _RemoveFreeBlock
  - >> _Alloc
  - >> _AddFreeMemory

  _InitOnce (Thumb, 156 bytes, Stack size 16 bytes, gui_alloc.o(i._InitOnce))
  [Stack]

  - Max Depth = 144
  - Call Chain = _InitOnce ⇒ _EnlargeBlocks ⇒ _Alloc ⇒ _InitOnce (Cycle)
  [Calls]
  - >> _TestRAM
  - >> _EnlargeBlocks
  - >> _AddFreeMemory
  - >> GUI__RegisterExit
  [Called By]
  - >> GUI_ALLOC_GetMaxSize
  - >> _Alloc
  - >> GUI_ALLOC_GetFixedBlock

  _OnExit (Thumb, 48 bytes, Stack size 8 bytes, gui_alloc.o(i._OnExit))
  [Stack]

  - Max Depth = 16
  - Call Chain = _OnExit ⇒ GUI__memset
  [Calls]
  - >> GUI__memset
  [Address Reference Count : 1]
  - gui_alloc.o(i._InitOnce)

  _PopFreeBlock (Thumb, 60 bytes, Stack size 8 bytes, gui_alloc.o(i._PopFreeBlock))
  [Stack]

  - Max Depth = 8 + In Cycle
  - Call Chain = _PopFreeBlock ⇒ _EnlargeBlocks (Cycle)
  [Calls]
  - >> _EnlargeBlocks
  [Called By]
  - >> _Alloc

  _PushFreeBlock (Thumb, 34 bytes, Stack size 8 bytes, gui_alloc.o(i._PushFreeBlock))
  [Stack]

  - Max Depth = 8
  - Call Chain = _PushFreeBlock
  [Called By]
  - >> GUI_ALLOC_Free
  - >> _Alloc

  _RemoveFreeBlock (Thumb, 46 bytes, Stack size 8 bytes, gui_alloc.o(i._RemoveFreeBlock))
  [Stack]

  - Max Depth = 8
  - Call Chain = _RemoveFreeBlock
  [Calls]
  - >> _GetMinIndex
  [Called By]
  - >> _RemoveHoles
  - >> _Alloc
  - >> _AddFreeMemory
  - >> GUI_ALLOC_GetFixedBlock

  _RemoveHoles (Thumb, 156 bytes, Stack size 40 bytes, gui_alloc.o(i._RemoveHoles))
  [Stack]

  - Max Depth = 72
  - Call Chain = _RemoveHoles ⇒ _AddFreeMemory ⇒ _RemoveFreeBlock
  [Calls]
  - >> _RemoveFreeBlock
  - >> _AddFreeMemory
  - >> __aeabi_memmove
  [Called By]
  - >> _Alloc
  - >> GUI_ALLOC_GetFixedBlock

  _TestRAM (Thumb, 234 bytes, Stack size 20 bytes, gui_alloc.o(i._TestRAM))
  [Stack]

  - Max Depth = 20
  - Call Chain = _TestRAM
  [Called By]
  - >> _InitOnce

  _WriteTagData (Thumb, 14 bytes, Stack size 0 bytes, gui_alloc.o(i._WriteTagData))
  [Called By]

  - >> _Alloc
  - >> _AddFreeMemory

  _InitContext (Thumb, 98 bytes, Stack size 16 bytes, gui_core.o(i._InitContext))
  [Stack]

  - Max Depth = 16
  - Call Chain = _InitContext
  [Calls]
  - >> WM_GetDesktopWindow
  - >> LCD_SetColor
  - >> LCD_SetBkColor
  [Called By]
  - >> GUI_Init

  _OnExit (Thumb, 34 bytes, Stack size 8 bytes, gui_core.o(i._OnExit))
  [Stack]

  - Max Depth = 16
  - Call Chain = _OnExit ⇒ GUI__memset
  [Calls]
  - >> GUI__memset
  [Address Reference Count : 1]
  - gui_core.o(i.GUI__Config)

  _UnlinkDevice (Thumb, 42 bytes, Stack size 0 bytes, gui_device.o(i._UnlinkDevice))
  [Called By]

  - >> GUI_DEVICE_Unlink

  _SetRotation (Thumb, 28 bytes, Stack size 8 bytes, gui_dispstringinrectex.o(i._SetRotation))
  [Stack]

  - Max Depth = 8
  - Call Chain = _SetRotation
  [Called By]
  - >> GUI_DispStringInRectEx

  _Color2IndexBulk (Thumb, 62 bytes, Stack size 16 bytes, guicc_m565.o(i._Color2IndexBulk))
  [Stack]

  - Max Depth = 16
  - Call Chain = _Color2IndexBulk
  [Address Reference Count : 1]
  - guicc_m565.o(.constdata)

  _Color2Index_M565 (Thumb, 34 bytes, Stack size 8 bytes, guicc_m565.o(i._Color2Index_M565))
  [Stack]

  - Max Depth = 8
  - Call Chain = _Color2Index_M565
  [Address Reference Count : 1]
  - guicc_m565.o(.constdata)

  _GetIndexMask_M565 (Thumb, 6 bytes, Stack size 0 bytes, guicc_m565.o(i._GetIndexMask_M565))
  [Address Reference Count : 1]

  - guicc_m565.o(.constdata)

  _Index2ColorBulk (Thumb, 76 bytes, Stack size 16 bytes, guicc_m565.o(i._Index2ColorBulk))
  [Stack]

  - Max Depth = 16
  - Call Chain = _Index2ColorBulk
  [Address Reference Count : 1]
  - guicc_m565.o(.constdata)

  _Color2IndexBulk (Thumb, 46 bytes, Stack size 16 bytes, guicc_m888.o(i._Color2IndexBulk))
  [Stack]

  - Max Depth = 16
  - Call Chain = _Color2IndexBulk
  [Address Reference Count : 1]
  - guicc_m888.o(.constdata)

  _Color2Index_M888 (Thumb, 20 bytes, Stack size 0 bytes, guicc_m888.o(i._Color2Index_M888))
  [Address Reference Count : 1]

  - guicc_m888.o(.constdata)

  _GetIndexMask_M888 (Thumb, 6 bytes, Stack size 0 bytes, guicc_m888.o(i._GetIndexMask_M888))
  [Address Reference Count : 1]

  - guicc_m888.o(.constdata)

  _Index2ColorBulk (Thumb, 46 bytes, Stack size 16 bytes, guicc_m888.o(i._Index2ColorBulk))
  [Stack]

  - Max Depth = 16
  - Call Chain = _Index2ColorBulk
  [Address Reference Count : 1]
  - guicc_m888.o(.constdata)

  _SetBkColor (Thumb, 28 bytes, Stack size 8 bytes, lcd.o(i._SetBkColor))
  [Stack]

  - Max Depth = 8
  - Call Chain = _SetBkColor
  [Calls]
  - >> LCD_SetBkColorIndex
  - >> LCD_Color2Index
  [Address Reference Count : 1]
  - lcd.o(.constdata)

  _SetColor (Thumb, 28 bytes, Stack size 8 bytes, lcd.o(i._SetColor))
  [Stack]

  - Max Depth = 8
  - Call Chain = _SetColor
  [Calls]
  - >> LCD_SetColorIndex
  - >> LCD_Color2Index
  [Address Reference Count : 1]
  - lcd.o(.constdata)

  _SetDrawMode (Thumb, 40 bytes, Stack size 12 bytes, lcd.o(i._SetDrawMode))
  [Stack]

  - Max Depth = 12
  - Call Chain = _SetDrawMode
  [Address Reference Count : 1]
  - lcd.o(.constdata)

  _OnExit (Thumb, 16 bytes, Stack size 8 bytes, lcd_color.o(i._OnExit))
  [Stack]

  - Max Depth = 8
  - Call Chain = _OnExit
  [Calls]
  - >> GUI_ALLOC_FreeFixedBlock
  [Address Reference Count : 1]
  - lcd_color.o(i.LCD_InitColors)

  _GetDevProp (Thumb, 30 bytes, Stack size 16 bytes, lcd_getex.o(i._GetDevProp))
  [Stack]

  - Max Depth = 16
  - Call Chain = _GetDevProp
  [Calls]
  - >> GUI_DEVICE__GetpDriver
  [Called By]
  - >> LCD_GetSwapXYEx
  - >> LCD_GetBitsPerPixelEx
  - >> LCD_GetYSizeEx
  - >> LCD_GetYSize
  - >> LCD_GetXSizeEx
  - >> LCD_GetXSize
  - >> LCD_GetVYSizeEx
  - >> LCD_GetVXSizeEx
  - >> LCD_GetNumColors
  - >> LCD_GetMirrorYEx
  - >> LCD_GetMirrorXEx
  - >> _GetMaxValue
  - >> LCD_GetNumColorsEx

  _GetMaxValue (Thumb, 30 bytes, Stack size 16 bytes, lcd_getex.o(i._GetMaxValue))
  [Stack]

  - Max Depth = 32
  - Call Chain = _GetMaxValue ⇒ _GetDevProp
  [Calls]
  - >> _GetDevProp
  [Called By]
  - >> LCD_GetVXSizeMax

  _DrawBitLine1BPP (Thumb, 256 bytes, Stack size 56 bytes, lcd_rotatecw.o(i._DrawBitLine1BPP))
  [Stack]

  - Max Depth = 56
  - Call Chain = _DrawBitLine1BPP
  [Called By]
  - >> _DrawBitmap

  _DrawBitmap (Thumb, 290 bytes, Stack size 80 bytes, lcd_rotatecw.o(i._DrawBitmap))
  [Stack]

  - Max Depth = 136
  - Call Chain = _DrawBitmap ⇒ _DrawBitLine1BPP
  [Calls]
  - >> LCD__GetPfSetPixel
  - >> _DrawBitLine1BPP
  [Called By]
  - >> _DrawBitmapCW

  _DrawBitmapCW (Thumb, 456 bytes, Stack size 112 bytes, lcd_rotatecw.o(i._DrawBitmapCW))
  [Stack]

  - Max Depth = 248
  - Call Chain = _DrawBitmapCW ⇒ _DrawBitmap ⇒ _DrawBitLine1BPP
  [Calls]
  - >> LCD_FillRect
  - >> _TransformPoint
  - >> _DrawBitmap
  [Address Reference Count : 1]
  - lcd_rotatecw.o(.data)

  _Rect2TextRect (Thumb, 24 bytes, Stack size 8 bytes, lcd_rotatecw.o(i._Rect2TextRect))
  [Stack]

  - Max Depth = 8
  - Call Chain = _Rect2TextRect
  [Address Reference Count : 1]
  - lcd_rotatecw.o(.data)

  _TransformPoint (Thumb, 110 bytes, Stack size 24 bytes, lcd_rotatecw.o(i._TransformPoint))
  [Stack]

  - Max Depth = 40
  - Call Chain = _TransformPoint ⇒ LCD_GetYSize ⇒ _GetDevProp
  [Calls]
  - >> WM_GetWindowRect
  - >> LCD_GetYSize
  - >> LCD_GetXSize
  [Called By]
  - >> _TransformRect
  - >> _DrawBitmapCW

  _TransformRect (Thumb, 62 bytes, Stack size 24 bytes, lcd_rotatecw.o(i._TransformRect))
  [Stack]

  - Max Depth = 64
  - Call Chain = _TransformRect ⇒ _TransformPoint ⇒ LCD_GetYSize ⇒ _GetDevProp
  [Calls]
  - >> _TransformPoint
  [Address Reference Count : 1]
  - lcd_rotatecw.o(.data)

  _CopyBuffer (Thumb, 80 bytes, Stack size 24 bytes, guidrv_lin_32.o(i._CopyBuffer))
  [Stack]

  - Max Depth = 200
  - Call Chain = _CopyBuffer ⇒ _InitOnce ⇒ GUI_ALLOC_GetFixedBlock ⇒ _InitOnce ⇒ _EnlargeBlocks ⇒ _Alloc ⇒ _InitOnce (Cycle)
  [Calls]
  - >> _InitOnce
  - >> __aeabi_memcpy
  [Address Reference Count : 1]
  - guidrv_lin_32.o(i._GetDevFunc)

  _DrawBitLine1BPP (Thumb, 250 bytes, Stack size 40 bytes, guidrv_lin_32.o(i._DrawBitLine1BPP))
  [Stack]

  - Max Depth = 48
  - Call Chain = _DrawBitLine1BPP ⇒ _SetPixelIndex
  [Calls]
  - >> _SetPixelIndex
  - >> _GetPixelIndex
  [Called By]
  - >> _DrawBitmap

  _DrawBitLine2BPP (Thumb, 142 bytes, Stack size 20 bytes, guidrv_lin_32.o(i._DrawBitLine2BPP))
  [Stack]

  - Max Depth = 20
  - Call Chain = _DrawBitLine2BPP
  [Called By]
  - >> _DrawBitmap

  _DrawBitLine4BPP (Thumb, 150 bytes, Stack size 20 bytes, guidrv_lin_32.o(i._DrawBitLine4BPP))
  [Stack]

  - Max Depth = 20
  - Call Chain = _DrawBitLine4BPP
  [Called By]
  - >> _DrawBitmap

  _DrawBitLine8BPP (Thumb, 236 bytes, Stack size 16 bytes, guidrv_lin_32.o(i._DrawBitLine8BPP))
  [Stack]

  - Max Depth = 16
  - Call Chain = _DrawBitLine8BPP
  [Called By]
  - >> _DrawBitmap

  _DrawBitmap (Thumb, 386 bytes, Stack size 72 bytes, guidrv_lin_32.o(i._DrawBitmap))
  [Stack]

  - Max Depth = 120
  - Call Chain = _DrawBitmap ⇒ _DrawBitLine1BPP ⇒ _SetPixelIndex
  [Calls]
  - >> _DrawBitLine8BPP
  - >> _DrawBitLine4BPP
  - >> _DrawBitLine2BPP
  - >> _DrawBitLine1BPP
  [Address Reference Count : 1]
  - guidrv_lin_32.o(.constdata)

  _DrawHLine (Thumb, 10 bytes, Stack size 8 bytes, guidrv_lin_32.o(i._DrawHLine))
  [Stack]

  - Max Depth = 64
  - Call Chain = _DrawHLine ⇒ _FillRect ⇒ _FillRectOpt32
  [Calls]
  - >> _FillRect
  [Address Reference Count : 1]
  - guidrv_lin_32.o(.constdata)

  _DrawVLine (Thumb, 12 bytes, Stack size 8 bytes, guidrv_lin_32.o(i._DrawVLine))
  [Stack]

  - Max Depth = 64
  - Call Chain = _DrawVLine ⇒ _FillRect ⇒ _FillRectOpt32
  [Calls]
  - >> _FillRect
  [Address Reference Count : 1]
  - guidrv_lin_32.o(.constdata)

  _FillRect (Thumb, 36 bytes, Stack size 24 bytes, guidrv_lin_32.o(i._FillRect))
  [Stack]

  - Max Depth = 56
  - Call Chain = _FillRect ⇒ _FillRectOpt32
  [Calls]
  - >> _FillRectOpt32
  [Called By]
  - >> _DrawVLine
  - >> _DrawHLine
  [Address Reference Count : 1]
  - guidrv_lin_32.o(.constdata)

  _FillRectOpt32 (Thumb, 208 bytes, Stack size 32 bytes, guidrv_lin_32.o(i._FillRectOpt32))
  [Stack]

  - Max Depth = 32
  - Call Chain = _FillRectOpt32
  [Called By]
  - >> _FillRect

  _GetDevData (Thumb, 12 bytes, Stack size 0 bytes, guidrv_lin_32.o(i._GetDevData))
  [Address Reference Count : 1]

  - guidrv_lin_32.o(.constdata)

  _GetDevFunc (Thumb, 150 bytes, Stack size 0 bytes, guidrv_lin_32.o(i._GetDevFunc))
  [Address Reference Count : 1]

  - guidrv_lin_32.o(.constdata)

  _GetDevProp (Thumb, 60 bytes, Stack size 0 bytes, guidrv_lin_32.o(i._GetDevProp))
  [Address Reference Count : 1]

  - guidrv_lin_32.o(.constdata)

  _GetPixelIndex (Thumb, 16 bytes, Stack size 0 bytes, guidrv_lin_32.o(i._GetPixelIndex))
  [Called By]

  - >> _XorPixel
  - >> _DrawBitLine1BPP
  [Address Reference Count : 1]
  - guidrv_lin_32.o(.constdata)

  _GetPos (Thumb, 28 bytes, Stack size 16 bytes, guidrv_lin_32.o(i._GetPos))
  [Stack]

  - Max Depth = 192
  - Call Chain = _GetPos ⇒ _InitOnce ⇒ GUI_ALLOC_GetFixedBlock ⇒ _InitOnce ⇒ _EnlargeBlocks ⇒ _Alloc ⇒ _InitOnce (Cycle)
  [Calls]
  - >> _InitOnce
  [Address Reference Count : 1]
  - guidrv_lin_32.o(i._GetDevFunc)

  _GetRect (Thumb, 22 bytes, Stack size 0 bytes, guidrv_lin_32.o(i._GetRect))
  [Address Reference Count : 1]

  - guidrv_lin_32.o(.constdata)

  _Init (Thumb, 24 bytes, Stack size 16 bytes, guidrv_lin_32.o(i._Init))
  [Stack]

  - Max Depth = 192
  - Call Chain = _Init ⇒ _InitOnce ⇒ GUI_ALLOC_GetFixedBlock ⇒ _InitOnce ⇒ _EnlargeBlocks ⇒ _Alloc ⇒ _InitOnce (Cycle)
  [Calls]
  - >> LCD_X_DisplayDriver
  - >> _InitOnce
  [Address Reference Count : 1]
  - guidrv_lin_32.o(i._GetDevFunc)

  _InitOnce (Thumb, 36 bytes, Stack size 8 bytes, guidrv_lin_32.o(i._InitOnce))
  [Stack]

  - Max Depth = 176
  - Call Chain = _InitOnce ⇒ GUI_ALLOC_GetFixedBlock ⇒ _InitOnce ⇒ _EnlargeBlocks ⇒ _Alloc ⇒ _InitOnce (Cycle)
  [Calls]
  - >> GUI__memset
  - >> GUI_ALLOC_GetFixedBlock
  [Called By]
  - >> _ShowBuffer
  - >> _SetVis
  - >> _SetVSize
  - >> _SetVRAMAddr
  - >> _SetSize
  - >> _SetPos
  - >> _SetDevFunc
  - >> _SetAlpha
  - >> _Init
  - >> _GetPos
  - >> _CopyBuffer

  _Off (Thumb, 10 bytes, Stack size 0 bytes, guidrv_lin_32.o(i._Off))
  [Stack]

  - Max Depth = 156
  - Call Chain = _Off ⇒ LCD_X_DisplayDriver ⇒ LCD_LL_LayerInit ⇒ HAL_LTDC_ConfigLayer ⇒ LTDC_SetConfig
  [Calls]
  - >> LCD_X_DisplayDriver
  [Address Reference Count : 1]
  - guidrv_lin_32.o(i._GetDevFunc)

  _On (Thumb, 10 bytes, Stack size 0 bytes, guidrv_lin_32.o(i._On))
  [Stack]

  - Max Depth = 156
  - Call Chain = _On ⇒ LCD_X_DisplayDriver ⇒ LCD_LL_LayerInit ⇒ HAL_LTDC_ConfigLayer ⇒ LTDC_SetConfig
  [Calls]
  - >> LCD_X_DisplayDriver
  [Address Reference Count : 1]
  - guidrv_lin_32.o(i._GetDevFunc)

  _ReadRect (Thumb, 48 bytes, Stack size 20 bytes, guidrv_lin_32.o(i._ReadRect))
  [Stack]

  - Max Depth = 20
  - Call Chain = _ReadRect
  [Address Reference Count : 1]
  - guidrv_lin_32.o(i._GetDevFunc)

  _SetAlpha (Thumb, 38 bytes, Stack size 16 bytes, guidrv_lin_32.o(i._SetAlpha))
  [Stack]

  - Max Depth = 192
  - Call Chain = _SetAlpha ⇒ _InitOnce ⇒ GUI_ALLOC_GetFixedBlock ⇒ _InitOnce ⇒ _EnlargeBlocks ⇒ _Alloc ⇒ _InitOnce (Cycle)
  [Calls]
  - >> LCD_X_DisplayDriver
  - >> _InitOnce
  [Address Reference Count : 1]
  - guidrv_lin_32.o(i._GetDevFunc)

  _SetAlphaMode (Thumb, 16 bytes, Stack size 8 bytes, guidrv_lin_32.o(i._SetAlphaMode))
  [Stack]

  - Max Depth = 164
  - Call Chain = _SetAlphaMode ⇒ LCD_X_DisplayDriver ⇒ LCD_LL_LayerInit ⇒ HAL_LTDC_ConfigLayer ⇒ LTDC_SetConfig
  [Calls]
  - >> LCD_X_DisplayDriver
  [Address Reference Count : 1]
  - guidrv_lin_32.o(i._GetDevFunc)

  _SetChroma (Thumb, 18 bytes, Stack size 16 bytes, guidrv_lin_32.o(i._SetChroma))
  [Stack]

  - Max Depth = 172
  - Call Chain = _SetChroma ⇒ LCD_X_DisplayDriver ⇒ LCD_LL_LayerInit ⇒ HAL_LTDC_ConfigLayer ⇒ LTDC_SetConfig
  [Calls]
  - >> LCD_X_DisplayDriver
  [Address Reference Count : 1]
  - guidrv_lin_32.o(i._GetDevFunc)

  _SetChromaMode (Thumb, 16 bytes, Stack size 8 bytes, guidrv_lin_32.o(i._SetChromaMode))
  [Stack]

  - Max Depth = 164
  - Call Chain = _SetChromaMode ⇒ LCD_X_DisplayDriver ⇒ LCD_LL_LayerInit ⇒ HAL_LTDC_ConfigLayer ⇒ LTDC_SetConfig
  [Calls]
  - >> LCD_X_DisplayDriver
  [Address Reference Count : 1]
  - guidrv_lin_32.o(i._GetDevFunc)

  _SetDevFunc (Thumb, 68 bytes, Stack size 16 bytes, guidrv_lin_32.o(i._SetDevFunc))
  [Stack]

  - Max Depth = 192
  - Call Chain = _SetDevFunc ⇒ _InitOnce ⇒ GUI_ALLOC_GetFixedBlock ⇒ _InitOnce ⇒ _EnlargeBlocks ⇒ _Alloc ⇒ _InitOnce (Cycle)
  [Calls]
  - >> _InitOnce
  [Address Reference Count : 1]
  - guidrv_lin_32.o(i._GetDevFunc)

  _SetOrg (Thumb, 164 bytes, Stack size 32 bytes, guidrv_lin_32.o(i._SetOrg))
  [Stack]

  - Max Depth = 188
  - Call Chain = _SetOrg ⇒ LCD_X_DisplayDriver ⇒ LCD_LL_LayerInit ⇒ HAL_LTDC_ConfigLayer ⇒ LTDC_SetConfig
  [Calls]
  - >> LCD_GetSwapXYEx
  - >> LCD_X_DisplayDriver
  - >> LCD_GetMirrorYEx
  - >> LCD_GetMirrorXEx
  [Address Reference Count : 1]
  - guidrv_lin_32.o(.constdata)

  _SetPixelIndex (Thumb, 18 bytes, Stack size 8 bytes, guidrv_lin_32.o(i._SetPixelIndex))
  [Stack]

  - Max Depth = 8
  - Call Chain = _SetPixelIndex
  [Called By]
  - >> _XorPixel
  - >> _DrawBitLine1BPP
  [Address Reference Count : 1]
  - guidrv_lin_32.o(.constdata)

  _SetPos (Thumb, 46 bytes, Stack size 24 bytes, guidrv_lin_32.o(i._SetPos))
  [Stack]

  - Max Depth = 200
  - Call Chain = _SetPos ⇒ _InitOnce ⇒ GUI_ALLOC_GetFixedBlock ⇒ _InitOnce ⇒ _EnlargeBlocks ⇒ _Alloc ⇒ _InitOnce (Cycle)
  [Calls]
  - >> LCD_X_DisplayDriver
  - >> _InitOnce
  [Address Reference Count : 1]
  - guidrv_lin_32.o(i._GetDevFunc)

  _SetSize (Thumb, 68 bytes, Stack size 32 bytes, guidrv_lin_32.o(i._SetSize))
  [Stack]

  - Max Depth = 208
  - Call Chain = _SetSize ⇒ _InitOnce ⇒ GUI_ALLOC_GetFixedBlock ⇒ _InitOnce ⇒ _EnlargeBlocks ⇒ _Alloc ⇒ _InitOnce (Cycle)
  [Calls]
  - >> LCD_GetSwapXYEx
  - >> LCD_X_DisplayDriver
  - >> _InitOnce
  [Address Reference Count : 1]
  - guidrv_lin_32.o(i._GetDevFunc)

  _SetVRAMAddr (Thumb, 40 bytes, Stack size 16 bytes, guidrv_lin_32.o(i._SetVRAMAddr))
  [Stack]

  - Max Depth = 192
  - Call Chain = _SetVRAMAddr ⇒ _InitOnce ⇒ GUI_ALLOC_GetFixedBlock ⇒ _InitOnce ⇒ _EnlargeBlocks ⇒ _Alloc ⇒ _InitOnce (Cycle)
  [Calls]
  - >> LCD_X_DisplayDriver
  - >> _InitOnce
  [Address Reference Count : 1]
  - guidrv_lin_32.o(i._GetDevFunc)

  _SetVSize (Thumb, 42 bytes, Stack size 24 bytes, guidrv_lin_32.o(i._SetVSize))
  [Stack]

  - Max Depth = 200
  - Call Chain = _SetVSize ⇒ _InitOnce ⇒ GUI_ALLOC_GetFixedBlock ⇒ _InitOnce ⇒ _EnlargeBlocks ⇒ _Alloc ⇒ _InitOnce (Cycle)
  [Calls]
  - >> LCD_GetSwapXYEx
  - >> _InitOnce
  [Address Reference Count : 1]
  - guidrv_lin_32.o(i._GetDevFunc)

  _SetVis (Thumb, 38 bytes, Stack size 16 bytes, guidrv_lin_32.o(i._SetVis))
  [Stack]

  - Max Depth = 192
  - Call Chain = _SetVis ⇒ _InitOnce ⇒ GUI_ALLOC_GetFixedBlock ⇒ _InitOnce ⇒ _EnlargeBlocks ⇒ _Alloc ⇒ _InitOnce (Cycle)
  [Calls]
  - >> LCD_X_DisplayDriver
  - >> _InitOnce
  [Address Reference Count : 1]
  - guidrv_lin_32.o(i._GetDevFunc)

  _ShowBuffer (Thumb, 36 bytes, Stack size 16 bytes, guidrv_lin_32.o(i._ShowBuffer))
  [Stack]

  - Max Depth = 192
  - Call Chain = _ShowBuffer ⇒ _InitOnce ⇒ GUI_ALLOC_GetFixedBlock ⇒ _InitOnce ⇒ _EnlargeBlocks ⇒ _Alloc ⇒ _InitOnce (Cycle)
  [Calls]
  - >> LCD_X_DisplayDriver
  - >> _InitOnce
  [Address Reference Count : 1]
  - guidrv_lin_32.o(i._GetDevFunc)

  _XorPixel (Thumb, 40 bytes, Stack size 24 bytes, guidrv_lin_32.o(i._XorPixel))
  [Stack]

  - Max Depth = 32
  - Call Chain = _XorPixel ⇒ _SetPixelIndex
  [Calls]
  - >> _SetPixelIndex
  - >> _GetPixelIndex
  [Address Reference Count : 1]
  - guidrv_lin_32.o(.constdata)

  _Color2Index_16 (Thumb, 114 bytes, Stack size 20 bytes, guicc_16.o(i._Color2Index_16))
  [Stack]

  - Max Depth = 20
  - Call Chain = _Color2Index_16
  [Address Reference Count : 1]
  - guicc_16.o(.constdata)

  _GetIndexMask_16 (Thumb, 4 bytes, Stack size 0 bytes, guicc_16.o(i._GetIndexMask_16))
  [Address Reference Count : 1]

  - guicc_16.o(.constdata)

  _Index2Color_16 (Thumb, 54 bytes, Stack size 16 bytes, guicc_16.o(i._Index2Color_16))
  [Stack]

  - Max Depth = 16
  - Call Chain = _Index2Color_16
  [Address Reference Count : 1]
  - guicc_16.o(.constdata)

  _GotoX (Thumb, 10 bytes, Stack size 0 bytes, gui_goto.o(i._GotoX))
  [Called By]

  - >> GUI_GotoXY

  _GotoY (Thumb, 10 bytes, Stack size 0 bytes, gui_goto.o(i._GotoY))
  [Called By]

  - >> GUI_GotoXY

  _CalcSizeOfChar (Thumb, 4 bytes, Stack size 0 bytes, gui_uc_encodenone.o(i._CalcSizeOfChar))
  [Address Reference Count : 1]

  - gui_uc_encodenone.o(.constdata)

  _Encode (Thumb, 6 bytes, Stack size 0 bytes, gui_uc_encodenone.o(i._Encode))
  [Address Reference Count : 1]

  - gui_uc_encodenone.o(.constdata)

  _GetCharCode (Thumb, 4 bytes, Stack size 0 bytes, gui_uc_encodenone.o(i._GetCharCode))
  [Address Reference Count : 1]

  - gui_uc_encodenone.o(.constdata)

  _GetCharSize (Thumb, 4 bytes, Stack size 0 bytes, gui_uc_encodenone.o(i._GetCharSize))
  [Address Reference Count : 1]

  - gui_uc_encodenone.o(.constdata)

  _Color2Index_0 (Thumb, 84 bytes, Stack size 32 bytes, guicc_0.o(i._Color2Index_0))
  [Stack]

  - Max Depth = 48
  - Call Chain = _Color2Index_0 ⇒ LCD_GetNumColors ⇒ _GetDevProp
  [Calls]
  - >> GUI_CalcColorDist
  - >> LCD_GetPalette
  - >> LCD_GetNumColors
  [Address Reference Count : 1]
  - guicc_0.o(.constdata)

  _GetIndexMask_0 (Thumb, 82 bytes, Stack size 8 bytes, guicc_0.o(i._GetIndexMask_0))
  [Stack]

  - Max Depth = 24
  - Call Chain = _GetIndexMask_0 ⇒ LCD_GetNumColors ⇒ _GetDevProp
  [Calls]
  - >> LCD_GetNumColors
  [Address Reference Count : 1]
  - guicc_0.o(.constdata)

  _Index2Color_0 (Thumb, 32 bytes, Stack size 16 bytes, guicc_0.o(i._Index2Color_0))
  [Stack]

  - Max Depth = 32
  - Call Chain = _Index2Color_0 ⇒ LCD_GetNumColors ⇒ _GetDevProp
  [Calls]
  - >> LCD_GetPalette
  - >> LCD_GetNumColors
  [Address Reference Count : 1]
  - guicc_0.o(.constdata)

  LCD_ReadRectEx (Thumb, 404 bytes, Stack size 64 bytes, lcd_readrect.o(i.LCD_ReadRectEx))
  [Stack]

  - Max Depth = 64
  - Call Chain = LCD_ReadRectEx
  [Calls]
  - >> GUI_GetBitsPerPixelEx
  [Called By]
  - >> GUI_ReadRectEx

  _DrawBitLine1BPP (Thumb, 276 bytes, Stack size 56 bytes, guidev_32.o(i._DrawBitLine1BPP))
  [Stack]

  - Max Depth = 56
  - Call Chain = _DrawBitLine1BPP
  [Called By]
  - >> _DrawBitmap

  _DrawBitLine2BPP (Thumb, 218 bytes, Stack size 56 bytes, guidev_32.o(i._DrawBitLine2BPP))
  [Stack]

  - Max Depth = 56
  - Call Chain = _DrawBitLine2BPP
  [Called By]
  - >> _DrawBitmap

  _DrawBitLine32BPP_DDB (Thumb, 148 bytes, Stack size 32 bytes, guidev_32.o(i._DrawBitLine32BPP_DDB))
  [Stack]

  - Max Depth = 48
  - Call Chain = _DrawBitLine32BPP_DDB ⇒ GUI__MixColors
  [Calls]
  - >> GUI__MixColors
  - >> __aeabi_memcpy4
  [Called By]
  - >> _DrawBitmap

  _DrawBitLine4BPP (Thumb, 340 bytes, Stack size 40 bytes, guidev_32.o(i._DrawBitLine4BPP))
  [Stack]

  - Max Depth = 40
  - Call Chain = _DrawBitLine4BPP
  [Called By]
  - >> _DrawBitmap

  _DrawBitmap (Thumb, 666 bytes, Stack size 104 bytes, guidev_32.o(i._DrawBitmap))
  [Stack]

  - Max Depth = 160
  - Call Chain = _DrawBitmap ⇒ _DrawBitLine2BPP
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> GUI_USAGE_AddRect
  - >> _XY2PTR
  - >> _DrawBitLine4BPP
  - >> _DrawBitLine32BPP_DDB
  - >> _DrawBitLine2BPP
  - >> _DrawBitLine1BPP
  - >> __aeabi_memcpy
  [Address Reference Count : 1]
  - guidev_32.o(.constdata)

  _DrawHLine (Thumb, 10 bytes, Stack size 8 bytes, guidev_32.o(i._DrawHLine))
  [Stack]

  - Max Depth = 80
  - Call Chain = _DrawHLine ⇒ _FillRect ⇒ GUI_USAGE_AddRect
  [Calls]
  - >> _FillRect
  [Address Reference Count : 1]
  - guidev_32.o(.constdata)

  _DrawVLine (Thumb, 166 bytes, Stack size 40 bytes, guidev_32.o(i._DrawVLine))
  [Stack]

  - Max Depth = 56
  - Call Chain = _DrawVLine ⇒ _XY2PTR
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> _XY2PTR
  [Address Reference Count : 1]
  - guidev_32.o(.constdata)

  _FillRect (Thumb, 160 bytes, Stack size 48 bytes, guidev_32.o(i._FillRect))
  [Stack]

  - Max Depth = 72
  - Call Chain = _FillRect ⇒ GUI_USAGE_AddRect
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> GUI_USAGE_AddRect
  - >> _XY2PTR
  [Called By]
  - >> _DrawHLine
  [Address Reference Count : 1]
  - guidev_32.o(.constdata)

  _GetDevData (Thumb, 12 bytes, Stack size 0 bytes, guidev_32.o(i._GetDevData))
  [Address Reference Count : 1]

  - guidev_32.o(.constdata)

  _GetDevFunc (Thumb, 12 bytes, Stack size 0 bytes, guidev_32.o(i._GetDevFunc))
  [Address Reference Count : 1]

  - guidev_32.o(.constdata)

  _GetDevProp (Thumb, 12 bytes, Stack size 0 bytes, guidev_32.o(i._GetDevProp))
  [Address Reference Count : 1]

  - guidev_32.o(.constdata)

  _GetPixelIndex (Thumb, 14 bytes, Stack size 8 bytes, guidev_32.o(i._GetPixelIndex))
  [Stack]

  - Max Depth = 24
  - Call Chain = _GetPixelIndex ⇒ _XY2PTR
  [Calls]
  - >> _XY2PTR
  [Address Reference Count : 1]
  - guidev_32.o(.constdata)

  _GetRect (Thumb, 48 bytes, Stack size 16 bytes, guidev_32.o(i._GetRect))
  [Stack]

  - Max Depth = 16
  - Call Chain = _GetRect
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  [Address Reference Count : 1]
  - guidev_32.o(.constdata)

  _SetOrg (Thumb, 8 bytes, Stack size 0 bytes, guidev_32.o(i._SetOrg))
  [Address Reference Count : 1]

  - guidev_32.o(.constdata)

  _SetPixelIndex (Thumb, 66 bytes, Stack size 24 bytes, guidev_32.o(i._SetPixelIndex))
  [Stack]

  - Max Depth = 40
  - Call Chain = _SetPixelIndex ⇒ _XY2PTR
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> _XY2PTR
  [Address Reference Count : 1]
  - guidev_32.o(.constdata)

  _XY2PTR (Thumb, 56 bytes, Stack size 16 bytes, guidev_32.o(i._XY2PTR))
  [Stack]

  - Max Depth = 16
  - Call Chain = _XY2PTR
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  [Called By]
  - >> _XorPixel
  - >> _SetPixelIndex
  - >> _GetPixelIndex
  - >> _FillRect
  - >> _DrawVLine
  - >> _DrawBitmap

  _XorPixel (Thumb, 82 bytes, Stack size 32 bytes, guidev_32.o(i._XorPixel))
  [Stack]

  - Max Depth = 48
  - Call Chain = _XorPixel ⇒ _XY2PTR
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> _XY2PTR
  [Address Reference Count : 1]
  - guidev_32.o(.constdata)

  WM__PaintWinAndOverlays (Thumb, 116 bytes, Stack size 16 bytes, wm.o(i.WM__PaintWinAndOverlays))
  [Stack]

  - Max Depth = 96
  - Call Chain = WM__PaintWinAndOverlays ⇒ _PaintTransChildren ⇒ _PaintTransChildren (Cycle)
  [Calls]
  - >> GUI_ALLOC_h2p
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> _PaintTransChildren
  - >> _Paint1Trans
  - >> _Paint1
  [Called By]
  - >> _cbPaintMemDev
  - >> WM__Paint

  _DeleteAllChildren (Thumb, 18 bytes, Stack size 8 bytes, wm.o(i._DeleteAllChildren))
  [Stack]

  - Max Depth = 8 + In Cycle
  - Call Chain = _DeleteAllChildren ⇒ WM_DeleteWindow (Cycle)
  [Calls]
  - >> WM_DeleteWindow
  [Called By]
  - >> WM_DeleteWindow

  _DesktopHandle2Index (Thumb, 28 bytes, Stack size 0 bytes, wm.o(i._DesktopHandle2Index))
  [Called By]

  - >> WM__ClipAtParentBorders
  - >> cbBackWin
  - >> WM__GetTopLevelLayer

  _DrawNext (Thumb, 82 bytes, Stack size 136 bytes, wm.o(i._DrawNext))
  [Stack]

  - Max Depth = 624
  - Call Chain = _DrawNext ⇒ WM__Paint ⇒ GUI_MEMDEV_Draw ⇒ GUI_MEMDEV_CopyToLCD ⇒ GUI_MEMDEV_CopyToLCDAt ⇒ GUI_MEMDEV__WriteToActiveOpaque ⇒ _WriteToActiveOpaque_8 ⇒ LCD__DrawBitmap_1bpp ⇒ LCD_FillRect
  [Calls]
  - >> GUI_SetColor
  - >> GUI_ALLOC_h2p
  - >> GUI_SetBkColor
  - >> GUI_SaveContext_W
  - >> GUI_RestoreContext
  - >> WM__Paint
  [Called By]
  - >> WM_Exec

  _Exec1Input (Thumb, 100 bytes, Stack size 24 bytes, wm.o(i._Exec1Input))
  [Stack]

  - Max Depth = 256
  - Call Chain = _Exec1Input ⇒ WM_DeleteWindow ⇒ WM__SendMsgNoData ⇒ WM__SendMessage ⇒ WM_DefaultProc ⇒ WM_InvalidateWindow ⇒ WM_InvalidateRect ⇒ WM__InvalidateRectEx ⇒ WM__InvalidateRect ⇒ WM__InvalidateRect (Cycle)
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> WM_DeleteWindow
  - >> GUI_PollKeyMsg
  [Called By]
  - >> WM_Exec

  _FindNext_IVR (Thumb, 318 bytes, Stack size 32 bytes, wm.o(i._FindNext_IVR))
  [Stack]

  - Max Depth = 80
  - Call Chain = _FindNext_IVR ⇒ _Findy1 ⇒ _Findy1 (Cycle)
  [Calls]
  - >> GUI_ALLOC_h2p
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> _Findy1
  - >> _Findx1
  - >> _Findx0
  [Called By]
  - >> WM__GetNextIVR

  _Findx0 (Thumb, 124 bytes, Stack size 32 bytes, wm.o(i._Findx0))
  [Stack]

  - Max Depth = 48 + In Cycle
  - Call Chain = _Findx0 ⇒ _Findx0 (Cycle)
  [Calls]
  - >> GUI__IntersectRects
  - >> GUI_ALLOC_h2p
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> _Findx0
  - >> GUI_RectsIntersect
  [Called By]
  - >> _Findx0
  - >> _FindNext_IVR

  _Findx1 (Thumb, 114 bytes, Stack size 32 bytes, wm.o(i._Findx1))
  [Stack]

  - Max Depth = 48 + In Cycle
  - Call Chain = _Findx1 ⇒ _Findx1 (Cycle)
  [Calls]
  - >> GUI__IntersectRects
  - >> GUI_ALLOC_h2p
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> _Findx1
  - >> GUI_RectsIntersect
  [Called By]
  - >> _Findx1
  - >> _FindNext_IVR

  _Findy1 (Thumb, 166 bytes, Stack size 32 bytes, wm.o(i._Findy1))
  [Stack]

  - Max Depth = 48 + In Cycle
  - Call Chain = _Findy1 ⇒ _Findy1 (Cycle)
  [Calls]
  - >> GUI__IntersectRects
  - >> GUI_ALLOC_h2p
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> _Findy1
  - >> GUI_RectsIntersect
  [Called By]
  - >> _Findy1
  - >> _FindNext_IVR

  _Invalidate1Abs (Thumb, 122 bytes, Stack size 32 bytes, wm.o(i._Invalidate1Abs))
  [Stack]

  - Max Depth = 48
  - Call Chain = _Invalidate1Abs ⇒ GUI__IntersectRects
  [Calls]
  - >> GUI__IntersectRects
  - >> GUI_ALLOC_h2p
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> GUI_SignalEvent
  - >> GUI_MergeRect
  - >> WM__RectIsNZ
  [Called By]
  - >> WM_InvalidateWindowAndDescsEx
  - >> WM__InvalidateRect
  - >> WM__Invalidate1Abs

  _OnExit (Thumb, 48 bytes, Stack size 8 bytes, wm.o(i._OnExit))
  [Stack]

  - Max Depth = 8
  - Call Chain = _OnExit
  [Address Reference Count : 1]
  - wm.o(i.WM_Init)

  _Paint1 (Thumb, 28 bytes, Stack size 8 bytes, wm.o(i._Paint1))
  [Stack]

  - Max Depth = 8
  - Call Chain = _Paint1
  [Calls]
  - >> GUI_ALLOC_h2p
  [Called By]
  - >> _Paint1Trans
  - >> WM__PaintWinAndOverlays

  _Paint1Trans (Thumb, 130 bytes, Stack size 32 bytes, wm.o(i._Paint1Trans))
  [Stack]

  - Max Depth = 48
  - Call Chain = _Paint1Trans ⇒ GUI__IntersectRects
  [Calls]
  - >> GUI__IntersectRects
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> _Paint1
  - >> GUI_RectsIntersect
  [Called By]
  - >> _PaintTransChildren
  - >> WM__PaintWinAndOverlays

  _PaintTransChildren (Thumb, 154 bytes, Stack size 32 bytes, wm.o(i._PaintTransChildren))
  [Stack]

  - Max Depth = 80 + In Cycle
  - Call Chain = _PaintTransChildren ⇒ _PaintTransChildren (Cycle)
  [Calls]
  - >> GUI_ALLOC_h2p
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> _PaintTransChildren
  - >> _Paint1Trans
  - >> GUI_RectsIntersect
  [Called By]
  - >> _PaintTransChildren
  - >> WM__PaintWinAndOverlays

  _SetClipRectUserIntersect (Thumb, 68 bytes, Stack size 24 bytes, wm.o(i._SetClipRectUserIntersect))
  [Stack]

  - Max Depth = 64
  - Call Chain = _SetClipRectUserIntersect ⇒ LCD_SetClipRectEx ⇒ GUI__IntersectRects
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> WM__Client2Screen
  - >> LCD_SetClipRectEx
  - >> GUI__IntersectRect
  [Called By]
  - >> WM__ActivateClipRect

  _cbPaintMemDev (Thumb, 64 bytes, Stack size 24 bytes, wm.o(i._cbPaintMemDev))
  [Stack]

  - Max Depth = 120
  - Call Chain = _cbPaintMemDev ⇒ WM__PaintWinAndOverlays ⇒ _PaintTransChildren ⇒ _PaintTransChildren (Cycle)
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> WM__PaintWinAndOverlays
  [Address Reference Count : 1]
  - wm.o(i.WM__Paint)

  cbBackWin (Thumb, 74 bytes, Stack size 8 bytes, wm.o(i.cbBackWin))
  [Stack]

  - Max Depth = 176
  - Call Chain = cbBackWin ⇒ WM_DefaultProc ⇒ WM_InvalidateWindow ⇒ WM_InvalidateRect ⇒ WM__InvalidateRectEx ⇒ WM__InvalidateRect ⇒ WM__InvalidateRect (Cycle)
  [Calls]
  - >> GUI_Clear
  - >> WM_DefaultProc
  - >> _DesktopHandle2Index
  - >> GUI_SetBkColor
  - >> GUI_StoreKey
  [Address Reference Count : 1]
  - wm.o(i.WM_Init)

  _DispLine (Thumb, 104 bytes, Stack size 32 bytes, gui_charline.o(i._DispLine))
  [Stack]

  - Max Depth = 64
  - Call Chain = _DispLine ⇒ GUI__ManageCache ⇒ GUI__ManageCacheEx
  [Calls]
  - >> GUI_UC__GetCharCodeInc
  - >> GUI__ManageCache
  - >> GUI_RectsIntersect
  [Called By]
  - >> GUI__DispLine

  _Log2VisBuffered (Thumb, 2 bytes, Stack size 0 bytes, gui_charline.o(i._Log2VisBuffered))
  [Address Reference Count : 1]

  - gui_charline.o(.data)

  _IncPointer (Thumb, 24 bytes, Stack size 0 bytes, gui_onkey.o(i._IncPointer))
  [Called By]

  - >> _IncReadPointer

  _IncReadPointer (Thumb, 6 bytes, Stack size 0 bytes, gui_onkey.o(i._IncReadPointer))
  [Calls]

  - >> _IncPointer
  [Called By]
  - >> GUI_PollKeyMsg

  _Min (Thumb, 8 bytes, Stack size 0 bytes, guidev_banding.o(i._Min))
  [Called By]

  - >> GUI_MEMDEV_Draw

  _CreateStaticDevice (Thumb, 308 bytes, Stack size 56 bytes, guidev_staticdevices.o(i._CreateStaticDevice))
  [Stack]

  - Max Depth = 512
  - Call Chain = _CreateStaticDevice ⇒ WM_SetSize ⇒ WM_ResizeWindow ⇒ WM__UpdateChildPositions ⇒ WM_ResizeWindow (Cycle)
  [Calls]
  - >> WM_GetDesktopWindow
  - >> GUI__memset
  - >> GUI_ALLOC_h2p
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> LCD_GetYSize
  - >> LCD_GetXSize
  - >> WM_SetSize
  - >> WM_GetWindowOrgX
  - >> GUI__AlphaSuppressMixing
  - >> GUI_MEMDEV_GetDataPtr
  - >> GUI_MEMDEV_SetOrg
  - >> GUI_MEMDEV__CreateFixed
  - >> GUI_MEMDEV_Select
  - >> WM__Paint1
  [Called By]
  - >> GUI_MEMDEV_Paint1Static

  _RemoveFromLinList (Thumb, 86 bytes, Stack size 24 bytes, gui_timer.o(i._RemoveFromLinList))
  [Stack]

  - Max Depth = 24
  - Call Chain = _RemoveFromLinList
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  [Called By]
  - >> GUI_TIMER_Delete

  _Unlink (Thumb, 74 bytes, Stack size 24 bytes, gui_timer.o(i._Unlink))
  [Stack]

  - Max Depth = 24
  - Call Chain = _Unlink
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  [Called By]
  - >> GUI_TIMER_Delete

  _Color2IndexBulk (Thumb, 14 bytes, Stack size 8 bytes, guicc_8888.o(i._Color2IndexBulk))
  [Stack]

  - Max Depth = 8
  - Call Chain = _Color2IndexBulk
  [Address Reference Count : 1]
  - guicc_8888.o(.constdata)

  _Color2Index_8888 (Thumb, 2 bytes, Stack size 0 bytes, guicc_8888.o(i._Color2Index_8888))
  [Address Reference Count : 1]

  - guicc_8888.o(.constdata)

  _GetIndexMask_8888 (Thumb, 6 bytes, Stack size 0 bytes, guicc_8888.o(i._GetIndexMask_8888))
  [Address Reference Count : 1]

  - guicc_8888.o(.constdata)

  _Index2ColorBulk (Thumb, 14 bytes, Stack size 8 bytes, guicc_8888.o(i._Index2ColorBulk))
  [Stack]

  - Max Depth = 8
  - Call Chain = _Index2ColorBulk
  [Address Reference Count : 1]
  - guicc_8888.o(.constdata)

  GUI_USAGE_BM_AddHLine (Thumb, 116 bytes, Stack size 16 bytes, guidev_usagebm.o(i.GUI_USAGE_BM_AddHLine))
  [Stack]

  - Max Depth = 16
  - Call Chain = GUI_USAGE_BM_AddHLine
  [Calls]
  - >> __aeabi_memset
  [Address Reference Count : 1]
  - guidev_usagebm.o(.constdata)

  GUI_USAGE_BM_AddPixel (Thumb, 44 bytes, Stack size 8 bytes, guidev_usagebm.o(i.GUI_USAGE_BM_AddPixel))
  [Stack]

  - Max Depth = 8
  - Call Chain = GUI_USAGE_BM_AddPixel
  [Address Reference Count : 1]
  - guidev_usagebm.o(.constdata)

  GUI_USAGE_BM_Clear (Thumb, 14 bytes, Stack size 0 bytes, guidev_usagebm.o(i.GUI_USAGE_BM_Clear))
  [Calls]

  - >> __aeabi_memclr4
  [Address Reference Count : 1]
  - guidev_usagebm.o(.constdata)

  GUI_USAGE_BM_GetNextDirty (Thumb, 154 bytes, Stack size 16 bytes, guidev_usagebm.o(i.GUI_USAGE_BM_GetNextDirty))
  [Stack]

  - Max Depth = 16
  - Call Chain = GUI_USAGE_BM_GetNextDirty
  [Address Reference Count : 1]
  - guidev_usagebm.o(.constdata)

  _GUI_USAGE_BM_Delete (Thumb, 4 bytes, Stack size 0 bytes, guidev_usagebm.o(i._GUI_USAGE_BM_Delete))
  [Stack]

  - Max Depth = 40
  - Call Chain = _GUI_USAGE_BM_Delete ⇒ GUI_ALLOC_Free ⇒ _AddFreeMemory ⇒ _RemoveFreeBlock
  [Calls]
  - >> GUI_ALLOC_Free
  [Address Reference Count : 1]
  - guidev_usagebm.o(.constdata)

  _Convert16 (Thumb, 62 bytes, Stack size 40 bytes, guidev_writetoactiveopaque.o(i._Convert16))
  [Stack]

  - Max Depth = 48
  - Call Chain = _Convert16 ⇒ GUI__CompactPixelIndices
  [Calls]
  - >> GUI__CompactPixelIndices
  [Called By]
  - >> _WriteToActiveOpaque_8

  _Convert8 (Thumb, 62 bytes, Stack size 40 bytes, guidev_writetoactiveopaque.o(i._Convert8))
  [Stack]

  - Max Depth = 48
  - Call Chain = _Convert8 ⇒ GUI__CompactPixelIndices
  [Calls]
  - >> GUI__CompactPixelIndices
  [Called By]
  - >> _WriteToActiveOpaque_8

  _WriteToActiveOpaque_8 (Thumb, 824 bytes, Stack size 168 bytes, guidev_writetoactiveopaque.o(i._WriteToActiveOpaque_8))
  [Stack]

  - Max Depth = 288
  - Call Chain = _WriteToActiveOpaque_8 ⇒ LCD__DrawBitmap_1bpp ⇒ LCD_FillRect
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> GUI_ALLOC_Free
  - >> GUI_ALLOC_AllocNoInit
  - >> GUI_GetpfIndex2ColorEx
  - >> GUI_GetBitsPerPixelEx
  - >> GUI_GetpfColor2IndexEx
  - >> LCD__DrawBitmap_1bpp
  - >> LCD_DrawBitmap
  - >> _Convert8
  - >> _Convert16
  - >> GUI_MEMDEV_GetDataPtr
  [Called By]
  - >> GUI_MEMDEV__WriteToActiveOpaque

  _WriteToActiveOpaque_HT (Thumb, 826 bytes, Stack size 144 bytes, guidev_writetoactiveopaque.o(i._WriteToActiveOpaque_HT))
  [Stack]

  - Max Depth = 248
  - Call Chain = _WriteToActiveOpaque_HT ⇒ LCD_DrawBitmap ⇒ LCD_FillRect
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> GUI_ALLOC_Free
  - >> GUI_ALLOC_AllocNoInit
  - >> GUI_GetBitsPerPixelEx
  - >> LCD_DrawBitmap
  [Called By]
  - >> GUI_MEMDEV__WriteToActiveOpaque

  _MoveDescendents (Thumb, 110 bytes, Stack size 72 bytes, wm_move.o(i._MoveDescendents))
  [Stack]

  - Max Depth = 256 + In Cycle
  - Call Chain = _MoveDescendents ⇒ _MoveDescendents (Cycle)
  [Calls]
  - >> GUI_ALLOC_UnlockH
  - >> GUI_ALLOC_LockH
  - >> WM__SendMessage
  - >> GUI_MoveRect
  - >> _MoveDescendents
  [Called By]
  - >> WM__MoveWindow
  - >> _MoveDescendents

  _fp_digits (Thumb, 334 bytes, Stack size 56 bytes, printfa.o(i._fp_digits), UNUSED)
  [Calls]

  - >> __aeabi_dmul
  - >> __aeabi_ddiv
  - >> __aeabi_dadd
  - >> __aeabi_cdrcmple
  - >> __aeabi_uldivmod
  - >> __aeabi_d2ulz
  [Called By]
  - >> _printf_core

  _printf_core (Thumb, 1744 bytes, Stack size 136 bytes, printfa.o(i._printf_core), UNUSED)
  [Calls]

  - >> __aeabi_uldivmod
  - >> __aeabi_uidivmod
  - >> _printf_pre_padding
  - >> _printf_post_padding
  - >> _fp_digits
  [Called By]
  - >> __0sprintf

  _printf_post_padding (Thumb, 36 bytes, Stack size 24 bytes, printfa.o(i._printf_post_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _printf_pre_padding (Thumb, 46 bytes, Stack size 24 bytes, printfa.o(i._printf_pre_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _sputc (Thumb, 10 bytes, Stack size 0 bytes, printfa.o(i._sputc))
  [Called By]

  - >> __0sprintf
  [Address Reference Count : 1]
  - printfa.o(i.__0sprintf)

  ### Undefined Global Symbols