| MAXREFDES82# Code Documentation V01.00 Maxim Smart Force Sensor

- Main Page
- Modules
- Files

- File List
- Globals

- All
- Functions
- Variables
- Macros

- _
- a
- b
- c
- d
- f
- g
- h
- l
- m
- n
- o
- p
- r
- s
- t
- u
- v
- x
- y

All Files Functions Variables Macros Groups Pages
Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - _ -

- __ALIGN_END : usbd_desc.c

### - a -

- AHBPrescTable : system_stm32f4xx.c
- APP_RX_DATA_SIZE : usbd_cdc_interface.c
- APP_TX_DATA_SIZE : usbd_cdc_interface.c

### - b -

- BK_COLOR : LCDConf_stm32f429i_disco_MB1075.c
- BusFault_Handler() : stm32f4xx_it.c

### - c -

- Calibration() : maintask.c
- cell0Grams : maintask.c
- cell0Load : maintask.c
- cell0Load0 : maintask.c
- cell0Load0Int : maintask.c
- cell0Load0Sign : maintask.c
- cell0Load700 : maintask.c
- cell0Load700Int : maintask.c
- cell0Load700Sign : maintask.c
- cell0Powerup : maintask.c
- cell1Grams : maintask.c
- cell1Load : maintask.c
- cell1Load0 : maintask.c
- cell1Load0Int : maintask.c
- cell1Load0Sign : maintask.c
- cell1Load700 : maintask.c
- cell1Load700Int : maintask.c
- cell1Load700Sign : maintask.c
- cell1Powerup : maintask.c
- cell2Grams : maintask.c
- cell2Load : maintask.c
- cell2Load0 : maintask.c
- cell2Load0Int : maintask.c
- cell2Load0Sign : maintask.c
- cell2Load700 : maintask.c
- cell2Load700Int : maintask.c
- cell2Load700Sign : maintask.c
- cell2Powerup : maintask.c
- cell3Grams : maintask.c
- cell3Load : maintask.c
- cell3Load0 : maintask.c
- cell3Load0Int : maintask.c
- cell3Load0Sign : maintask.c
- cell3Load700 : maintask.c
- cell3Load700Int : maintask.c
- cell3Load700Sign : maintask.c
- cell3Powerup : maintask.c
- COLOR_CONVERSION_0 : LCDConf_stm32f429i_disco_MB1075.c
- ConfigureMAX11254() : maintask.c
- ConfigureSPIandGPIO() : maintask.c

### - d -

- data0 : maintask.c
- data0BO : maintask.c
- data1 : maintask.c
- data1BO : maintask.c
- data2 : maintask.c
- data2BO : maintask.c
- data3 : maintask.c
- data3BO : maintask.c
- DebugMon_Handler() : stm32f4xx_it.c
- DEFINEDMA2D_COLORCONVERSION : LCDConf_stm32f429i_disco_MB1075.c
- DISPLAY_DRIVER_0 : LCDConf_stm32f429i_disco_MB1075.c

### - f -

- FACOTRY_CAL_NUM : maintask.c

### - g -

- GUI_Initialized : MAXREFDES82.c
- GUI_NUM_LAYERS : LCDConf_stm32f429i_disco_MB1075.c
- GUI_NUMBYTES : GUIConf.c
- GUI_X_Config() : GUIConf.c

### - h -

- HAL_DMA2D_MspDeInit() : LCDConf_stm32f429i_disco_MB1075.c
- HAL_DMA2D_MspInit() : LCDConf_stm32f429i_disco_MB1075.c
- HAL_LTDC_LineEvenCallback() : LCDConf_stm32f429i_disco_MB1075.c
- HAL_LTDC_MspDeInit() : LCDConf_stm32f429i_disco_MB1075.c
- HAL_LTDC_MspInit() : LCDConf_stm32f429i_disco_MB1075.c
- HAL_PCD_ConnectCallback() : usbd_conf.c
- HAL_PCD_DataInStageCallback() : usbd_conf.c
- HAL_PCD_DataOutStageCallback() : usbd_conf.c
- HAL_PCD_DisconnectCallback() : usbd_conf.c
- HAL_PCD_ISOINIncompleteCallback() : usbd_conf.c
- HAL_PCD_ISOOUTIncompleteCallback() : usbd_conf.c
- HAL_PCD_MspDeInit() : usbd_conf.c
- HAL_PCD_MspInit() : usbd_conf.c
- HAL_PCD_ResetCallback() : usbd_conf.c
- HAL_PCD_ResumeCallback() : usbd_conf.c
- HAL_PCD_SetupStageCallback() : usbd_conf.c
- HAL_PCD_SOFCallback() : usbd_conf.c
- HAL_PCD_SuspendCallback() : usbd_conf.c
- HAL_TIM_PeriodElapsedCallback() : usbd_cdc_interface.c
- HAL_UART_ErrorCallback() : usbd_cdc_interface.c
- HAL_UART_MspDeInit() : stm32f4xx_hal_msp.c
- HAL_UART_MspInit() : stm32f4xx_hal_msp.c
- HAL_UART_RxCpltCallback() : usbd_cdc_interface.c
- HAL_UART_TxCpltCallback() : usbd_cdc_interface.c
- HardFault_Handler() : stm32f4xx_it.c
- hltdc : LCDConf_stm32f429i_disco_MB1075.c , stm32f4xx_it.c
- hpcd : stm32f4xx_it.c , usbd_conf.c
- HSE_VALUE : system_stm32f4xx.c
- HSI_VALUE : system_stm32f4xx.c

### - l -

- LCD_LAYER0_FRAME_BUFFER : LCDConf_stm32f429i_disco_MB1075.c
- LCD_LAYER1_FRAME_BUFFER : LCDConf_stm32f429i_disco_MB1075.c
- LCD_MIRROR_Y : LCDConf_stm32f429i_disco_MB1075.c
- LCD_SWAP_XY : LCDConf_stm32f429i_disco_MB1075.c
- LCD_X_Config() : LCDConf_stm32f429i_disco_MB1075.c
- LCD_X_DisplayDriver() : LCDConf_stm32f429i_disco_MB1075.c
- LineCoding : usbd_cdc_interface.c
- LTDC_IRQHandler() : stm32f4xx_it.c

### - m -

- main() : MAXREFDES82.c
- MainTask() : maintask.c , MAXREFDES82.c
- MAJORVERSION : maintask.c
- MemManage_Handler() : stm32f4xx_it.c
- MINORVERSION : maintask.c

### - n -

- NMI_Handler() : stm32f4xx_it.c
- NUM_BUFFERS : LCDConf_stm32f429i_disco_MB1075.c
- NUM_VSCREENS : LCDConf_stm32f429i_disco_MB1075.c

### - o -

- OS_TimeMS : stm32f4xx_it.c
- OTG_HS_IRQHandler() : stm32f4xx_it.c

### - p -

- PendSV_Handler() : stm32f4xx_it.c
- POWERUP_CAL_NUM : maintask.c

### - r -

- r : maintask.c
- ReadMAX11254Results() : maintask.c
- Rect : maintask.c
- request : maintask.c , usbd_cdc_interface.c

### - s -

- SectorError : maintask.c
- spiWritePacket : maintask.c
- SVC_Handler() : stm32f4xx_it.c
- SystemCoreClock : system_stm32f4xx.c
- SystemCoreClockUpdate() : system_stm32f4xx.c
- SystemInit() : system_stm32f4xx.c
- SysTick_Handler() : stm32f4xx_it.c

### - t -

- TimHandle : stm32f4xx_it.c , usbd_cdc_interface.c
- TIMx_IRQHandler() : stm32f4xx_it.c

### - u -

- UartHandle : stm32f4xx_it.c , usbd_cdc_interface.c
- UsageFault_Handler() : stm32f4xx_it.c
- USARTx_DMA_TX_IRQHandler() : stm32f4xx_it.c
- USARTx_IRQHandler() : stm32f4xx_it.c
- USBD_CDC_fops : usbd_cdc_interface.c
- USBD_CONFIGURATION_FS_STRING : usbd_desc.c
- USBD_CONFIGURATION_HS_STRING : usbd_desc.c
- USBD_Device : maintask.c , MAXREFDES82.c , usbd_cdc_interface.c
- USBD_INTERFACE_FS_STRING : usbd_desc.c
- USBD_INTERFACE_HS_STRING : usbd_desc.c
- USBD_LANGID_STRING : usbd_desc.c
- USBD_LL_ClearStallEP() : usbd_conf.c
- USBD_LL_CloseEP() : usbd_conf.c
- USBD_LL_DeInit() : usbd_conf.c
- USBD_LL_Delay() : usbd_conf.c
- USBD_LL_FlushEP() : usbd_conf.c
- USBD_LL_GetRxDataSize() : usbd_conf.c
- USBD_LL_Init() : usbd_conf.c
- USBD_LL_IsStallEP() : usbd_conf.c
- USBD_LL_OpenEP() : usbd_conf.c
- USBD_LL_PrepareReceive() : usbd_conf.c
- USBD_LL_SetUSBAddress() : usbd_conf.c
- USBD_LL_StallEP() : usbd_conf.c
- USBD_LL_Start() : usbd_conf.c
- USBD_LL_Stop() : usbd_conf.c
- USBD_LL_Transmit() : usbd_conf.c
- USBD_MANUFACTURER_STRING : usbd_desc.c
- USBD_PID : usbd_desc.c
- USBD_PRODUCT_FS_STRING : usbd_desc.c
- USBD_PRODUCT_HS_STRING : usbd_desc.c
- USBD_StringSerial : usbd_desc.c
- USBD_VCP_ConfigStrDescriptor() : usbd_desc.c
- USBD_VCP_DeviceDescriptor() : usbd_desc.c
- USBD_VCP_InterfaceStrDescriptor() : usbd_desc.c
- USBD_VCP_LangIDStrDescriptor() : usbd_desc.c
- USBD_VCP_ManufacturerStrDescriptor() : usbd_desc.c
- USBD_VCP_ProductStrDescriptor() : usbd_desc.c
- USBD_VCP_SerialStrDescriptor() : usbd_desc.c
- USBD_VID : usbd_desc.c
- usbTxBuf : maintask.c
- UserRxBuffer : usbd_cdc_interface.c
- UserTxBuffer : usbd_cdc_interface.c
- UserTxBufPtrIn : usbd_cdc_interface.c
- UserTxBufPtrOut : usbd_cdc_interface.c

### - v -

- VCP_Desc : usbd_desc.c
- VECT_TAB_OFFSET : system_stm32f4xx.c

### - x -

- x : maintask.c
- XSIZE_PHYS : LCDConf_stm32f429i_disco_MB1075.c

### - y -

- y : maintask.c
- YSIZE_PHYS : LCDConf_stm32f429i_disco_MB1075.c