| MAXREFDES82# Code Documentation V01.00 Maxim Smart Force Sensor

- Main Page
- Modules
- Files

- File List
- Globals

All Files Functions Variables Macros Groups Pages
GUIConf.c
Go to the documentation of this file.
1 /*********************************************************************
2 * Portions COPYRIGHT 2015 STMicroelectronics *
3 * Portions SEGGER Microcontroller GmbH & Co. KG *
4 * Solutions for real time microcontroller applications *
5 **********************************************************************
6 * *
7 * (c) 1996 - 2015 SEGGER Microcontroller GmbH & Co. KG *
8 * *
9 * Internet: www.segger.com Support: support@segger.com *
10 * *
11 **********************************************************************
12
13 ** emWin V5.28 - Graphical user interface for embedded applications **
14 All Intellectual Property rights in the Software belongs to SEGGER.
15 emWin is protected by international copyright laws. Knowledge of the
16 source code may not be used to write a similar product. This file may
17 only be used in accordance with the following terms:
18
19 The software has been licensed to STMicroelectronics International
20 N.V. a Dutch company with a Swiss branch and its headquarters in Plan-
21 les-Ouates, Geneva, 39 Chemin du Champ des Filles, Switzerland for the
22 purposes of creating libraries for ARM Cortex-M-based 32-bit microcon_
23 troller products commercialized by Licensee only, sublicensed and dis_
24 tributed under the terms and conditions of the End User License Agree_
25 ment supplied by STMicroelectronics International N.V.
26 Full source code is available at: www.segger.com
27
28 We appreciate your understanding and fairness.
29 ----------------------------------------------------------------------
30 File : GUIConf.c
31 Purpose : Display controller initialization
32 ---------------------------END-OF-HEADER------------------------------
33 */
34
54 #include "GUI.h"
55
56 /*********************************************************************
57 *
58 * Defines
59 *
60 **********************************************************************
61 */
62 //
63 // Define the available number of bytes available for the GUI
64 //
65 #define GUI_NUMBYTES (1024) * 150
66
67
68 /*********************************************************************
69 *
70 * Public code
71 *
72 **********************************************************************
73 */
74 /*********************************************************************
75 *
76 * GUI_X_Config
77 *
78 * Purpose:
79 * Called during the initialization process in order to set up the
80 * available memory for the GUI.
81 */
82 void GUI_X_Config(void) {
83 //
84 // 32 bit aligned memory area
85 //
86 static U32 aMemory[GUI_NUMBYTES / 4];
87 //
88 // Assign memory to emWin
89 //
90 GUI_ALLOC_AssignMemory(aMemory, GUI_NUMBYTES);
91 //
92 // Set default font
93 //
94 GUI_SetDefaultFont(GUI_FONT_6X8);
95 }
96
97 /*************************** End of file ****************************/