| MAXREFDES82# Code Documentation V01.00 Maxim Smart Force Sensor

- Main Page
- Modules
- Files

All Files Functions Variables Macros Groups Pages
Functions
USBD_USR_MAIN
USBD_USER

This file is the CDC application main file. More...

## Functions
void | HAL_UART_MspInit (UART_HandleTypeDef *huart)
| UART MSP Initialization This function configures the hardware resources used in this application:
void | HAL_UART_MspDeInit (UART_HandleTypeDef *huart)
| UART MSP De-Initialization This function frees the hardware resources used in this application:

## Detailed Description

This file is the CDC application main file.

## Function Documentation

void HAL_UART_MspDeInit | ( | UART_HandleTypeDef * | huart | ) |

UART MSP De-Initialization This function frees the hardware resources used in this application:

         - Disable the Peripheral's clock
         - Revert GPIO, and NVIC configuration to their default state

Parameters

  huart,: | UART handle pointer

Return values

  None |

Definition at line 148 of file stm32f4xx_hal_msp.c.

void HAL_UART_MspInit | ( | UART_HandleTypeDef * | huart | ) |

UART MSP Initialization This function configures the hardware resources used in this application:

          - Peripheral's clock enable
          - Peripheral's GPIO Configuration
          - NVIC configuration for UART interrupt request enable

Parameters

  huart,: | UART handle pointer

Return values

  None |

Definition at line 68 of file stm32f4xx_hal_msp.c.