-------------------------------------------------------------------
        Release Notes for the Power Monitor Utility
-------------------------------------------------------------------

                Microchip Technology, Inc.




-------------------------------------------------------------------
System Requirements
-------------------------------------------------------------------
Operating System:  Windows XP SP3 or later
Other:  .NET4 Framework (Client Profile)


** NOTE:  Admin privileges are required for installation. **



-------------------------------------------------------------------
Important Information   
-------------------------------------------------------------------
******* Driver Installation *******

  BE SURE TO ACCEPT ANY WARNINGS GIVEN DURING THE INSTALLATION. A 
required driver for the USB device communication is installed 
during the application installation and the warning must be accepted
in order for the application to run properly. Please be aware that 
the driver installation can take some time (up to a few minutes).


****** Driver Uninstallation *******

  To uninstall this driver, simply go to the Windows Control Panel
and select "Add/Remove Programs" (or "Programs and Features" in 
Vista and 7).  Double-click (uninstall) the item named the following:
"Windows Driver Package - Microchip Technology, Inc. (usbser) ..."

  

-------------------------------------------------------------------
Versioning History
-------------------------------------------------------------------
Version 1.4.2 (12-Jun-2019)
 - added DC current offset calibration for MCP39F511A
 
Version 1.4.1.1 (16-Aug-2018)
 - fixed: MCP39F511A frequency register was not written during calibration
 
Version 1.4.1 (20-Jun-2018)
 - calibration register file is saved in MyDocuments, not the program folder

Version 1.4 (14-Mar-2018)
 - added support for MCP39F511A
 
Version 1.3.1 (Released 28-Sept-2016)
 - fixed: event selection not working for MCP39F521
 
Version 1.3 (Relelased 23-June-2016)
 - fixed register file for MCP39F511 FW rev < 0xFA14
 - fixed: MCP39F511 (FW > 0xFA14) could not reconnect to board after
          changing the baud rate and saving to flash.
          
Version 1.2 (Released 4-Jan-2016)
 - added support for MCP39F511N
 
Version 1.1
 - updated layout
 - added support for MCP39F511 system version 0xFA14

Version 1.0.0 (Released 16-Sept-2015):
 - Initial release of the software



-------------------------------------------------------------------
Contact Information
-------------------------------------------------------------------
Main Website: 		http://www.microchip.com
Technical Support: 	http://support.microchip.com

