Cross Section Report
C:/svn_work/cc13xx/CC13xx_EM_Design/7x7/CC13xxEM-7XD-7793_4L/Cadence/allegro/CC13xxEM-7XD-7793_4L.brd
Mon Jun 22 15:16:25 2015

Design Cross Section
Subclass Name,Type,Material,Thickness (MM),Conductivity (mho/cm),Dielectric Constant,Loss Tangent,Negative Artwork,Shield,Width (MM),Unused Pin Pad Suppression,Unused Via Pad Suppression
,SURFACE,AIR,,0,1,0,,,,,
TOP,CONDUCTOR,COPPER,0.035,595900,4.5,0,,,0.127,,
,DIELECTRIC,FR-4,0.175,0,4.5,0.035,,,,,
L2,PLANE,COPPER,0.0175,595900,4.5,0.035,,Yes,,,
,DIELECTRIC,FR-4,1.140000,0,4.5,0.035,,,,,
L3,PLANE,COPPER,0.0175,595900,4.5,0.035,,Yes,,,
,DIELECTRIC,FR-4,0.175,0,4.5,0.035,,,,,
BOTTOM,CONDUCTOR,COPPER,0.035,595900,4.5,0,,,0.127,,
,SURFACE,AIR,,0,1,0,,,,,

Total Thickness: 1.595 MM
