<?xml version="1.0" encoding="UTF-8" standalone="no"?>
<configurations XML_version="1.2" id="configurations_0">
<configuration XML_version="1.2" id="Texas Instruments XDS100v2 USB Debug Probe_0">
        <instance XML_version="1.2" desc="Texas Instruments XDS100v2 USB Debug Probe_0" href="connections/TIXDS100v2_Connection.xml" id="Texas Instruments XDS100v2 USB Debug Probe_0" xml="TIXDS100v2_Connection.xml" xmlpath="connections"/>
        <connection XML_version="1.2" id="Texas Instruments XDS100v2 USB Debug Probe_0">
            <instance XML_version="1.2" href="drivers/tixds100v2icepick_d.xml" id="drivers" xml="tixds100v2icepick_d.xml" xmlpath="drivers"/>
            <instance XML_version="1.2" href="drivers/tixds100v2c674x.xml" id="drivers" xml="tixds100v2c674x.xml" xmlpath="drivers"/>
            <instance XML_version="1.2" href="drivers/tixds100v2arm9.xml" id="drivers" xml="tixds100v2arm9.xml" xmlpath="drivers"/>
            <instance XML_version="1.2" href="drivers/tixds100v2cs_dap.xml" id="drivers" xml="tixds100v2cs_dap.xml" xmlpath="drivers"/>
            <instance XML_version="1.2" href="drivers/tixds100v2cortexM.xml" id="drivers" xml="tixds100v2cortexM.xml" xmlpath="drivers"/>
            <instance XML_version="1.2" href="drivers/tixds100v2cs_child.xml" id="drivers" xml="tixds100v2cs_child.xml" xmlpath="drivers"/>
            <instance XML_version="1.2" href="drivers/tixds100v2cortexA.xml" id="drivers" xml="tixds100v2cortexA.xml" xmlpath="drivers"/>
            <instance XML_version="1.2" href="drivers/tixds100v2csstm.xml" id="drivers" xml="tixds100v2csstm.xml" xmlpath="drivers"/>
            <instance XML_version="1.2" href="drivers/tixds100v2etbcs.xml" id="drivers" xml="tixds100v2etbcs.xml" xmlpath="drivers"/>
            <property Type="choicelist" Value="3" id="The JTAG TCLK Frequency (MHz)"/>
            <platform XML_version="1.2" id="platform_0">
                <instance XML_version="1.2" desc="TI814x_0" href="devices/ti814x.xml" id="TI814x_0" xml="ti814x.xml" xmlpath="devices"/>
                <device HW_revision="1" XML_version="1.2" description="TI814x" id="TI814x_0" partnum="TI814x">
                    <router HW_revision="1.0" XML_version="1.2" description="ICEPick_D Router" id="IcePick_D_0" isa="ICEPICK_D">
                        <subpath id="subpath_10">
                            <router HW_revision="1.0" XML_version="1.2" description="CS_DAP Router" id="CS_DAP_1" isa="CS_DAP">
                                <subpath id="subpath_2">
                                    <property Type="numericfield" Value="0x1a" desc="Port Number_0" id="Port Number"/>
                                    <cpu HW_revision="1.0" XML_version="1.2" desc="ICECrusherCS_1" description="Cross Triggering" id="ICECrusherCS_0" isa="cs_child"/>
                                </subpath>
                            </router>
                        </subpath>
                        <subpath id="subpath_11">
                            <router HW_revision="1.0" XML_version="1.2" description="CS_DAP Router" id="CS_DAP_2" isa="CS_DAP">
                                <subpath id="subpath_3">
                                    <property Type="numericfield" Value="0x1b" desc="Port Number_1" id="Port Number"/>
                                </subpath>
                            </router>
                        </subpath>
                    </router>
                </device>
            </platform>
        </connection>
    </configuration>
</configurations>
