JUMPER CONFIG	OCT 7 99

JP10 IS CW/CADENCED SELECT IN = CW OUT = CADENCED
WHEN IN:
	IF 	1) 	JP14 IS IN OR
		2)	SW1 IS DEPRESSED OR
		3)  	CADENCE IN IS PULLED LOW

	THEN	CONTINOUS SINEWAVE IS OUTPUT.
	ELSE	CONTINOUS ZERO IS OUTPUT

WHEN OUT:
	IF 	1) 	JP14 IS IN OR
		2)	SW1 IS DEPRESSED OR
		3)  	CADENCE IN IS PULLED LOW

	THEN	CADENCED SINEWAVE IS OUTPUT
	ELSE	CONTINOUS ZERO IS OUTPUT

JP12 IS CONNECT RELAY MODE IN = TEST OUT = NORMAL

	WHEN	JP12 IS IN AND
		JP10 IS IN AND

	IF 	1) 	JP14 IS IN OR
		2)	SW1 IS DEPRESSED OR
		3)  	CADENCE IN IS PULLED LOW

	THEN	CONTINOUS SINEWAVE IS OUTPUT.
		THE CONNECT RELAY (TP13) IS ENERGIZED EVERY EIGHTH CYCLE

	ELSE	CONTINOUS ZERO IS OUTPUT
		THE CONNECT RELAY (TP13) IS DE-ENERGIZED CONTINOUSLY		

	WHEN	JP12 IS IN AND
		JP10 IS OUT AND

	IF 	1) 	JP14 IS IN OR
		2)	SW1 IS DEPRESSED OR
		3)  	CADENCE IN IS PULLED LOW

	THEN	CADENCED SINEWAVE IS OUTPUT.
		THE CONNECT RELAY (TP13) IS ENERGIZED EVERY EIGHTH CADENCE

	ELSE	CONTINOUS ZERO IS OUTPUT
		THE CONNECT RELAY (TP13) IS DE-ENERGIZED CONTINOUSLY



	WHEN	JP12 IS OUT AND
		JP10 IS IN AND

	IF 	1) 	JP14 IS IN OR
		2)	SW1 IS DEPRESSED OR
		3)  	CADENCE IN IS PULLED LOW

	THEN	CONTINOUS SINEWAVE IS OUTPUT.
		THE CONNECT RELAY (TP13) IS ENERGIZED CONTINOUSLY

	ELSE	CONTINOUS ZERO IS OUTPUT
		THE CONNECT RELAY (TP13) IS DE-ENERGIZED CONTINOUSLY

	WHEN	JP12 IS OUT AND
		JP10 IS OUT AND

	IF 	1) 	JP14 IS IN OR
		2)	SW1 IS DEPRESSED OR
		3)  	CADENCE IN IS PULLED LOW

	THEN	CADENCED SINEWAVE IS OUTPUT.
		THE CONNECT RELAY (TP13) IS ENERGIZED EVERY CADENCED CYCLE

	ELSE	CONTINOUS ZERO IS OUTPUT
		THE CONNECT RELAY (TP13) IS DE-ENERGIZED CONTINOUSLY


	
JUMPER 6:	SOFTSTART AND UNDERVOLTAGE LOCKOUT DISABLE

	WHEN 	JP6 IS IN	THERE IS NO SOFTSTART OR UNDERVOLTAGE LOCKOUT\
		JP6 IS OUT 	SOFTSTART STARTS @ 4.75V AND
				UNDERVOLTAGE LOCKOUT SHUTS DOWN AT 4.5V

JUMPERS 4 & 5	HIGH OUTPUT CURRENT / LOW OUTPUT CURRENT
	
	WHEN 	JP4&5 ARE IN 	THE OUTPUT CAPACITY OF THE DEMO BOARD IS 10 REN
		JP4&5 ARE OUT	THE OUTPUT CAPACITY IS 1 REN



PATH CONFIGURATION JUMPERS:

JUMPER 15	PWM SOURCE SELECTOR

	WHEN	JP15 IS BRIDGING 1&2	INTERNAL PWM IS SELECTED
		JP15 IS BRIDGING 2&3	EXTERNAL PWM IS SELECTED VIA TP8


JUMPERS 1&2&3	REFERENCE MODE JUMPERS
	THE ORIGIONAL SOFTWARE 10/11/99 DOES NOT SUPPORT VARIABLE REFERENCE MODE
	SO THE JUMPERS MUST BE PLACED AS FOLLOWS:

		JP1 MUST BRIDGE PINS 2&3
		JP2 MUST BRIDGE PINS 2&3
		JP3 MUST BRIDGE PINS 1&2


UNUSED JUMPERS:
		JP7
		JP8
		JP9
		JP11
		JP13

UNUSED I/O PORTS:
		BNC		ANALOG IN
		J4		RS232 IN
		TP10,11,12	SMBUSS


FOR TEST SET JUMPERS AS FOLLOWS
	JP1	BRIDGE PINS 2&3
	JP2	BRIDGE PINS 2&3
	JP3	BRIDGE PINS	1&2
	JP4 	INSTALLED
	JP5 	INSTALLED
	JP6	OPEN
	JP7	OMIT
	JP8	OMIT
	JP9	OMIT
	JP10	OPEN
	JP11	OMIT
	JP12	OPEN
	JP13 	OMIT
	JP14	INSTALLED
	JP15	BRIDGE PINS 1&2

APPLY 5V BY J2 (+ IN CENTER)
APPLY RIGHT INDEX FINGER TO TP1
APPLY RIGHT LONG FINGER TO TP2
LOOK AT THE LEDS TWINKLE
