Sonoma (MAXREFDES14#) Code Documentation V01.00 Isolated EMP (Energy Measurement Processor)

- Main Page
- Data Structures
- Files

- File List
- Globals

- All
- Functions
- Variables
- Macros

- c
- d
- e
- g
- h
- i
- l
- m
- n
- p
- r
- s
- w

All Data Structures Files Functions Variables Macros Pages

### - c -

- check_if_i2c_device_is_present() : utilities.c , utilities.h
- cleanup_platform() : platform.c , platform.h

### - d -

- delay() : utilities.c , utilities.h
- disable_caches() : platform.c

### - e -

- enable_caches() : platform.c

### - g -

- GetLine() : utilities.c , utilities.h
- getUartByte() : utilities.c , utilities.h

### - h -

- htoi() : utilities.c , utilities.h

### - i -

- init_platform() : platform.c , platform.h
- init_uart() : platform.c

### - l -

- led_knight_rider() : utilities.c , utilities.h

### - m -

- main() : MAXREFDES14.c
- max_configure_PMOD_port() : utilities.c , utilities.h
- menu_cls() : menu.c , menu.h
- menu_print_line() : menu.c
- menu_print_main_menu() : menu.h , menu.c
- menu_print_maxim_banner() : menu.c , menu.h
- menu_print_maxim_banner_big() : menu.c , menu.h
- menu_print_prompt() : menu.h , menu.c
- menu_read_reg() : menu.c
- menu_retrieve_keypress() : menu.h , menu.c

### - n -

- number_raised_to_power() : utilities.c , utilities.h

### - p -

- print_asterisks() : utilities.c , utilities.h
- print_seven_segment_four_digits() : utilities.h
- print_seven_segment_number() : utilities.h
- print_seven_segment_temperature() : utilities.h
- print_seven_segment_time() : utilities.h
- printf_temp() : utilities.h , utilities.c

### - r -

- read_reg() : maximDeviceSpecificUtilities.c , maximDeviceSpecificUtilities.h
- receive_byte_with_timeout() : utilities.c , utilities.h

### - s -

- set_seven_segment_character() : utilities.h
- SpiRW() : utilities.h , utilities.c

### - w -

- write_reg() : maximDeviceSpecificUtilities.c , maximDeviceSpecificUtilities.h