Description
  Default configuration for ZedBoard Created 28 Aug 2012 See more at www.zedboard.org Change Log 28 Aug 2012 - Changed DDR3 part to MT41J128M16 HA-15E

## Preset Info

Device Size | xc7z020
Package | clg484
Speed Grade | -1

## Zynq PS configuration

Peripheral | Status | Signal Group | MIO | Freq
--- | --- | --- | --- | ---
CAN0 | Disabled |  |  |
CAN1 | Disabled |  |  |
ENET0 | Enabled | default | MIO 16 .. 27 | 1000 MBPS
|  | GRP_MDIO | MIO 52 .. 53 |
ENET1 | Disabled |  |  |
GPIO | Enabled | default | MIO |
I2C0 | Disabled |  |  |
I2C1 | Disabled |  |  |
MODE | Disabled |  |  |
NAND | Disabled |  |  |
NOR | Disabled |  |  |
PJTAG | Disabled |  |  |
QSPI | Enabled | default | MIO 1 .. 6 | 200.000000
|  | GRP_FBCLK | MIO 8 |
SD0 | Enabled | default | MIO 40 .. 45 |
|  | GRP_CD | MIO 47 |
|  | GRP_WP | MIO 46 |
SD1 | Disabled |  |  |
SPI0 | Disabled |  |  |
SPI1 | Disabled |  |  |
TRACE | Disabled |  |  |
TTC0 | Enabled | default | EMIO |
TTC1 | Disabled |  |  |
UART0 | Disabled |  |  |
UART1 | Enabled | default | MIO 48 .. 49 | 50
USB0 | Enabled | default | MIO 28 .. 39 |
USB1 | Disabled |  |  |
VCFG | Disabled |  |  |
WDT | Disabled |  |  |