Following peripherals are selected in the design.

## Peripheral Selected

- Quad SPI Flash
- SD 0
- UART 1
- SPI 1

To see detailed information please follow below links:

- MIO Configuration Table
- Zynq Peripheral Configuration
- DDR Configuration Information
- SLCR settings

- PLL Init Data
- Clock Init Data
- DDR Init Data
- MIO Init Data

## MIO configuration Table

MIO Pin | Peripheral | Signal | IO type | Speed | Pullup | Direction
--- | --- | --- | --- | --- | --- | ---
MIO 0 |  |  |  |  |  |
MIO 1 | Quad SPI Flash | qspi0_ss_b | LVCMOS 3.3V | fast | disabled | out
MIO 2 | Quad SPI Flash | qspi0_io[0] | LVCMOS 3.3V | fast | disabled | inout
MIO 3 | Quad SPI Flash | qspi0_io[1] | LVCMOS 3.3V | fast | disabled | inout
MIO 4 | Quad SPI Flash | qspi0_io[2] | LVCMOS 3.3V | fast | disabled | inout
MIO 5 | Quad SPI Flash | qspi0_io[3] | LVCMOS 3.3V | fast | disabled | inout
MIO 6 | Quad SPI Flash | qspi0_sclk | LVCMOS 3.3V | fast | disabled | out
MIO 7 |  |  |  |  |  |
MIO 8 | Quad SPI Flash | qspi_fbclk | LVCMOS 3.3V | fast | disabled | out
MIO 9 |  |  |  |  |  |
MIO 10 |  |  |  |  |  |
MIO 11 |  |  |  |  |  |
MIO 12 |  |  |  |  |  |
MIO 13 |  |  |  |  |  |
MIO 14 |  |  |  |  |  |
MIO 15 |  |  |  |  |  |
MIO 16 |  |  |  |  |  |
MIO 17 |  |  |  |  |  |
MIO 18 |  |  |  |  |  |
MIO 19 |  |  |  |  |  |
MIO 20 |  |  |  |  |  |
MIO 21 |  |  |  |  |  |
MIO 22 |  |  |  |  |  |
MIO 23 |  |  |  |  |  |
MIO 24 |  |  |  |  |  |
MIO 25 |  |  |  |  |  |
MIO 26 |  |  |  |  |  |
MIO 27 |  |  |  |  |  |
MIO 28 |  |  |  |  |  |
MIO 29 |  |  |  |  |  |
MIO 30 |  |  |  |  |  |
MIO 31 |  |  |  |  |  |
MIO 32 |  |  |  |  |  |
MIO 33 |  |  |  |  |  |
MIO 34 |  |  |  |  |  |
MIO 35 |  |  |  |  |  |
MIO 36 |  |  |  |  |  |
MIO 37 |  |  |  |  |  |
MIO 38 |  |  |  |  |  |
MIO 39 |  |  |  |  |  |
MIO 40 | SD 0 | clk | LVCMOS 1.8V | fast | disabled | out
MIO 41 | SD 0 | cmd | LVCMOS 1.8V | fast | disabled | inout
MIO 42 | SD 0 | data[0] | LVCMOS 1.8V | fast | disabled | inout
MIO 43 | SD 0 | data[1] | LVCMOS 1.8V | fast | disabled | inout
MIO 44 | SD 0 | data[2] | LVCMOS 1.8V | fast | disabled | inout
MIO 45 | SD 0 | data[3] | LVCMOS 1.8V | fast | disabled | inout
MIO 46 | SD 0 | wp | LVCMOS 1.8V | slow | disabled | in
MIO 47 | SD 0 | cd | LVCMOS 1.8V | slow | disabled | in
MIO 48 | UART 1 | tx | LVCMOS 1.8V | slow | disabled | out
MIO 49 | UART 1 | rx | LVCMOS 1.8V | slow | disabled | in
MIO 50 |  |  |  |  |  |
MIO 51 |  |  |  |  |  |
MIO 52 |  |  |  |  |  |
MIO 53 |  |  |  |  |  |

- Go To TOP

## Zynq Peripheral Configuration

Peripheral | Signal Group | Signal | MIO
Quad SPI Flash |  |  | MIO 1 .. 6
| Dual Quad SPI (4 bit) |  | Disabled
| Dual Quad SPI (Parallel 8 bit) |  | Disabled
| Feedback Clk |  | MIO 8
SRAM/NOR Flash |  |  | Disabled
NAND Flash |  |  | Disabled
Enet 0 |  |  | Disabled
Enet 1 |  |  | Disabled
USB 0 |  |  | Disabled
USB 1 |  |  | Disabled
SD 0 |  |  | MIO 40 .. 45
| CD |  | MIO 47
| WP |  | MIO 46
| Power |  | Disabled
SD 1 |  |  | Disabled
UART 0 |  |  | Disabled
UART 1 |  |  | MIO 48 .. 49
|  | rx | MIO 49
|  | tx | MIO 48
| Modem Signals |  | Disabled
I2C 0 |  |  | Disabled
I2C 1 |  |  | Disabled
SPI 0 |  |  | Disabled
SPI 1 |  |  | EMIO
| SS[0] |  | EMIO
| SS[1] |  | EMIO
| SS[2] |  | EMIO
CAN 0 |  |  | Disabled
CAN 1 |  |  | Disabled
Trace |  |  | Disabled
Timer 0 |  |  | Disabled
Timer 1 |  |  | Disabled
Watchdog |  |  | Disabled
PJTAG |  |  | Disabled
GPIO |  |  | Disabled
Mode |  |  | Disabled
VCfg |  |  | Disabled

- Go To TOP

## DDR Memory information

### DDR Controller Configuration

Parameter | Value
Enable DDR | 1
Memory Type | DDR 3
Memory Part | MT41J128M16 HA-15E
DRAM bus width | 32 Bit
ECC | Disabled
BURST Length (lppdr only) | 8
Internal Vref | 1
Operating Frequency (MHz) | 533.333333
HIGH temperature | Normal (0-85)

### Memory Part Configuration

Parameter | Value
DRAM IC bus width | 16 Bits
DRAM Device Capacity | 2048 MBits
Speed Bin | DDR3_1066F
BANK Address Count | 3
ROW Address Count | 14
COLUMN Address Count | 10
CAS Latency | 7
CAS Write Latency | 6
RAS to CAS Delay | 7
RECHARGE Time | 7
tRC (ns ) | 49.5
tRASmin ( ns ) | 36.0
tFAW | 45.0
ADDITIVE Latency | 0

### Training/Board Details

Parameter | Value
Write levelling | 1
Read gate | 1
Read data eye | 1
DQS to Clock delay [0] (ns) | 0.025
DQS to Clock delay [1] (ns) | 0.028
DQS to Clock delay [2] (ns) | -0.009
DQS to Clock delay [3] (ns) | -0.061
Board delay [0] (ns) | 0.41
Board delay [1] (ns) | 0.411
Board delay [2] (ns) | 0.341
Board delay [3] (ns) | 0.358

- Go To TOP

# ps7_pll_init_data

## SLCR SETTINGS

SLCR SETTINGS

- Register : SLCR_UNLOCK @ 0XF8000008

  Bitfield | Bits | Mask | Value | Shifted Value
  UNLOCK_KEY | 15:0 | ffff | df0d | df0d
  SLCR_UNLOCK @ 0XF8000008 |  | ffff |  | df0d

## PLL SLCR REGISTERS

PLL SLCR REGISTERS

## ARM PLL INIT

ARM PLL INIT

- Register : ARM_PLL_CFG @ 0XF8000110

  Bitfield | Bits | Mask | Value | Shifted Value
  PLL_RES | 7:4 | f0 | 2 | 20
  PLL_CP | 11:8 | f00 | 2 | 200
  LOCK_CNT | 21:12 | 3ff000 | fa | fa000
  ARM_PLL_CFG @ 0XF8000110 |  | 3ffff0 |  | fa220

## UPDATE FB_DIV

UPDATE FB_DIV

- Register : ARM_PLL_CTRL @ 0XF8000100

  Bitfield | Bits | Mask | Value | Shifted Value
  PLL_FDIV | 18:12 | 7f000 | 28 | 28000
  ARM_PLL_CTRL @ 0XF8000100 |  | 7f000 |  | 28000

## BY PASS PLL

BY PASS PLL

- Register : ARM_PLL_CTRL @ 0XF8000100

  Bitfield | Bits | Mask | Value | Shifted Value
  PLL_BYPASS_FORCE | 4:4 | 10 | 1 | 10
  ARM_PLL_CTRL @ 0XF8000100 |  | 10 |  | 10

## ASSERT RESET

ASSERT RESET

- Register : ARM_PLL_CTRL @ 0XF8000100

  Bitfield | Bits | Mask | Value | Shifted Value
  PLL_RESET | 0:0 | 1 | 1 | 1
  ARM_PLL_CTRL @ 0XF8000100 |  | 1 |  | 1

## DEASSERT RESET

DEASSERT RESET

- Register : ARM_PLL_CTRL @ 0XF8000100

  Bitfield | Bits | Mask | Value | Shifted Value
  PLL_RESET | 0:0 | 1 | 0 | 0
  ARM_PLL_CTRL @ 0XF8000100 |  | 1 |  | 0

## CHECK PLL STATUS

CHECK PLL STATUS

- Register : PLL_STATUS @ 0XF800010C

  Bitfield | Bits | Mask | Value | Shifted Value
  ARM_PLL_LOCK | 0:0 | 1 | 1 | 1
  PLL_STATUS @ 0XF800010C |  | 1 |  | 1

## REMOVE PLL BY PASS

REMOVE PLL BY PASS

- Register : ARM_PLL_CTRL @ 0XF8000100

  Bitfield | Bits | Mask | Value | Shifted Value
  PLL_BYPASS_FORCE | 4:4 | 10 | 0 | 0
  ARM_PLL_CTRL @ 0XF8000100 |  | 10 |  | 0

- Register : ARM_CLK_CTRL @ 0XF8000120

  Bitfield | Bits | Mask | Value | Shifted Value
  SRCSEL | 5:4 | 30 | 0 | 0
  DIVISOR | 13:8 | 3f00 | 2 | 200
  CPU_6OR4XCLKACT | 24:24 | 1000000 | 1 | 1000000
  CPU_3OR2XCLKACT | 25:25 | 2000000 | 1 | 2000000
  CPU_2XCLKACT | 26:26 | 4000000 | 1 | 4000000
  CPU_1XCLKACT | 27:27 | 8000000 | 1 | 8000000
  CPU_PERI_CLKACT | 28:28 | 10000000 | 1 | 10000000
  ARM_CLK_CTRL @ 0XF8000120 |  | 1f003f30 |  | 1f000200

## DDR PLL INIT

DDR PLL INIT

- Register : DDR_PLL_CFG @ 0XF8000114

  Bitfield | Bits | Mask | Value | Shifted Value
  PLL_RES | 7:4 | f0 | 2 | 20
  PLL_CP | 11:8 | f00 | 2 | 200
  LOCK_CNT | 21:12 | 3ff000 | 12c | 12c000
  DDR_PLL_CFG @ 0XF8000114 |  | 3ffff0 |  | 12c220

## UPDATE FB_DIV

UPDATE FB_DIV

- Register : DDR_PLL_CTRL @ 0XF8000104

  Bitfield | Bits | Mask | Value | Shifted Value
  PLL_FDIV | 18:12 | 7f000 | 20 | 20000
  DDR_PLL_CTRL @ 0XF8000104 |  | 7f000 |  | 20000

## BY PASS PLL

BY PASS PLL

- Register : DDR_PLL_CTRL @ 0XF8000104

  Bitfield | Bits | Mask | Value | Shifted Value
  PLL_BYPASS_FORCE | 4:4 | 10 | 1 | 10
  DDR_PLL_CTRL @ 0XF8000104 |  | 10 |  | 10

## ASSERT RESET

ASSERT RESET

- Register : DDR_PLL_CTRL @ 0XF8000104

  Bitfield | Bits | Mask | Value | Shifted Value
  PLL_RESET | 0:0 | 1 | 1 | 1
  DDR_PLL_CTRL @ 0XF8000104 |  | 1 |  | 1

## DEASSERT RESET

DEASSERT RESET

- Register : DDR_PLL_CTRL @ 0XF8000104

  Bitfield | Bits | Mask | Value | Shifted Value
  PLL_RESET | 0:0 | 1 | 0 | 0
  DDR_PLL_CTRL @ 0XF8000104 |  | 1 |  | 0

## CHECK PLL STATUS

CHECK PLL STATUS

- Register : PLL_STATUS @ 0XF800010C

  Bitfield | Bits | Mask | Value | Shifted Value
  DDR_PLL_LOCK | 1:1 | 2 | 1 | 2
  PLL_STATUS @ 0XF800010C |  | 2 |  | 2

## REMOVE PLL BY PASS

REMOVE PLL BY PASS

- Register : DDR_PLL_CTRL @ 0XF8000104

  Bitfield | Bits | Mask | Value | Shifted Value
  PLL_BYPASS_FORCE | 4:4 | 10 | 0 | 0
  DDR_PLL_CTRL @ 0XF8000104 |  | 10 |  | 0

- Register : DDR_CLK_CTRL @ 0XF8000124

  Bitfield | Bits | Mask | Value | Shifted Value
  DDR_3XCLKACT | 0:0 | 1 | 1 | 1
  DDR_2XCLKACT | 1:1 | 2 | 1 | 2
  DDR_3XCLK_DIVISOR | 25:20 | 3f00000 | 2 | 200000
  DDR_2XCLK_DIVISOR | 31:26 | fc000000 | 3 | c000000
  DDR_CLK_CTRL @ 0XF8000124 |  | fff00003 |  | c200003

## IO PLL INIT

IO PLL INIT

- Register : IO_PLL_CFG @ 0XF8000118

  Bitfield | Bits | Mask | Value | Shifted Value
  PLL_RES | 7:4 | f0 | 4 | 40
  PLL_CP | 11:8 | f00 | 2 | 200
  LOCK_CNT | 21:12 | 3ff000 | fa | fa000
  IO_PLL_CFG @ 0XF8000118 |  | 3ffff0 |  | fa240

## UPDATE FB_DIV

UPDATE FB_DIV

- Register : IO_PLL_CTRL @ 0XF8000108

  Bitfield | Bits | Mask | Value | Shifted Value
  PLL_FDIV | 18:12 | 7f000 | 30 | 30000
  IO_PLL_CTRL @ 0XF8000108 |  | 7f000 |  | 30000

## BY PASS PLL

BY PASS PLL

- Register : IO_PLL_CTRL @ 0XF8000108

  Bitfield | Bits | Mask | Value | Shifted Value
  PLL_BYPASS_FORCE | 4:4 | 10 | 1 | 10
  IO_PLL_CTRL @ 0XF8000108 |  | 10 |  | 10

## ASSERT RESET

ASSERT RESET

- Register : IO_PLL_CTRL @ 0XF8000108

  Bitfield | Bits | Mask | Value | Shifted Value
  PLL_RESET | 0:0 | 1 | 1 | 1
  IO_PLL_CTRL @ 0XF8000108 |  | 1 |  | 1

## DEASSERT RESET

DEASSERT RESET

- Register : IO_PLL_CTRL @ 0XF8000108

  Bitfield | Bits | Mask | Value | Shifted Value
  PLL_RESET | 0:0 | 1 | 0 | 0
  IO_PLL_CTRL @ 0XF8000108 |  | 1 |  | 0

## CHECK PLL STATUS

CHECK PLL STATUS

- Register : PLL_STATUS @ 0XF800010C

  Bitfield | Bits | Mask | Value | Shifted Value
  IO_PLL_LOCK | 2:2 | 4 | 1 | 4
  PLL_STATUS @ 0XF800010C |  | 4 |  | 4

## REMOVE PLL BY PASS

REMOVE PLL BY PASS

- Register : IO_PLL_CTRL @ 0XF8000108

  Bitfield | Bits | Mask | Value | Shifted Value
  PLL_BYPASS_FORCE | 4:4 | 10 | 0 | 0
  IO_PLL_CTRL @ 0XF8000108 |  | 10 |  | 0

## LOCK IT BACK

LOCK IT BACK

- Register : SLCR_LOCK @ 0XF8000004

  Bitfield | Bits | Mask | Value | Shifted Value
  LOCK_KEY | 15:0 | ffff | 767b | 767b
  SLCR_LOCK @ 0XF8000004 |  | ffff |  | 767b

# ps7_clock_init_data

## SLCR SETTINGS

SLCR SETTINGS

- Register : SLCR_UNLOCK @ 0XF8000008

  Bitfield | Bits | Mask | Value | Shifted Value
  UNLOCK_KEY | 15:0 | ffff | df0d | df0d
  SLCR_UNLOCK @ 0XF8000008 |  | ffff |  | df0d

## CLOCK CONTROL SLCR REGISTERS

CLOCK CONTROL SLCR REGISTERS

- Register : DCI_CLK_CTRL @ 0XF8000128

  Bitfield | Bits | Mask | Value | Shifted Value
  CLKACT | 0:0 | 1 | 0 | 0
  DIVISOR0 | 13:8 | 3f00 | 23 | 2300
  DIVISOR1 | 25:20 | 3f00000 | 3 | 300000
  DCI_CLK_CTRL @ 0XF8000128 |  | 3f03f01 |  | 302300

- Register : LQSPI_CLK_CTRL @ 0XF800014C

  Bitfield | Bits | Mask | Value | Shifted Value
  CLKACT | 0:0 | 1 | 1 | 1
  SRCSEL | 5:4 | 30 | 2 | 20
  DIVISOR | 13:8 | 3f00 | 7 | 700
  LQSPI_CLK_CTRL @ 0XF800014C |  | 3f31 |  | 721

- Register : SDIO_CLK_CTRL @ 0XF8000150

  Bitfield | Bits | Mask | Value | Shifted Value
  CLKACT0 | 0:0 | 1 | 1 | 1
  CLKACT1 | 1:1 | 2 | 0 | 0
  SRCSEL | 5:4 | 30 | 0 | 0
  DIVISOR | 13:8 | 3f00 | 20 | 2000
  SDIO_CLK_CTRL @ 0XF8000150 |  | 3f33 |  | 2001

- Register : UART_CLK_CTRL @ 0XF8000154

  Bitfield | Bits | Mask | Value | Shifted Value
  CLKACT0 | 0:0 | 1 | 0 | 0
  CLKACT1 | 1:1 | 2 | 1 | 2
  SRCSEL | 5:4 | 30 | 0 | 0
  DIVISOR | 13:8 | 3f00 | 20 | 2000
  UART_CLK_CTRL @ 0XF8000154 |  | 3f33 |  | 2002

- Register : SPI_CLK_CTRL @ 0XF8000158

  Bitfield | Bits | Mask | Value | Shifted Value
  CLKACT0 | 0:0 | 1 | 0 | 0
  CLKACT1 | 1:1 | 2 | 1 | 2
  SRCSEL | 5:4 | 30 | 0 | 0
  DIVISOR | 13:8 | 3f00 | a | a00
  SPI_CLK_CTRL @ 0XF8000158 |  | 3f33 |  | a02

- Register : PCAP_CLK_CTRL @ 0XF8000168

  Bitfield | Bits | Mask | Value | Shifted Value
  CLKACT | 0:0 | 1 | 1 | 1
  SRCSEL | 5:4 | 30 | 0 | 0
  DIVISOR | 13:8 | 3f00 | 8 | 800
  PCAP_CLK_CTRL @ 0XF8000168 |  | 3f31 |  | 801

- Register : FPGA0_CLK_CTRL @ 0XF8000170

  Bitfield | Bits | Mask | Value | Shifted Value
  SRCSEL | 5:4 | 30 | 0 | 0
  DIVISOR0 | 13:8 | 3f00 | 10 | 1000
  DIVISOR1 | 25:20 | 3f00000 | 1 | 100000
  FPGA0_CLK_CTRL @ 0XF8000170 |  | 3f03f30 |  | 101000

- Register : FPGA1_CLK_CTRL @ 0XF8000180

  Bitfield | Bits | Mask | Value | Shifted Value
  SRCSEL | 5:4 | 30 | 0 | 0
  DIVISOR0 | 13:8 | 3f00 | d | d00
  DIVISOR1 | 25:20 | 3f00000 | 1 | 100000
  FPGA1_CLK_CTRL @ 0XF8000180 |  | 3f03f30 |  | 100d00

- Register : FPGA2_CLK_CTRL @ 0XF8000190

  Bitfield | Bits | Mask | Value | Shifted Value
  SRCSEL | 5:4 | 30 | 0 | 0
  DIVISOR0 | 13:8 | 3f00 | 20 | 2000
  DIVISOR1 | 25:20 | 3f00000 | 1 | 100000
  FPGA2_CLK_CTRL @ 0XF8000190 |  | 3f03f30 |  | 102000

- Register : FPGA3_CLK_CTRL @ 0XF80001A0

  Bitfield | Bits | Mask | Value | Shifted Value
  SRCSEL | 5:4 | 30 | 0 | 0
  DIVISOR0 | 13:8 | 3f00 | 20 | 2000
  DIVISOR1 | 25:20 | 3f00000 | 1 | 100000
  FPGA3_CLK_CTRL @ 0XF80001A0 |  | 3f03f30 |  | 102000

- Register : CLK_621_TRUE @ 0XF80001C4

  Bitfield | Bits | Mask | Value | Shifted Value
  CLK_621_TRUE | 0:0 | 1 | 1 | 1
  CLK_621_TRUE @ 0XF80001C4 |  | 1 |  | 1

- Register : APER_CLK_CTRL @ 0XF800012C

  Bitfield | Bits | Mask | Value | Shifted Value
  DMA_CPU_2XCLKACT | 0:0 | 1 | 1 | 1
  USB0_CPU_1XCLKACT | 2:2 | 4 | 1 | 4
  USB1_CPU_1XCLKACT | 3:3 | 8 | 1 | 8
  GEM0_CPU_1XCLKACT | 6:6 | 40 | 0 | 0
  GEM1_CPU_1XCLKACT | 7:7 | 80 | 0 | 0
  SDI0_CPU_1XCLKACT | 10:10 | 400 | 1 | 400
  SDI1_CPU_1XCLKACT | 11:11 | 800 | 0 | 0
  SPI0_CPU_1XCLKACT | 14:14 | 4000 | 0 | 0
  SPI1_CPU_1XCLKACT | 15:15 | 8000 | 1 | 8000
  CAN0_CPU_1XCLKACT | 16:16 | 10000 | 0 | 0
  CAN1_CPU_1XCLKACT | 17:17 | 20000 | 0 | 0
  I2C0_CPU_1XCLKACT | 18:18 | 40000 | 1 | 40000
  I2C1_CPU_1XCLKACT | 19:19 | 80000 | 1 | 80000
  UART0_CPU_1XCLKACT | 20:20 | 100000 | 0 | 0
  UART1_CPU_1XCLKACT | 21:21 | 200000 | 1 | 200000
  GPIO_CPU_1XCLKACT | 22:22 | 400000 | 1 | 400000
  LQSPI_CPU_1XCLKACT | 23:23 | 800000 | 1 | 800000
  SMC_CPU_1XCLKACT | 24:24 | 1000000 | 1 | 1000000
  APER_CLK_CTRL @ 0XF800012C |  | 1ffcccd |  | 1ec840d

## THIS SHOULD BE BLANK

THIS SHOULD BE BLANK

## LOCK IT BACK

LOCK IT BACK

- Register : SLCR_LOCK @ 0XF8000004

  Bitfield | Bits | Mask | Value | Shifted Value
  LOCK_KEY | 15:0 | ffff | 767b | 767b
  SLCR_LOCK @ 0XF8000004 |  | ffff |  | 767b

# ps7_ddr_init_data

## DDR INITIALIZATION

DDR INITIALIZATION

## LOCK DDR

LOCK DDR

- Register : ddrc_ctrl @ 0XF8006000

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_ddrc_soft_rstb | 0:0 | 1 | 0 | 0
  reg_ddrc_powerdown_en | 1:1 | 2 | 0 | 0
  reg_ddrc_data_bus_width | 3:2 | c | 0 | 0
  reg_ddrc_burst8_refresh | 6:4 | 70 | 0 | 0
  reg_ddrc_rdwr_idle_gap | 13:7 | 3f80 | 1 | 80
  reg_ddrc_dis_rd_bypass | 14:14 | 4000 | 0 | 0
  reg_ddrc_dis_act_bypass | 15:15 | 8000 | 0 | 0
  reg_ddrc_dis_auto_refresh | 16:16 | 10000 | 0 | 0
  ddrc_ctrl @ 0XF8006000 |  | 1ffff |  | 80

- Register : Two_rank_cfg @ 0XF8006004

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_ddrc_t_rfc_nom_x32 | 11:0 | fff | 81 | 81
  reg_ddrc_active_ranks | 13:12 | 3000 | 1 | 1000
  reg_ddrc_addrmap_cs_bit0 | 18:14 | 7c000 | 0 | 0
  reg_ddrc_wr_odt_block | 20:19 | 180000 | 1 | 80000
  reg_ddrc_diff_rank_rd_2cycle_gap | 21:21 | 200000 | 0 | 0
  reg_ddrc_addrmap_cs_bit1 | 26:22 | 7c00000 | 0 | 0
  reg_ddrc_addrmap_open_bank | 27:27 | 8000000 | 0 | 0
  reg_ddrc_addrmap_4bank_ram | 28:28 | 10000000 | 0 | 0
  Two_rank_cfg @ 0XF8006004 |  | 1fffffff |  | 81081

- Register : HPR_reg @ 0XF8006008

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_ddrc_hpr_min_non_critical_x32 | 10:0 | 7ff | f | f
  reg_ddrc_hpr_max_starve_x32 | 21:11 | 3ff800 | f | 7800
  reg_ddrc_hpr_xact_run_length | 25:22 | 3c00000 | f | 3c00000
  HPR_reg @ 0XF8006008 |  | 3ffffff |  | 3c0780f

- Register : LPR_reg @ 0XF800600C

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_ddrc_lpr_min_non_critical_x32 | 10:0 | 7ff | 1 | 1
  reg_ddrc_lpr_max_starve_x32 | 21:11 | 3ff800 | 2 | 1000
  reg_ddrc_lpr_xact_run_length | 25:22 | 3c00000 | 8 | 2000000
  LPR_reg @ 0XF800600C |  | 3ffffff |  | 2001001

- Register : WR_reg @ 0XF8006010

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_ddrc_w_min_non_critical_x32 | 10:0 | 7ff | 1 | 1
  reg_ddrc_w_xact_run_length | 14:11 | 7800 | 8 | 4000
  reg_ddrc_w_max_starve_x32 | 25:15 | 3ff8000 | 2 | 10000
  WR_reg @ 0XF8006010 |  | 3ffffff |  | 14001

- Register : DRAM_param_reg0 @ 0XF8006014

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_ddrc_t_rc | 5:0 | 3f | 1b | 1b
  reg_ddrc_t_rfc_min | 13:6 | 3fc0 | 56 | 1580
  reg_ddrc_post_selfref_gap_x32 | 20:14 | 1fc000 | 10 | 40000
  DRAM_param_reg0 @ 0XF8006014 |  | 1fffff |  | 4159b

- Register : DRAM_param_reg1 @ 0XF8006018

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_ddrc_wr2pre | 4:0 | 1f | 12 | 12
  reg_ddrc_powerdown_to_x32 | 9:5 | 3e0 | 6 | c0
  reg_ddrc_t_faw | 15:10 | fc00 | 18 | 6000
  reg_ddrc_t_ras_max | 21:16 | 3f0000 | 24 | 240000
  reg_ddrc_t_ras_min | 26:22 | 7c00000 | 14 | 5000000
  reg_ddrc_t_cke | 31:28 | f0000000 | 4 | 40000000
  DRAM_param_reg1 @ 0XF8006018 |  | f7ffffff |  | 452460d2

- Register : DRAM_param_reg2 @ 0XF800601C

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_ddrc_write_latency | 4:0 | 1f | 5 | 5
  reg_ddrc_rd2wr | 9:5 | 3e0 | 7 | e0
  reg_ddrc_wr2rd | 14:10 | 7c00 | e | 3800
  reg_ddrc_t_xp | 19:15 | f8000 | 4 | 20000
  reg_ddrc_pad_pd | 22:20 | 700000 | 0 | 0
  reg_ddrc_rd2pre | 27:23 | f800000 | 4 | 2000000
  reg_ddrc_t_rcd | 31:28 | f0000000 | 7 | 70000000
  DRAM_param_reg2 @ 0XF800601C |  | ffffffff |  | 720238e5

- Register : DRAM_param_reg3 @ 0XF8006020

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_ddrc_t_ccd | 4:2 | 1c | 4 | 10
  reg_ddrc_t_rrd | 7:5 | e0 | 6 | c0
  reg_ddrc_refresh_margin | 11:8 | f00 | 2 | 200
  reg_ddrc_t_rp | 15:12 | f000 | 7 | 7000
  reg_ddrc_refresh_to_x32 | 20:16 | 1f0000 | 8 | 80000
  reg_ddrc_sdram | 21:21 | 200000 | 1 | 200000
  reg_ddrc_mobile | 22:22 | 400000 | 0 | 0
  reg_ddrc_clock_stop_en | 23:23 | 800000 | 0 | 0
  reg_ddrc_read_latency | 28:24 | 1f000000 | 7 | 7000000
  reg_phy_mode_ddr1_ddr2 | 29:29 | 20000000 | 1 | 20000000
  reg_ddrc_dis_pad_pd | 30:30 | 40000000 | 0 | 0
  reg_ddrc_loopback | 31:31 | 80000000 | 0 | 0
  DRAM_param_reg3 @ 0XF8006020 |  | fffffffc |  | 272872d0

- Register : DRAM_param_reg4 @ 0XF8006024

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_ddrc_en_2t_timing_mode | 0:0 | 1 | 0 | 0
  reg_ddrc_prefer_write | 1:1 | 2 | 0 | 0
  reg_ddrc_max_rank_rd | 5:2 | 3c | f | 3c
  reg_ddrc_mr_wr | 6:6 | 40 | 0 | 0
  reg_ddrc_mr_addr | 8:7 | 180 | 0 | 0
  reg_ddrc_mr_data | 24:9 | 1fffe00 | 0 | 0
  ddrc_reg_mr_wr_busy | 25:25 | 2000000 | 0 | 0
  reg_ddrc_mr_type | 26:26 | 4000000 | 0 | 0
  reg_ddrc_mr_rdata_valid | 27:27 | 8000000 | 0 | 0
  DRAM_param_reg4 @ 0XF8006024 |  | fffffff |  | 3c

- Register : DRAM_init_param @ 0XF8006028

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_ddrc_final_wait_x32 | 6:0 | 7f | 7 | 7
  reg_ddrc_pre_ocd_x32 | 10:7 | 780 | 0 | 0
  reg_ddrc_t_mrd | 13:11 | 3800 | 4 | 2000
  DRAM_init_param @ 0XF8006028 |  | 3fff |  | 2007

- Register : DRAM_EMR_reg @ 0XF800602C

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_ddrc_emr2 | 15:0 | ffff | 8 | 8
  reg_ddrc_emr3 | 31:16 | ffff0000 | 0 | 0
  DRAM_EMR_reg @ 0XF800602C |  | ffffffff |  | 8

- Register : DRAM_EMR_MR_reg @ 0XF8006030

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_ddrc_mr | 15:0 | ffff | 930 | 930
  reg_ddrc_emr | 31:16 | ffff0000 | 4 | 40000
  DRAM_EMR_MR_reg @ 0XF8006030 |  | ffffffff |  | 40930

- Register : DRAM_burst8_rdwr @ 0XF8006034

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_ddrc_burst_rdwr | 3:0 | f | 4 | 4
  reg_ddrc_pre_cke_x1024 | 13:4 | 3ff0 | 1 | 10
  reg_ddrc_post_cke_x1024 | 25:16 | 3ff0000 | 1 | 10000
  reg_ddrc_burstchop | 28:28 | 10000000 | 0 | 0
  DRAM_burst8_rdwr @ 0XF8006034 |  | 13ff3fff |  | 10014

- Register : DRAM_disable_DQ @ 0XF8006038

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_ddrc_force_low_pri_n | 0:0 | 1 | 0 | 0
  reg_ddrc_dis_dq | 1:1 | 2 | 0 | 0
  reg_phy_debug_mode | 6:6 | 40 | 0 | 0
  reg_phy_wr_level_start | 7:7 | 80 | 0 | 0
  reg_phy_rd_level_start | 8:8 | 100 | 0 | 0
  reg_phy_dq0_wait_t | 12:9 | 1e00 | 0 | 0
  DRAM_disable_DQ @ 0XF8006038 |  | 1fc3 |  | 0

- Register : DRAM_addr_map_bank @ 0XF800603C

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_ddrc_addrmap_bank_b0 | 3:0 | f | 7 | 7
  reg_ddrc_addrmap_bank_b1 | 7:4 | f0 | 7 | 70
  reg_ddrc_addrmap_bank_b2 | 11:8 | f00 | 7 | 700
  reg_ddrc_addrmap_col_b5 | 15:12 | f000 | 0 | 0
  reg_ddrc_addrmap_col_b6 | 19:16 | f0000 | 0 | 0
  DRAM_addr_map_bank @ 0XF800603C |  | fffff |  | 777

- Register : DRAM_addr_map_col @ 0XF8006040

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_ddrc_addrmap_col_b2 | 3:0 | f | 0 | 0
  reg_ddrc_addrmap_col_b3 | 7:4 | f0 | 0 | 0
  reg_ddrc_addrmap_col_b4 | 11:8 | f00 | 0 | 0
  reg_ddrc_addrmap_col_b7 | 15:12 | f000 | 0 | 0
  reg_ddrc_addrmap_col_b8 | 19:16 | f0000 | 0 | 0
  reg_ddrc_addrmap_col_b9 | 23:20 | f00000 | f | f00000
  reg_ddrc_addrmap_col_b10 | 27:24 | f000000 | f | f000000
  reg_ddrc_addrmap_col_b11 | 31:28 | f0000000 | f | f0000000
  DRAM_addr_map_col @ 0XF8006040 |  | ffffffff |  | fff00000

- Register : DRAM_addr_map_row @ 0XF8006044

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_ddrc_addrmap_row_b0 | 3:0 | f | 6 | 6
  reg_ddrc_addrmap_row_b1 | 7:4 | f0 | 6 | 60
  reg_ddrc_addrmap_row_b2_11 | 11:8 | f00 | 6 | 600
  reg_ddrc_addrmap_row_b12 | 15:12 | f000 | 6 | 6000
  reg_ddrc_addrmap_row_b13 | 19:16 | f0000 | 6 | 60000
  reg_ddrc_addrmap_row_b14 | 23:20 | f00000 | f | f00000
  reg_ddrc_addrmap_row_b15 | 27:24 | f000000 | f | f000000
  DRAM_addr_map_row @ 0XF8006044 |  | fffffff |  | ff66666

- Register : DRAM_ODT_reg @ 0XF8006048

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_ddrc_rank0_rd_odt | 2:0 | 7 | 0 | 0
  reg_ddrc_rank0_wr_odt | 5:3 | 38 | 1 | 8
  reg_ddrc_rank1_rd_odt | 8:6 | 1c0 | 1 | 40
  reg_ddrc_rank1_wr_odt | 11:9 | e00 | 1 | 200
  reg_phy_rd_local_odt | 13:12 | 3000 | 0 | 0
  reg_phy_wr_local_odt | 15:14 | c000 | 3 | c000
  reg_phy_idle_local_odt | 17:16 | 30000 | 3 | 30000
  reg_ddrc_rank2_rd_odt | 20:18 | 1c0000 | 0 | 0
  reg_ddrc_rank2_wr_odt | 23:21 | e00000 | 0 | 0
  reg_ddrc_rank3_rd_odt | 26:24 | 7000000 | 0 | 0
  reg_ddrc_rank3_wr_odt | 29:27 | 38000000 | 0 | 0
  DRAM_ODT_reg @ 0XF8006048 |  | 3fffffff |  | 3c248

- Register : phy_cmd_timeout_rddata_cpt @ 0XF8006050

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_phy_rd_cmd_to_data | 3:0 | f | 0 | 0
  reg_phy_wr_cmd_to_data | 7:4 | f0 | 0 | 0
  reg_phy_rdc_we_to_re_delay | 11:8 | f00 | 8 | 800
  reg_phy_rdc_fifo_rst_disable | 15:15 | 8000 | 0 | 0
  reg_phy_use_fixed_re | 16:16 | 10000 | 1 | 10000
  reg_phy_rdc_fifo_rst_err_cnt_clr | 17:17 | 20000 | 0 | 0
  reg_phy_dis_phy_ctrl_rstn | 18:18 | 40000 | 0 | 0
  reg_phy_clk_stall_level | 19:19 | 80000 | 0 | 0
  reg_phy_gatelvl_num_of_dq0 | 27:24 | f000000 | 7 | 7000000
  reg_phy_wrlvl_num_of_dq0 | 31:28 | f0000000 | 7 | 70000000
  phy_cmd_timeout_rddata_cpt @ 0XF8006050 |  | ff0f8fff |  | 77010800

- Register : DLL_calib @ 0XF8006058

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_ddrc_dll_calib_to_min_x1024 | 7:0 | ff | 1 | 1
  reg_ddrc_dll_calib_to_max_x1024 | 15:8 | ff00 | 1 | 100
  reg_ddrc_dis_dll_calib | 16:16 | 10000 | 0 | 0
  DLL_calib @ 0XF8006058 |  | 1ffff |  | 101

- Register : ODT_delay_hold @ 0XF800605C

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_ddrc_rd_odt_delay | 3:0 | f | 3 | 3
  reg_ddrc_wr_odt_delay | 7:4 | f0 | 0 | 0
  reg_ddrc_rd_odt_hold | 11:8 | f00 | 0 | 0
  reg_ddrc_wr_odt_hold | 15:12 | f000 | 5 | 5000
  ODT_delay_hold @ 0XF800605C |  | ffff |  | 5003

- Register : ctrl_reg1 @ 0XF8006060

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_ddrc_pageclose | 0:0 | 1 | 0 | 0
  reg_ddrc_lpr_num_entries | 6:1 | 7e | 1f | 3e
  reg_ddrc_auto_pre_en | 7:7 | 80 | 0 | 0
  reg_ddrc_refresh_update_level | 8:8 | 100 | 0 | 0
  reg_ddrc_dis_wc | 9:9 | 200 | 0 | 0
  reg_ddrc_dis_collision_page_opt | 10:10 | 400 | 0 | 0
  reg_ddrc_selfref_en | 12:12 | 1000 | 0 | 0
  ctrl_reg1 @ 0XF8006060 |  | 17ff |  | 3e

- Register : ctrl_reg2 @ 0XF8006064

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_ddrc_go2critical_hysteresis | 12:5 | 1fe0 | 0 | 0
  reg_arb_go2critical_en | 17:17 | 20000 | 1 | 20000
  ctrl_reg2 @ 0XF8006064 |  | 21fe0 |  | 20000

- Register : ctrl_reg3 @ 0XF8006068

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_ddrc_wrlvl_ww | 7:0 | ff | 41 | 41
  reg_ddrc_rdlvl_rr | 15:8 | ff00 | 41 | 4100
  reg_ddrc_dfi_t_wlmrd | 25:16 | 3ff0000 | 28 | 280000
  ctrl_reg3 @ 0XF8006068 |  | 3ffffff |  | 284141

- Register : ctrl_reg4 @ 0XF800606C

  Bitfield | Bits | Mask | Value | Shifted Value
  dfi_t_ctrlupd_interval_min_x1024 | 7:0 | ff | 10 | 10
  dfi_t_ctrlupd_interval_max_x1024 | 15:8 | ff00 | 16 | 1600
  ctrl_reg4 @ 0XF800606C |  | ffff |  | 1610

- Register : CHE_REFRESH_TIMER01 @ 0XF80060A0

  Bitfield | Bits | Mask | Value | Shifted Value
  refresh_timer0_start_value_x32 | 11:0 | fff | 0 | 0
  refresh_timer1_start_value_x32 | 23:12 | fff000 | 8 | 8000
  CHE_REFRESH_TIMER01 @ 0XF80060A0 |  | ffffff |  | 8000

- Register : CHE_T_ZQ @ 0XF80060A4

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_ddrc_dis_auto_zq | 0:0 | 1 | 0 | 0
  reg_ddrc_ddr3 | 1:1 | 2 | 1 | 2
  reg_ddrc_t_mod | 11:2 | ffc | 200 | 800
  reg_ddrc_t_zq_long_nop | 21:12 | 3ff000 | 200 | 200000
  reg_ddrc_t_zq_short_nop | 31:22 | ffc00000 | 40 | 10000000
  CHE_T_ZQ @ 0XF80060A4 |  | ffffffff |  | 10200802

- Register : CHE_T_ZQ_Short_Interval_Reg @ 0XF80060A8

  Bitfield | Bits | Mask | Value | Shifted Value
  t_zq_short_interval_x1024 | 19:0 | fffff | cb73 | cb73
  dram_rstn_x1024 | 27:20 | ff00000 | 2 | 200000
  CHE_T_ZQ_Short_Interval_Reg @ 0XF80060A8 |  | fffffff |  | 20cb73

- Register : deep_pwrdwn_reg @ 0XF80060AC

  Bitfield | Bits | Mask | Value | Shifted Value
  deeppowerdown_en | 0:0 | 1 | 0 | 0
  deeppowerdown_to_x1024 | 8:1 | 1fe | ff | 1fe
  deep_pwrdwn_reg @ 0XF80060AC |  | 1ff |  | 1fe

- Register : reg_2c @ 0XF80060B0

  Bitfield | Bits | Mask | Value | Shifted Value
  dfi_wrlvl_max_x1024 | 11:0 | fff | fff | fff
  dfi_rdlvl_max_x1024 | 23:12 | fff000 | fff | fff000
  ddrc_reg_twrlvl_max_error | 24:24 | 1000000 | 0 | 0
  ddrc_reg_trdlvl_max_error | 25:25 | 2000000 | 0 | 0
  reg_ddrc_dfi_wr_level_en | 26:26 | 4000000 | 1 | 4000000
  reg_ddrc_dfi_rd_dqs_gate_level | 27:27 | 8000000 | 1 | 8000000
  reg_ddrc_dfi_rd_data_eye_train | 28:28 | 10000000 | 1 | 10000000
  reg_2c @ 0XF80060B0 |  | 1fffffff |  | 1cffffff

- Register : reg_2d @ 0XF80060B4

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_ddrc_2t_delay | 8:0 | 1ff | 0 | 0
  reg_ddrc_skip_ocd | 9:9 | 200 | 1 | 200
  reg_ddrc_dis_pre_bypass | 10:10 | 400 | 0 | 0
  reg_2d @ 0XF80060B4 |  | 7ff |  | 200

- Register : dfi_timing @ 0XF80060B8

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_ddrc_dfi_t_rddata_en | 4:0 | 1f | 6 | 6
  reg_ddrc_dfi_t_ctrlup_min | 14:5 | 7fe0 | 3 | 60
  reg_ddrc_dfi_t_ctrlup_max | 24:15 | 1ff8000 | 40 | 200000
  dfi_timing @ 0XF80060B8 |  | 1ffffff |  | 200066

- Register : refresh_timer_2 @ 0XF80060BC

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_ddrc_refresh_timer2_start_value_x32 | 11:0 | fff | 0 | 0
  reg_ddrc_refresh_timer3_start_value_x32 | 23:12 | fff000 | 0 | 0
  refresh_timer_2 @ 0XF80060BC |  | ffffff |  | 0

- Register : CHE_ECC_CONTROL_REG_OFFSET @ 0XF80060C4

  Bitfield | Bits | Mask | Value | Shifted Value
  Clear_Uncorrectable_DRAM_ECC_error | 0:0 | 1 | 0 | 0
  Clear_Correctable_DRAM_ECC_error | 1:1 | 2 | 0 | 0
  CHE_ECC_CONTROL_REG_OFFSET @ 0XF80060C4 |  | 3 |  | 0

- Register : CHE_CORR_ECC_LOG_REG_OFFSET @ 0XF80060C8

  Bitfield | Bits | Mask | Value | Shifted Value
  CORR_ECC_LOG_VALID | 0:0 | 1 | 0 | 0
  ECC_CORRECTED_BIT_NUM | 7:1 | fe | 0 | 0
  CHE_CORR_ECC_LOG_REG_OFFSET @ 0XF80060C8 |  | ff |  | 0

- Register : CHE_UNCORR_ECC_LOG_REG_OFFSET @ 0XF80060DC

  Bitfield | Bits | Mask | Value | Shifted Value
  UNCORR_ECC_LOG_VALID | 0:0 | 1 | 0 | 0
  CHE_UNCORR_ECC_LOG_REG_OFFSET @ 0XF80060DC |  | 1 |  | 0

- Register : CHE_ECC_STATS_REG_OFFSET @ 0XF80060F0

  Bitfield | Bits | Mask | Value | Shifted Value
  STAT_NUM_CORR_ERR | 15:8 | ff00 | 0 | 0
  STAT_NUM_UNCORR_ERR | 7:0 | ff | 0 | 0
  CHE_ECC_STATS_REG_OFFSET @ 0XF80060F0 |  | ffff |  | 0

- Register : ECC_scrub @ 0XF80060F4

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_ddrc_ecc_mode | 2:0 | 7 | 0 | 0
  reg_ddrc_dis_scrub | 3:3 | 8 | 1 | 8
  ECC_scrub @ 0XF80060F4 |  | f |  | 8

- Register : phy_rcvr_enable @ 0XF8006114

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_phy_dif_on | 3:0 | f | 0 | 0
  reg_phy_dif_off | 7:4 | f0 | 0 | 0
  phy_rcvr_enable @ 0XF8006114 |  | ff |  | 0

- Register : PHY_Config0 @ 0XF8006118

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_phy_data_slice_in_use | 0:0 | 1 | 1 | 1
  reg_phy_rdlvl_inc_mode | 1:1 | 2 | 0 | 0
  reg_phy_gatelvl_inc_mode | 2:2 | 4 | 0 | 0
  reg_phy_wrlvl_inc_mode | 3:3 | 8 | 0 | 0
  reg_phy_board_lpbk_tx | 4:4 | 10 | 0 | 0
  reg_phy_board_lpbk_rx | 5:5 | 20 | 0 | 0
  reg_phy_bist_shift_dq | 14:6 | 7fc0 | 0 | 0
  reg_phy_bist_err_clr | 23:15 | ff8000 | 0 | 0
  reg_phy_dq_offset | 30:24 | 7f000000 | 40 | 40000000
  PHY_Config0 @ 0XF8006118 |  | 7fffffff |  | 40000001

- Register : PHY_Config1 @ 0XF800611C

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_phy_data_slice_in_use | 0:0 | 1 | 1 | 1
  reg_phy_rdlvl_inc_mode | 1:1 | 2 | 0 | 0
  reg_phy_gatelvl_inc_mode | 2:2 | 4 | 0 | 0
  reg_phy_wrlvl_inc_mode | 3:3 | 8 | 0 | 0
  reg_phy_board_lpbk_tx | 4:4 | 10 | 0 | 0
  reg_phy_board_lpbk_rx | 5:5 | 20 | 0 | 0
  reg_phy_bist_shift_dq | 14:6 | 7fc0 | 0 | 0
  reg_phy_bist_err_clr | 23:15 | ff8000 | 0 | 0
  reg_phy_dq_offset | 30:24 | 7f000000 | 40 | 40000000
  PHY_Config1 @ 0XF800611C |  | 7fffffff |  | 40000001

- Register : PHY_Config2 @ 0XF8006120

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_phy_data_slice_in_use | 0:0 | 1 | 1 | 1
  reg_phy_rdlvl_inc_mode | 1:1 | 2 | 0 | 0
  reg_phy_gatelvl_inc_mode | 2:2 | 4 | 0 | 0
  reg_phy_wrlvl_inc_mode | 3:3 | 8 | 0 | 0
  reg_phy_board_lpbk_tx | 4:4 | 10 | 0 | 0
  reg_phy_board_lpbk_rx | 5:5 | 20 | 0 | 0
  reg_phy_bist_shift_dq | 14:6 | 7fc0 | 0 | 0
  reg_phy_bist_err_clr | 23:15 | ff8000 | 0 | 0
  reg_phy_dq_offset | 30:24 | 7f000000 | 40 | 40000000
  reg_phy_data_slice_in_use | 0:0 | 1 | 1 | 1
  reg_phy_rdlvl_inc_mode | 1:1 | 2 | 0 | 0
  reg_phy_gatelvl_inc_mode | 2:2 | 4 | 0 | 0
  reg_phy_wrlvl_inc_mode | 3:3 | 8 | 0 | 0
  reg_phy_board_lpbk_tx | 4:4 | 10 | 0 | 0
  reg_phy_board_lpbk_rx | 5:5 | 20 | 0 | 0
  reg_phy_bist_shift_dq | 14:6 | 7fc0 | 0 | 0
  reg_phy_bist_err_clr | 23:15 | ff8000 | 0 | 0
  reg_phy_dq_offset | 30:24 | 7f000000 | 40 | 40000000
  PHY_Config2 @ 0XF8006120 |  | 7fffffff |  | 40000001

- Register : PHY_Config3 @ 0XF8006124

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_phy_data_slice_in_use | 0:0 | 1 | 1 | 1
  reg_phy_rdlvl_inc_mode | 1:1 | 2 | 0 | 0
  reg_phy_gatelvl_inc_mode | 2:2 | 4 | 0 | 0
  reg_phy_wrlvl_inc_mode | 3:3 | 8 | 0 | 0
  reg_phy_board_lpbk_tx | 4:4 | 10 | 0 | 0
  reg_phy_board_lpbk_rx | 5:5 | 20 | 0 | 0
  reg_phy_bist_shift_dq | 14:6 | 7fc0 | 0 | 0
  reg_phy_bist_err_clr | 23:15 | ff8000 | 0 | 0
  reg_phy_dq_offset | 30:24 | 7f000000 | 40 | 40000000
  PHY_Config3 @ 0XF8006124 |  | 7fffffff |  | 40000001

- Register : phy_init_ratio0 @ 0XF800612C

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_phy_wrlvl_init_ratio | 9:0 | 3ff | 3 | 3
  reg_phy_gatelvl_init_ratio | 19:10 | ffc00 | cf | 33c00
  phy_init_ratio0 @ 0XF800612C |  | fffff |  | 33c03

- Register : phy_init_ratio1 @ 0XF8006130

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_phy_wrlvl_init_ratio | 9:0 | 3ff | 3 | 3
  reg_phy_gatelvl_init_ratio | 19:10 | ffc00 | d0 | 34000
  phy_init_ratio1 @ 0XF8006130 |  | fffff |  | 34003

- Register : phy_init_ratio2 @ 0XF8006134

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_phy_wrlvl_init_ratio | 9:0 | 3ff | 0 | 0
  reg_phy_gatelvl_init_ratio | 19:10 | ffc00 | bd | 2f400
  phy_init_ratio2 @ 0XF8006134 |  | fffff |  | 2f400

- Register : phy_init_ratio3 @ 0XF8006138

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_phy_wrlvl_init_ratio | 9:0 | 3ff | 0 | 0
  reg_phy_gatelvl_init_ratio | 19:10 | ffc00 | c1 | 30400
  phy_init_ratio3 @ 0XF8006138 |  | fffff |  | 30400

- Register : phy_rd_dqs_cfg0 @ 0XF8006140

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_phy_rd_dqs_slave_ratio | 9:0 | 3ff | 35 | 35
  reg_phy_rd_dqs_slave_force | 10:10 | 400 | 0 | 0
  reg_phy_rd_dqs_slave_delay | 19:11 | ff800 | 0 | 0
  phy_rd_dqs_cfg0 @ 0XF8006140 |  | fffff |  | 35

- Register : phy_rd_dqs_cfg1 @ 0XF8006144

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_phy_rd_dqs_slave_ratio | 9:0 | 3ff | 35 | 35
  reg_phy_rd_dqs_slave_force | 10:10 | 400 | 0 | 0
  reg_phy_rd_dqs_slave_delay | 19:11 | ff800 | 0 | 0
  phy_rd_dqs_cfg1 @ 0XF8006144 |  | fffff |  | 35

- Register : phy_rd_dqs_cfg2 @ 0XF8006148

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_phy_rd_dqs_slave_ratio | 9:0 | 3ff | 35 | 35
  reg_phy_rd_dqs_slave_force | 10:10 | 400 | 0 | 0
  reg_phy_rd_dqs_slave_delay | 19:11 | ff800 | 0 | 0
  phy_rd_dqs_cfg2 @ 0XF8006148 |  | fffff |  | 35

- Register : phy_rd_dqs_cfg3 @ 0XF800614C

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_phy_rd_dqs_slave_ratio | 9:0 | 3ff | 35 | 35
  reg_phy_rd_dqs_slave_force | 10:10 | 400 | 0 | 0
  reg_phy_rd_dqs_slave_delay | 19:11 | ff800 | 0 | 0
  phy_rd_dqs_cfg3 @ 0XF800614C |  | fffff |  | 35

- Register : phy_wr_dqs_cfg0 @ 0XF8006154

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_phy_wr_dqs_slave_ratio | 9:0 | 3ff | 83 | 83
  reg_phy_wr_dqs_slave_force | 10:10 | 400 | 0 | 0
  reg_phy_wr_dqs_slave_delay | 19:11 | ff800 | 0 | 0
  phy_wr_dqs_cfg0 @ 0XF8006154 |  | fffff |  | 83

- Register : phy_wr_dqs_cfg1 @ 0XF8006158

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_phy_wr_dqs_slave_ratio | 9:0 | 3ff | 83 | 83
  reg_phy_wr_dqs_slave_force | 10:10 | 400 | 0 | 0
  reg_phy_wr_dqs_slave_delay | 19:11 | ff800 | 0 | 0
  phy_wr_dqs_cfg1 @ 0XF8006158 |  | fffff |  | 83

- Register : phy_wr_dqs_cfg2 @ 0XF800615C

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_phy_wr_dqs_slave_ratio | 9:0 | 3ff | 7f | 7f
  reg_phy_wr_dqs_slave_force | 10:10 | 400 | 0 | 0
  reg_phy_wr_dqs_slave_delay | 19:11 | ff800 | 0 | 0
  phy_wr_dqs_cfg2 @ 0XF800615C |  | fffff |  | 7f

- Register : phy_wr_dqs_cfg3 @ 0XF8006160

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_phy_wr_dqs_slave_ratio | 9:0 | 3ff | 78 | 78
  reg_phy_wr_dqs_slave_force | 10:10 | 400 | 0 | 0
  reg_phy_wr_dqs_slave_delay | 19:11 | ff800 | 0 | 0
  phy_wr_dqs_cfg3 @ 0XF8006160 |  | fffff |  | 78

- Register : phy_we_cfg0 @ 0XF8006168

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_phy_fifo_we_slave_ratio | 10:0 | 7ff | 124 | 124
  reg_phy_fifo_we_in_force | 11:11 | 800 | 0 | 0
  reg_phy_fifo_we_in_delay | 20:12 | 1ff000 | 0 | 0
  phy_we_cfg0 @ 0XF8006168 |  | 1fffff |  | 124

- Register : phy_we_cfg1 @ 0XF800616C

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_phy_fifo_we_slave_ratio | 10:0 | 7ff | 125 | 125
  reg_phy_fifo_we_in_force | 11:11 | 800 | 0 | 0
  reg_phy_fifo_we_in_delay | 20:12 | 1ff000 | 0 | 0
  phy_we_cfg1 @ 0XF800616C |  | 1fffff |  | 125

- Register : phy_we_cfg2 @ 0XF8006170

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_phy_fifo_we_slave_ratio | 10:0 | 7ff | 112 | 112
  reg_phy_fifo_we_in_force | 11:11 | 800 | 0 | 0
  reg_phy_fifo_we_in_delay | 20:12 | 1ff000 | 0 | 0
  phy_we_cfg2 @ 0XF8006170 |  | 1fffff |  | 112

- Register : phy_we_cfg3 @ 0XF8006174

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_phy_fifo_we_slave_ratio | 10:0 | 7ff | 116 | 116
  reg_phy_fifo_we_in_force | 11:11 | 800 | 0 | 0
  reg_phy_fifo_we_in_delay | 20:12 | 1ff000 | 0 | 0
  phy_we_cfg3 @ 0XF8006174 |  | 1fffff |  | 116

- Register : wr_data_slv0 @ 0XF800617C

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_phy_wr_data_slave_ratio | 9:0 | 3ff | c3 | c3
  reg_phy_wr_data_slave_force | 10:10 | 400 | 0 | 0
  reg_phy_wr_data_slave_delay | 19:11 | ff800 | 0 | 0
  wr_data_slv0 @ 0XF800617C |  | fffff |  | c3

- Register : wr_data_slv1 @ 0XF8006180

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_phy_wr_data_slave_ratio | 9:0 | 3ff | c3 | c3
  reg_phy_wr_data_slave_force | 10:10 | 400 | 0 | 0
  reg_phy_wr_data_slave_delay | 19:11 | ff800 | 0 | 0
  wr_data_slv1 @ 0XF8006180 |  | fffff |  | c3

- Register : wr_data_slv2 @ 0XF8006184

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_phy_wr_data_slave_ratio | 9:0 | 3ff | bf | bf
  reg_phy_wr_data_slave_force | 10:10 | 400 | 0 | 0
  reg_phy_wr_data_slave_delay | 19:11 | ff800 | 0 | 0
  wr_data_slv2 @ 0XF8006184 |  | fffff |  | bf

- Register : wr_data_slv3 @ 0XF8006188

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_phy_wr_data_slave_ratio | 9:0 | 3ff | b8 | b8
  reg_phy_wr_data_slave_force | 10:10 | 400 | 0 | 0
  reg_phy_wr_data_slave_delay | 19:11 | ff800 | 0 | 0
  wr_data_slv3 @ 0XF8006188 |  | fffff |  | b8

- Register : reg_64 @ 0XF8006190

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_phy_loopback | 0:0 | 1 | 0 | 0
  reg_phy_bl2 | 1:1 | 2 | 0 | 0
  reg_phy_at_spd_atpg | 2:2 | 4 | 0 | 0
  reg_phy_bist_enable | 3:3 | 8 | 0 | 0
  reg_phy_bist_force_err | 4:4 | 10 | 0 | 0
  reg_phy_bist_mode | 6:5 | 60 | 0 | 0
  reg_phy_invert_clkout | 7:7 | 80 | 1 | 80
  reg_phy_all_dq_mpr_rd_resp | 8:8 | 100 | 0 | 0
  reg_phy_sel_logic | 9:9 | 200 | 0 | 0
  reg_phy_ctrl_slave_ratio | 19:10 | ffc00 | 100 | 40000
  reg_phy_ctrl_slave_force | 20:20 | 100000 | 0 | 0
  reg_phy_ctrl_slave_delay | 27:21 | fe00000 | 0 | 0
  reg_phy_use_rank0_delays | 28:28 | 10000000 | 1 | 10000000
  reg_phy_lpddr | 29:29 | 20000000 | 0 | 0
  reg_phy_cmd_latency | 30:30 | 40000000 | 0 | 0
  reg_phy_int_lpbk | 31:31 | 80000000 | 0 | 0
  reg_64 @ 0XF8006190 |  | ffffffff |  | 10040080

- Register : reg_65 @ 0XF8006194

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_phy_wr_rl_delay | 4:0 | 1f | 2 | 2
  reg_phy_rd_rl_delay | 9:5 | 3e0 | 4 | 80
  reg_phy_dll_lock_diff | 13:10 | 3c00 | f | 3c00
  reg_phy_use_wr_level | 14:14 | 4000 | 1 | 4000
  reg_phy_use_rd_dqs_gate_level | 15:15 | 8000 | 1 | 8000
  reg_phy_use_rd_data_eye_level | 16:16 | 10000 | 1 | 10000
  reg_phy_dis_calib_rst | 17:17 | 20000 | 0 | 0
  reg_phy_ctrl_slave_delay | 19:18 | c0000 | 0 | 0
  reg_65 @ 0XF8006194 |  | fffff |  | 1fc82

- Register : page_mask @ 0XF8006204

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_arb_page_addr_mask | 31:0 | 0 | 0 | 0
  page_mask @ 0XF8006204 |  | 0 |  | 0

- Register : axi_priority_wr_port0 @ 0XF8006208

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_arb_pri_wr_portn | 9:0 | 3ff | 3ff | 3ff
  reg_arb_disable_aging_wr_portn | 16:16 | 10000 | 0 | 0
  reg_arb_disable_urgent_wr_portn | 17:17 | 20000 | 0 | 0
  reg_arb_dis_page_match_wr_portn | 18:18 | 40000 | 0 | 0
  reg_arb_dis_rmw_portn | 19:19 | 80000 | 1 | 80000
  axi_priority_wr_port0 @ 0XF8006208 |  | f03ff |  | 803ff

- Register : axi_priority_wr_port1 @ 0XF800620C

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_arb_pri_wr_portn | 9:0 | 3ff | 3ff | 3ff
  reg_arb_disable_aging_wr_portn | 16:16 | 10000 | 0 | 0
  reg_arb_disable_urgent_wr_portn | 17:17 | 20000 | 0 | 0
  reg_arb_dis_page_match_wr_portn | 18:18 | 40000 | 0 | 0
  reg_arb_dis_rmw_portn | 19:19 | 80000 | 1 | 80000
  axi_priority_wr_port1 @ 0XF800620C |  | f03ff |  | 803ff

- Register : axi_priority_wr_port2 @ 0XF8006210

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_arb_pri_wr_portn | 9:0 | 3ff | 3ff | 3ff
  reg_arb_disable_aging_wr_portn | 16:16 | 10000 | 0 | 0
  reg_arb_disable_urgent_wr_portn | 17:17 | 20000 | 0 | 0
  reg_arb_dis_page_match_wr_portn | 18:18 | 40000 | 0 | 0
  reg_arb_dis_rmw_portn | 19:19 | 80000 | 1 | 80000
  axi_priority_wr_port2 @ 0XF8006210 |  | f03ff |  | 803ff

- Register : axi_priority_wr_port3 @ 0XF8006214

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_arb_pri_wr_portn | 9:0 | 3ff | 3ff | 3ff
  reg_arb_disable_aging_wr_portn | 16:16 | 10000 | 0 | 0
  reg_arb_disable_urgent_wr_portn | 17:17 | 20000 | 0 | 0
  reg_arb_dis_page_match_wr_portn | 18:18 | 40000 | 0 | 0
  reg_arb_dis_rmw_portn | 19:19 | 80000 | 1 | 80000
  axi_priority_wr_port3 @ 0XF8006214 |  | f03ff |  | 803ff

- Register : axi_priority_rd_port0 @ 0XF8006218

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_arb_pri_rd_portn | 9:0 | 3ff | 3ff | 3ff
  reg_arb_disable_aging_rd_portn | 16:16 | 10000 | 0 | 0
  reg_arb_disable_urgent_rd_portn | 17:17 | 20000 | 0 | 0
  reg_arb_dis_page_match_rd_portn | 18:18 | 40000 | 0 | 0
  reg_arb_set_hpr_rd_portn | 19:19 | 80000 | 0 | 0
  axi_priority_rd_port0 @ 0XF8006218 |  | f03ff |  | 3ff

- Register : axi_priority_rd_port1 @ 0XF800621C

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_arb_pri_rd_portn | 9:0 | 3ff | 3ff | 3ff
  reg_arb_disable_aging_rd_portn | 16:16 | 10000 | 0 | 0
  reg_arb_disable_urgent_rd_portn | 17:17 | 20000 | 0 | 0
  reg_arb_dis_page_match_rd_portn | 18:18 | 40000 | 0 | 0
  reg_arb_set_hpr_rd_portn | 19:19 | 80000 | 0 | 0
  axi_priority_rd_port1 @ 0XF800621C |  | f03ff |  | 3ff

- Register : axi_priority_rd_port2 @ 0XF8006220

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_arb_pri_rd_portn | 9:0 | 3ff | 3ff | 3ff
  reg_arb_disable_aging_rd_portn | 16:16 | 10000 | 0 | 0
  reg_arb_disable_urgent_rd_portn | 17:17 | 20000 | 0 | 0
  reg_arb_dis_page_match_rd_portn | 18:18 | 40000 | 0 | 0
  reg_arb_set_hpr_rd_portn | 19:19 | 80000 | 0 | 0
  axi_priority_rd_port2 @ 0XF8006220 |  | f03ff |  | 3ff

- Register : axi_priority_rd_port3 @ 0XF8006224

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_arb_pri_rd_portn | 9:0 | 3ff | 3ff | 3ff
  reg_arb_disable_aging_rd_portn | 16:16 | 10000 | 0 | 0
  reg_arb_disable_urgent_rd_portn | 17:17 | 20000 | 0 | 0
  reg_arb_dis_page_match_rd_portn | 18:18 | 40000 | 0 | 0
  reg_arb_set_hpr_rd_portn | 19:19 | 80000 | 0 | 0
  axi_priority_rd_port3 @ 0XF8006224 |  | f03ff |  | 3ff

- Register : lpddr_ctrl0 @ 0XF80062A8

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_ddrc_lpddr2 | 0:0 | 1 | 0 | 0
  reg_ddrc_per_bank_refresh | 1:1 | 2 | 0 | 0
  reg_ddrc_derate_enable | 2:2 | 4 | 0 | 0
  reg_ddrc_mr4_margin | 11:4 | ff0 | 0 | 0
  lpddr_ctrl0 @ 0XF80062A8 |  | ff7 |  | 0

- Register : lpddr_ctrl1 @ 0XF80062AC

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_ddrc_mr4_read_interval | 31:0 | 0 | 0 | 0
  lpddr_ctrl1 @ 0XF80062AC |  | 0 |  | 0

- Register : lpddr_ctrl2 @ 0XF80062B0

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_ddrc_min_stable_clock_x1 | 3:0 | f | 5 | 5
  reg_ddrc_idle_after_reset_x32 | 11:4 | ff0 | 12 | 120
  reg_ddrc_t_mrw | 21:12 | 3ff000 | 5 | 5000
  lpddr_ctrl2 @ 0XF80062B0 |  | 3fffff |  | 5125

- Register : lpddr_ctrl3 @ 0XF80062B4

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_ddrc_max_auto_init_x1024 | 7:0 | ff | a8 | a8
  reg_ddrc_dev_zqinit_x32 | 17:8 | 3ff00 | 12 | 1200
  lpddr_ctrl3 @ 0XF80062B4 |  | 3ffff |  | 12a8

## UNLOCK DDR

UNLOCK DDR

- Register : ddrc_ctrl @ 0XF8006000

  Bitfield | Bits | Mask | Value | Shifted Value
  reg_ddrc_soft_rstb | 0:0 | 1 | 1 | 1
  reg_ddrc_powerdown_en | 1:1 | 2 | 0 | 0
  reg_ddrc_data_bus_width | 3:2 | c | 0 | 0
  reg_ddrc_burst8_refresh | 6:4 | 70 | 0 | 0
  reg_ddrc_rdwr_idle_gap | 13:7 | 3f80 | 1 | 80
  reg_ddrc_dis_rd_bypass | 14:14 | 4000 | 0 | 0
  reg_ddrc_dis_act_bypass | 15:15 | 8000 | 0 | 0
  reg_ddrc_dis_auto_refresh | 16:16 | 10000 | 0 | 0
  ddrc_ctrl @ 0XF8006000 |  | 1ffff |  | 81

# ps7_mio_init_data

## SLCR SETTINGS

SLCR SETTINGS

- Register : SLCR_UNLOCK @ 0XF8000008

  Bitfield | Bits | Mask | Value | Shifted Value
  UNLOCK_KEY | 15:0 | ffff | df0d | df0d
  SLCR_UNLOCK @ 0XF8000008 |  | ffff |  | df0d

## OCM REMAPPING

OCM REMAPPING

## DDRIOB SETTINGS

DDRIOB SETTINGS

- Register : DDRIOB_ADDR0 @ 0XF8000B40

  Bitfield | Bits | Mask | Value | Shifted Value
  INP_POWER | 0:0 | 1 | 0 | 0
  INP_TYPE | 2:1 | 6 | 0 | 0
  DCI_UPDATE | 3:3 | 8 | 0 | 0
  TERM_EN | 4:4 | 10 | 0 | 0
  DCR_TYPE | 6:5 | 60 | 0 | 0
  IBUF_DISABLE_MODE | 7:7 | 80 | 0 | 0
  TERM_DISABLE_MODE | 8:8 | 100 | 0 | 0
  OUTPUT_EN | 10:9 | 600 | 3 | 600
  PULLUP_EN | 11:11 | 800 | 0 | 0
  DDRIOB_ADDR0 @ 0XF8000B40 |  | fff |  | 600

- Register : DDRIOB_ADDR1 @ 0XF8000B44

  Bitfield | Bits | Mask | Value | Shifted Value
  INP_POWER | 0:0 | 1 | 0 | 0
  INP_TYPE | 2:1 | 6 | 0 | 0
  DCI_UPDATE | 3:3 | 8 | 0 | 0
  TERM_EN | 4:4 | 10 | 0 | 0
  DCR_TYPE | 6:5 | 60 | 0 | 0
  IBUF_DISABLE_MODE | 7:7 | 80 | 0 | 0
  TERM_DISABLE_MODE | 8:8 | 100 | 0 | 0
  OUTPUT_EN | 10:9 | 600 | 3 | 600
  PULLUP_EN | 11:11 | 800 | 0 | 0
  DDRIOB_ADDR1 @ 0XF8000B44 |  | fff |  | 600

- Register : DDRIOB_DATA0 @ 0XF8000B48

  Bitfield | Bits | Mask | Value | Shifted Value
  INP_POWER | 0:0 | 1 | 0 | 0
  INP_TYPE | 2:1 | 6 | 1 | 2
  DCI_UPDATE | 3:3 | 8 | 0 | 0
  TERM_EN | 4:4 | 10 | 1 | 10
  DCR_TYPE | 6:5 | 60 | 3 | 60
  IBUF_DISABLE_MODE | 7:7 | 80 | 0 | 0
  TERM_DISABLE_MODE | 8:8 | 100 | 0 | 0
  OUTPUT_EN | 10:9 | 600 | 3 | 600
  PULLUP_EN | 11:11 | 800 | 0 | 0
  DDRIOB_DATA0 @ 0XF8000B48 |  | fff |  | 672

- Register : DDRIOB_DATA1 @ 0XF8000B4C

  Bitfield | Bits | Mask | Value | Shifted Value
  INP_POWER | 0:0 | 1 | 0 | 0
  INP_TYPE | 2:1 | 6 | 1 | 2
  DCI_UPDATE | 3:3 | 8 | 0 | 0
  TERM_EN | 4:4 | 10 | 1 | 10
  DCR_TYPE | 6:5 | 60 | 3 | 60
  IBUF_DISABLE_MODE | 7:7 | 80 | 0 | 0
  TERM_DISABLE_MODE | 8:8 | 100 | 0 | 0
  OUTPUT_EN | 10:9 | 600 | 3 | 600
  PULLUP_EN | 11:11 | 800 | 0 | 0
  DDRIOB_DATA1 @ 0XF8000B4C |  | fff |  | 672

- Register : DDRIOB_DIFF0 @ 0XF8000B50

  Bitfield | Bits | Mask | Value | Shifted Value
  INP_POWER | 0:0 | 1 | 0 | 0
  INP_TYPE | 2:1 | 6 | 2 | 4
  DCI_UPDATE | 3:3 | 8 | 0 | 0
  TERM_EN | 4:4 | 10 | 1 | 10
  DCR_TYPE | 6:5 | 60 | 3 | 60
  IBUF_DISABLE_MODE | 7:7 | 80 | 0 | 0
  TERM_DISABLE_MODE | 8:8 | 100 | 0 | 0
  OUTPUT_EN | 10:9 | 600 | 3 | 600
  PULLUP_EN | 11:11 | 800 | 0 | 0
  DDRIOB_DIFF0 @ 0XF8000B50 |  | fff |  | 674

- Register : DDRIOB_DIFF1 @ 0XF8000B54

  Bitfield | Bits | Mask | Value | Shifted Value
  INP_POWER | 0:0 | 1 | 0 | 0
  INP_TYPE | 2:1 | 6 | 2 | 4
  DCI_UPDATE | 3:3 | 8 | 0 | 0
  TERM_EN | 4:4 | 10 | 1 | 10
  DCR_TYPE | 6:5 | 60 | 3 | 60
  IBUF_DISABLE_MODE | 7:7 | 80 | 0 | 0
  TERM_DISABLE_MODE | 8:8 | 100 | 0 | 0
  OUTPUT_EN | 10:9 | 600 | 3 | 600
  PULLUP_EN | 11:11 | 800 | 0 | 0
  DDRIOB_DIFF1 @ 0XF8000B54 |  | fff |  | 674

- Register : DDRIOB_CLOCK @ 0XF8000B58

  Bitfield | Bits | Mask | Value | Shifted Value
  INP_POWER | 0:0 | 1 | 0 | 0
  INP_TYPE | 2:1 | 6 | 0 | 0
  DCI_UPDATE | 3:3 | 8 | 0 | 0
  TERM_EN | 4:4 | 10 | 0 | 0
  DCR_TYPE | 6:5 | 60 | 0 | 0
  IBUF_DISABLE_MODE | 7:7 | 80 | 0 | 0
  TERM_DISABLE_MODE | 8:8 | 100 | 0 | 0
  OUTPUT_EN | 10:9 | 600 | 3 | 600
  PULLUP_EN | 11:11 | 800 | 0 | 0
  DDRIOB_CLOCK @ 0XF8000B58 |  | fff |  | 600

- Register : DDRIOB_DRIVE_SLEW_ADDR @ 0XF8000B5C

  Bitfield | Bits | Mask | Value | Shifted Value
  DRIVE_P | 6:0 | 7f | 1c | 1c
  DRIVE_N | 13:7 | 3f80 | c | 600
  SLEW_P | 18:14 | 7c000 | 1a | 68000
  SLEW_N | 23:19 | f80000 | 1a | d00000
  GTL | 26:24 | 7000000 | 0 | 0
  RTERM | 31:27 | f8000000 | 0 | 0
  DDRIOB_DRIVE_SLEW_ADDR @ 0XF8000B5C |  | ffffffff |  | d6861c

- Register : DDRIOB_DRIVE_SLEW_DATA @ 0XF8000B60

  Bitfield | Bits | Mask | Value | Shifted Value
  DRIVE_P | 6:0 | 7f | 1c | 1c
  DRIVE_N | 13:7 | 3f80 | c | 600
  SLEW_P | 18:14 | 7c000 | 6 | 18000
  SLEW_N | 23:19 | f80000 | 1f | f80000
  GTL | 26:24 | 7000000 | 0 | 0
  RTERM | 31:27 | f8000000 | 0 | 0
  DDRIOB_DRIVE_SLEW_DATA @ 0XF8000B60 |  | ffffffff |  | f9861c

- Register : DDRIOB_DRIVE_SLEW_DIFF @ 0XF8000B64

  Bitfield | Bits | Mask | Value | Shifted Value
  DRIVE_P | 6:0 | 7f | 1c | 1c
  DRIVE_N | 13:7 | 3f80 | c | 600
  SLEW_P | 18:14 | 7c000 | 6 | 18000
  SLEW_N | 23:19 | f80000 | 1f | f80000
  GTL | 26:24 | 7000000 | 0 | 0
  RTERM | 31:27 | f8000000 | 0 | 0
  DDRIOB_DRIVE_SLEW_DIFF @ 0XF8000B64 |  | ffffffff |  | f9861c

- Register : DDRIOB_DRIVE_SLEW_CLOCK @ 0XF8000B68

  Bitfield | Bits | Mask | Value | Shifted Value
  DRIVE_P | 6:0 | 7f | 1c | 1c
  DRIVE_N | 13:7 | 3f80 | c | 600
  SLEW_P | 18:14 | 7c000 | 1a | 68000
  SLEW_N | 23:19 | f80000 | 1a | d00000
  GTL | 26:24 | 7000000 | 0 | 0
  RTERM | 31:27 | f8000000 | 0 | 0
  DDRIOB_DRIVE_SLEW_CLOCK @ 0XF8000B68 |  | ffffffff |  | d6861c

- Register : DDRIOB_DDR_CTRL @ 0XF8000B6C

  Bitfield | Bits | Mask | Value | Shifted Value
  VREF_INT_EN | 0:0 | 1 | 1 | 1
  VREF_SEL | 4:1 | 1e | 4 | 8
  VREF_EXT_EN | 6:5 | 60 | 0 | 0
  VREF_PULLUP_EN | 8:7 | 180 | 0 | 0
  REFIO_EN | 9:9 | 200 | 1 | 200
  REFIO_TEST | 11:10 | c00 | 3 | c00
  REFIO_PULLUP_EN | 12:12 | 1000 | 0 | 0
  DRST_B_PULLUP_EN | 13:13 | 2000 | 0 | 0
  CKE_PULLUP_EN | 14:14 | 4000 | 0 | 0
  DDRIOB_DDR_CTRL @ 0XF8000B6C |  | 7fff |  | e09

## ASSERT RESET

ASSERT RESET

- Register : DDRIOB_DCI_CTRL @ 0XF8000B70

  Bitfield | Bits | Mask | Value | Shifted Value
  RESET | 0:0 | 1 | 1 | 1
  VRN_OUT | 5:5 | 20 | 1 | 20
  DDRIOB_DCI_CTRL @ 0XF8000B70 |  | 21 |  | 21

## DEASSERT RESET

DEASSERT RESET

- Register : DDRIOB_DCI_CTRL @ 0XF8000B70

  Bitfield | Bits | Mask | Value | Shifted Value
  RESET | 0:0 | 1 | 0 | 0
  VRN_OUT | 5:5 | 20 | 1 | 20
  DDRIOB_DCI_CTRL @ 0XF8000B70 |  | 21 |  | 20

- Register : DDRIOB_DCI_CTRL @ 0XF8000B70

  Bitfield | Bits | Mask | Value | Shifted Value
  RESET | 0:0 | 1 | 1 | 1
  ENABLE | 1:1 | 2 | 1 | 2
  VRP_TRI | 2:2 | 4 | 0 | 0
  VRN_TRI | 3:3 | 8 | 0 | 0
  VRP_OUT | 4:4 | 10 | 0 | 0
  VRN_OUT | 5:5 | 20 | 1 | 20
  NREF_OPT1 | 7:6 | c0 | 0 | 0
  NREF_OPT2 | 10:8 | 700 | 0 | 0
  NREF_OPT4 | 13:11 | 3800 | 1 | 800
  PREF_OPT1 | 16:14 | 1c000 | 0 | 0
  PREF_OPT2 | 19:17 | e0000 | 0 | 0
  UPDATE_CONTROL | 20:20 | 100000 | 0 | 0
  INIT_COMPLETE | 21:21 | 200000 | 0 | 0
  TST_CLK | 22:22 | 400000 | 0 | 0
  TST_HLN | 23:23 | 800000 | 0 | 0
  TST_HLP | 24:24 | 1000000 | 0 | 0
  TST_RST | 25:25 | 2000000 | 0 | 0
  INT_DCI_EN | 26:26 | 4000000 | 0 | 0
  DDRIOB_DCI_CTRL @ 0XF8000B70 |  | 7ffffff |  | 823

## MIO PROGRAMMING

MIO PROGRAMMING

- Register : MIO_PIN_00 @ 0XF8000700

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_00 @ 0XF8000700 |  | fe |  | 0

- Register : MIO_PIN_01 @ 0XF8000704

  Bitfield | Bits | Mask | Value | Shifted Value
  TRI_ENABLE | 0:0 | 1 | 0 | 0
  L0_SEL | 1:1 | 2 | 1 | 2
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  Speed | 8:8 | 100 | 1 | 100
  IO_Type | 11:9 | e00 | 3 | 600
  PULLUP | 12:12 | 1000 | 0 | 0
  DisableRcvr | 13:13 | 2000 | 0 | 0
  MIO_PIN_01 @ 0XF8000704 |  | 3fff |  | 702

- Register : MIO_PIN_02 @ 0XF8000708

  Bitfield | Bits | Mask | Value | Shifted Value
  TRI_ENABLE | 0:0 | 1 | 0 | 0
  L0_SEL | 1:1 | 2 | 1 | 2
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  Speed | 8:8 | 100 | 1 | 100
  IO_Type | 11:9 | e00 | 3 | 600
  PULLUP | 12:12 | 1000 | 0 | 0
  DisableRcvr | 13:13 | 2000 | 0 | 0
  MIO_PIN_02 @ 0XF8000708 |  | 3fff |  | 702

- Register : MIO_PIN_03 @ 0XF800070C

  Bitfield | Bits | Mask | Value | Shifted Value
  TRI_ENABLE | 0:0 | 1 | 0 | 0
  L0_SEL | 1:1 | 2 | 1 | 2
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  Speed | 8:8 | 100 | 1 | 100
  IO_Type | 11:9 | e00 | 3 | 600
  PULLUP | 12:12 | 1000 | 0 | 0
  DisableRcvr | 13:13 | 2000 | 0 | 0
  MIO_PIN_03 @ 0XF800070C |  | 3fff |  | 702

- Register : MIO_PIN_04 @ 0XF8000710

  Bitfield | Bits | Mask | Value | Shifted Value
  TRI_ENABLE | 0:0 | 1 | 0 | 0
  L0_SEL | 1:1 | 2 | 1 | 2
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  Speed | 8:8 | 100 | 1 | 100
  IO_Type | 11:9 | e00 | 3 | 600
  PULLUP | 12:12 | 1000 | 0 | 0
  DisableRcvr | 13:13 | 2000 | 0 | 0
  MIO_PIN_04 @ 0XF8000710 |  | 3fff |  | 702

- Register : MIO_PIN_05 @ 0XF8000714

  Bitfield | Bits | Mask | Value | Shifted Value
  TRI_ENABLE | 0:0 | 1 | 0 | 0
  L0_SEL | 1:1 | 2 | 1 | 2
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  Speed | 8:8 | 100 | 1 | 100
  IO_Type | 11:9 | e00 | 3 | 600
  PULLUP | 12:12 | 1000 | 0 | 0
  DisableRcvr | 13:13 | 2000 | 0 | 0
  MIO_PIN_05 @ 0XF8000714 |  | 3fff |  | 702

- Register : MIO_PIN_06 @ 0XF8000718

  Bitfield | Bits | Mask | Value | Shifted Value
  TRI_ENABLE | 0:0 | 1 | 0 | 0
  L0_SEL | 1:1 | 2 | 1 | 2
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  Speed | 8:8 | 100 | 1 | 100
  IO_Type | 11:9 | e00 | 3 | 600
  PULLUP | 12:12 | 1000 | 0 | 0
  DisableRcvr | 13:13 | 2000 | 0 | 0
  MIO_PIN_06 @ 0XF8000718 |  | 3fff |  | 702

- Register : MIO_PIN_07 @ 0XF800071C

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_07 @ 0XF800071C |  | fe |  | 0

- Register : MIO_PIN_08 @ 0XF8000720

  Bitfield | Bits | Mask | Value | Shifted Value
  TRI_ENABLE | 0:0 | 1 | 0 | 0
  L0_SEL | 1:1 | 2 | 1 | 2
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  Speed | 8:8 | 100 | 1 | 100
  IO_Type | 11:9 | e00 | 3 | 600
  PULLUP | 12:12 | 1000 | 0 | 0
  DisableRcvr | 13:13 | 2000 | 0 | 0
  MIO_PIN_08 @ 0XF8000720 |  | 3fff |  | 702

- Register : MIO_PIN_09 @ 0XF8000724

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_09 @ 0XF8000724 |  | fe |  | 0

- Register : MIO_PIN_10 @ 0XF8000728

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_10 @ 0XF8000728 |  | fe |  | 0

- Register : MIO_PIN_11 @ 0XF800072C

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_11 @ 0XF800072C |  | fe |  | 0

- Register : MIO_PIN_12 @ 0XF8000730

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_12 @ 0XF8000730 |  | fe |  | 0

- Register : MIO_PIN_13 @ 0XF8000734

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_13 @ 0XF8000734 |  | fe |  | 0

- Register : MIO_PIN_14 @ 0XF8000738

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_14 @ 0XF8000738 |  | fe |  | 0

- Register : MIO_PIN_15 @ 0XF800073C

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_15 @ 0XF800073C |  | fe |  | 0

- Register : MIO_PIN_16 @ 0XF8000740

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_16 @ 0XF8000740 |  | fe |  | 0

- Register : MIO_PIN_17 @ 0XF8000744

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_17 @ 0XF8000744 |  | fe |  | 0

- Register : MIO_PIN_18 @ 0XF8000748

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_18 @ 0XF8000748 |  | fe |  | 0

- Register : MIO_PIN_19 @ 0XF800074C

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_19 @ 0XF800074C |  | fe |  | 0

- Register : MIO_PIN_20 @ 0XF8000750

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_20 @ 0XF8000750 |  | fe |  | 0

- Register : MIO_PIN_21 @ 0XF8000754

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_21 @ 0XF8000754 |  | fe |  | 0

- Register : MIO_PIN_22 @ 0XF8000758

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_22 @ 0XF8000758 |  | fe |  | 0

- Register : MIO_PIN_23 @ 0XF800075C

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_23 @ 0XF800075C |  | fe |  | 0

- Register : MIO_PIN_24 @ 0XF8000760

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_24 @ 0XF8000760 |  | fe |  | 0

- Register : MIO_PIN_25 @ 0XF8000764

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_25 @ 0XF8000764 |  | fe |  | 0

- Register : MIO_PIN_26 @ 0XF8000768

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_26 @ 0XF8000768 |  | fe |  | 0

- Register : MIO_PIN_27 @ 0XF800076C

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_27 @ 0XF800076C |  | fe |  | 0

- Register : MIO_PIN_28 @ 0XF8000770

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_28 @ 0XF8000770 |  | fe |  | 0

- Register : MIO_PIN_29 @ 0XF8000774

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_29 @ 0XF8000774 |  | fe |  | 0

- Register : MIO_PIN_30 @ 0XF8000778

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_30 @ 0XF8000778 |  | fe |  | 0

- Register : MIO_PIN_31 @ 0XF800077C

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_31 @ 0XF800077C |  | fe |  | 0

- Register : MIO_PIN_32 @ 0XF8000780

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_32 @ 0XF8000780 |  | fe |  | 0

- Register : MIO_PIN_33 @ 0XF8000784

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_33 @ 0XF8000784 |  | fe |  | 0

- Register : MIO_PIN_34 @ 0XF8000788

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_34 @ 0XF8000788 |  | fe |  | 0

- Register : MIO_PIN_35 @ 0XF800078C

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_35 @ 0XF800078C |  | fe |  | 0

- Register : MIO_PIN_36 @ 0XF8000790

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_36 @ 0XF8000790 |  | fe |  | 0

- Register : MIO_PIN_37 @ 0XF8000794

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_37 @ 0XF8000794 |  | fe |  | 0

- Register : MIO_PIN_38 @ 0XF8000798

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_38 @ 0XF8000798 |  | fe |  | 0

- Register : MIO_PIN_39 @ 0XF800079C

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_39 @ 0XF800079C |  | fe |  | 0

- Register : MIO_PIN_40 @ 0XF80007A0

  Bitfield | Bits | Mask | Value | Shifted Value
  TRI_ENABLE | 0:0 | 1 | 0 | 0
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 4 | 80
  Speed | 8:8 | 100 | 1 | 100
  IO_Type | 11:9 | e00 | 1 | 200
  PULLUP | 12:12 | 1000 | 0 | 0
  DisableRcvr | 13:13 | 2000 | 0 | 0
  MIO_PIN_40 @ 0XF80007A0 |  | 3fff |  | 380

- Register : MIO_PIN_41 @ 0XF80007A4

  Bitfield | Bits | Mask | Value | Shifted Value
  TRI_ENABLE | 0:0 | 1 | 0 | 0
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 4 | 80
  Speed | 8:8 | 100 | 1 | 100
  IO_Type | 11:9 | e00 | 1 | 200
  PULLUP | 12:12 | 1000 | 0 | 0
  DisableRcvr | 13:13 | 2000 | 0 | 0
  MIO_PIN_41 @ 0XF80007A4 |  | 3fff |  | 380

- Register : MIO_PIN_42 @ 0XF80007A8

  Bitfield | Bits | Mask | Value | Shifted Value
  TRI_ENABLE | 0:0 | 1 | 0 | 0
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 4 | 80
  Speed | 8:8 | 100 | 1 | 100
  IO_Type | 11:9 | e00 | 1 | 200
  PULLUP | 12:12 | 1000 | 0 | 0
  DisableRcvr | 13:13 | 2000 | 0 | 0
  MIO_PIN_42 @ 0XF80007A8 |  | 3fff |  | 380

- Register : MIO_PIN_43 @ 0XF80007AC

  Bitfield | Bits | Mask | Value | Shifted Value
  TRI_ENABLE | 0:0 | 1 | 0 | 0
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 4 | 80
  Speed | 8:8 | 100 | 1 | 100
  IO_Type | 11:9 | e00 | 1 | 200
  PULLUP | 12:12 | 1000 | 0 | 0
  DisableRcvr | 13:13 | 2000 | 0 | 0
  MIO_PIN_43 @ 0XF80007AC |  | 3fff |  | 380

- Register : MIO_PIN_44 @ 0XF80007B0

  Bitfield | Bits | Mask | Value | Shifted Value
  TRI_ENABLE | 0:0 | 1 | 0 | 0
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 4 | 80
  Speed | 8:8 | 100 | 1 | 100
  IO_Type | 11:9 | e00 | 1 | 200
  PULLUP | 12:12 | 1000 | 0 | 0
  DisableRcvr | 13:13 | 2000 | 0 | 0
  MIO_PIN_44 @ 0XF80007B0 |  | 3fff |  | 380

- Register : MIO_PIN_45 @ 0XF80007B4

  Bitfield | Bits | Mask | Value | Shifted Value
  TRI_ENABLE | 0:0 | 1 | 0 | 0
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 4 | 80
  Speed | 8:8 | 100 | 1 | 100
  IO_Type | 11:9 | e00 | 1 | 200
  PULLUP | 12:12 | 1000 | 0 | 0
  DisableRcvr | 13:13 | 2000 | 0 | 0
  MIO_PIN_45 @ 0XF80007B4 |  | 3fff |  | 380

- Register : MIO_PIN_46 @ 0XF80007B8

  Bitfield | Bits | Mask | Value | Shifted Value
  TRI_ENABLE | 0:0 | 1 | 1 | 1
  Speed | 8:8 | 100 | 0 | 0
  IO_Type | 11:9 | e00 | 1 | 200
  PULLUP | 12:12 | 1000 | 0 | 0
  DisableRcvr | 13:13 | 2000 | 0 | 0
  MIO_PIN_46 @ 0XF80007B8 |  | 3f01 |  | 201

- Register : MIO_PIN_47 @ 0XF80007BC

  Bitfield | Bits | Mask | Value | Shifted Value
  TRI_ENABLE | 0:0 | 1 | 1 | 1
  Speed | 8:8 | 100 | 0 | 0
  IO_Type | 11:9 | e00 | 1 | 200
  PULLUP | 12:12 | 1000 | 0 | 0
  DisableRcvr | 13:13 | 2000 | 0 | 0
  MIO_PIN_47 @ 0XF80007BC |  | 3f01 |  | 201

- Register : MIO_PIN_48 @ 0XF80007C0

  Bitfield | Bits | Mask | Value | Shifted Value
  TRI_ENABLE | 0:0 | 1 | 0 | 0
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 7 | e0
  Speed | 8:8 | 100 | 0 | 0
  IO_Type | 11:9 | e00 | 1 | 200
  PULLUP | 12:12 | 1000 | 0 | 0
  DisableRcvr | 13:13 | 2000 | 0 | 0
  MIO_PIN_48 @ 0XF80007C0 |  | 3fff |  | 2e0

- Register : MIO_PIN_49 @ 0XF80007C4

  Bitfield | Bits | Mask | Value | Shifted Value
  TRI_ENABLE | 0:0 | 1 | 1 | 1
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 7 | e0
  Speed | 8:8 | 100 | 0 | 0
  IO_Type | 11:9 | e00 | 1 | 200
  PULLUP | 12:12 | 1000 | 0 | 0
  DisableRcvr | 13:13 | 2000 | 0 | 0
  MIO_PIN_49 @ 0XF80007C4 |  | 3fff |  | 2e1

- Register : MIO_PIN_50 @ 0XF80007C8

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_50 @ 0XF80007C8 |  | fe |  | 0

- Register : MIO_PIN_51 @ 0XF80007CC

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_51 @ 0XF80007CC |  | fe |  | 0

- Register : MIO_PIN_52 @ 0XF80007D0

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_52 @ 0XF80007D0 |  | fe |  | 0

- Register : MIO_PIN_53 @ 0XF80007D4

  Bitfield | Bits | Mask | Value | Shifted Value
  L0_SEL | 1:1 | 2 | 0 | 0
  L1_SEL | 2:2 | 4 | 0 | 0
  L2_SEL | 4:3 | 18 | 0 | 0
  L3_SEL | 7:5 | e0 | 0 | 0
  MIO_PIN_53 @ 0XF80007D4 |  | fe |  | 0

- Register : SD0_WP_CD_SEL @ 0XF8000830

  Bitfield | Bits | Mask | Value | Shifted Value
  SDIO0_WP_SEL | 5:0 | 3f | 2e | 2e
  SDIO0_CD_SEL | 21:16 | 3f0000 | 2f | 2f0000
  SD0_WP_CD_SEL @ 0XF8000830 |  | 3f003f |  | 2f002e

- Register : LVL_SHFTR_EN @ 0XF8000900

  Bitfield | Bits | Mask | Value | Shifted Value
  USER_INP_ICT_EN_0 | 1:0 | 3 | 3 | 3
  USER_INP_ICT_EN_1 | 3:2 | c | 3 | c
  LVL_SHFTR_EN @ 0XF8000900 |  | f |  | f

## LOCK IT BACK

LOCK IT BACK

- Register : SLCR_LOCK @ 0XF8000004

  Bitfield | Bits | Mask | Value | Shifted Value
  LOCK_KEY | 15:0 | ffff | 767b | 767b
  SLCR_LOCK @ 0XF8000004 |  | ffff |  | 767b

# ps7_peripherals_init_data

## UART REGISTERS

UART REGISTERS

- Register : Baud_rate_divider_reg0 @ 0XE0001034

  Bitfield | Bits | Mask | Value | Shifted Value
  BDIV | 7:0 | ff | 6 | 6
  Baud_rate_divider_reg0 @ 0XE0001034 |  | ff |  | 6

- Register : Baud_rate_gen_reg0 @ 0XE0001018

  Bitfield | Bits | Mask | Value | Shifted Value
  CD | 15:0 | ffff | 3e | 3e
  Baud_rate_gen_reg0 @ 0XE0001018 |  | ffff |  | 3e

- Register : Control_reg0 @ 0XE0001000

  Bitfield | Bits | Mask | Value | Shifted Value
  STPBRK | 8:8 | 100 | 0 | 0
  STTBRK | 7:7 | 80 | 0 | 0
  RSTTO | 6:6 | 40 | 0 | 0
  TXDIS | 5:5 | 20 | 0 | 0
  TXEN | 4:4 | 10 | 1 | 10
  RXDIS | 3:3 | 8 | 0 | 0
  RXEN | 2:2 | 4 | 1 | 4
  TXRES | 1:1 | 2 | 1 | 2
  RXRES | 0:0 | 1 | 1 | 1
  Control_reg0 @ 0XE0001000 |  | 1ff |  | 17

- Register : mode_reg0 @ 0XE0001004

  Bitfield | Bits | Mask | Value | Shifted Value
  IRMODE | 11:11 | 800 | 0 | 0
  UCLKEN | 10:10 | 400 | 0 | 0
  CHMODE | 9:8 | 300 | 0 | 0
  NBSTOP | 7:6 | c0 | 0 | 0
  PAR | 5:3 | 38 | 4 | 20
  CHRL | 2:1 | 6 | 0 | 0
  CLKS | 0:0 | 1 | 0 | 0
  mode_reg0 @ 0XE0001004 |  | fff |  | 20

## AFI REGISTERS

AFI REGISTERS

## AFI0 REGISTERS

AFI0 REGISTERS

## AFI1 REGISTERS

AFI1 REGISTERS

## AFI2 REGISTERS

AFI2 REGISTERS

## AFI3 REGISTERS

AFI3 REGISTERS