Sonoma (MAXREFDES14#) Code Documentation V01.00 Isolated EMP (Energy Measurement Processor)

- Main Page
- Data Structures
- Files

- File List
- Globals

- All
- Functions
- Variables
- Macros

- a
- b
- c
- d
- e
- f
- g
- h
- i
- k
- l
- m
- n
- o
- p
- r
- s
- t
- u
- w

All Data Structures Files Functions Variables Macros Pages
Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - a -

- ABOUT_ONE_SECOND : MAXREFDES14.h

### - b -

- BASE_FUNCTION_STATE : menu.h

### - c -

- checkUartEmpty() : utilities.c , utilities.h
- cleanup_platform() : platform.h , platform.c
- clearOLEDBuffer() : utilities.h , utilities.c

### - d -

- DEFAULT_HYPERTERMINAL_UART_ADDRESS : MAXREFDES14.h
- DEFAULT_HYPERTERMINAL_UART_ID : MAXREFDES14.h
- delay() : utilities.h , utilities.c
- disable_caches() : platform.c
- displayOLEDBuffer() : utilities.c , utilities.h

### - e -

- enable_caches() : platform.c

### - f -

- flipAndCopyDisplayBuffer() : utilities.c , utilities.h
- font : MAXREFDES14.c

### - g -

- g_nSampleRate : MAXREFDES14.h
- g_sInputString : MAXREFDES14.c , MAXREFDES14.h
- g_sTempString : MAXREFDES14.c
- g_structureOLED : MAXREFDES14.c , MAXREFDES14.h
- g_tempString : MAXREFDES14.h
- g_uchAtoDConverterChannel : MAXREFDES14.h
- g_unSampleSize : MAXREFDES14.h
- g_xGpioLed : MAXREFDES14.h , MAXREFDES14.c
- getUartByte() : utilities.h , utilities.c

### - h -

- htoi() : utilities.c , utilities.h

### - i -

- init_platform() : platform.c , platform.h
- init_uart() : platform.c
- initializeOLED() : utilities.c , utilities.h
- INPUT_STRING_MAX_SIZE : MAXREFDES14.h

### - k -

- KEYPRESS_ARROW_DOWN : menu.h
- KEYPRESS_ARROW_LEFT : menu.h
- KEYPRESS_ARROW_RIGHT : menu.h
- KEYPRESS_ARROW_UP : menu.h
- KEYPRESS_END : menu.h

### - l -

- led_knight_rider() : utilities.c , utilities.h

### - m -

- main() : MAXREFDES14.c
- MAIN_MENU : menu.h
- MAJOR_REVISION : MAXREFDES14.c
- menu_cls() : menu.c , menu.h
- menu_print_line() : menu.c
- menu_print_main_menu() : menu.h , menu.c
- menu_print_maxim_banner() : menu.c , menu.h
- menu_print_maxim_banner_big() : menu.c , menu.h
- menu_print_prompt() : menu.c , menu.h
- MENU_READ_REG : menu.h
- MENU_REG_ADDR : menu.h
- menu_retrieve_keypress() : menu.h , menu.c
- MENU_WRITE_REG : menu.h
- MINOR_REVISION : MAXREFDES14.c

### - n -

- number_raised_to_power() : utilities.c , utilities.h

### - o -

- OLED_DATA_COMMAND_B : utilities.c
- OLED_RESET_B : utilities.c
- OLED_SCLK : utilities.c
- OLED_SDIN : utilities.c
- OLED_VBAT : utilities.c
- OLED_VDD : utilities.c

### - p -

- print_asterisks() : utilities.c , utilities.h
- printfToBufferOLED() : utilities.h , utilities.c
- printfToOLED() : utilities.c , utilities.h
- putCharOLED() : utilities.h , utilities.c

### - r -

- read_reg() : maximDeviceSpecificUtilities.c , maximDeviceSpecificUtilities.h

### - s -

- sendOLEDSPI() : utilities.h
- sendUartByte() : utilities.h
- suchEndOLEDSPI() : utilities.c
- suchEndUartByte() : utilities.c

### - t -

- t : utilities.h

### - u -

- UART_BASEADDR : utilities.c
- UART_BAUD : platform.c

### - w -

- WAIT_KEYPRESS : menu.h
- write_reg() : maximDeviceSpecificUtilities.h , maximDeviceSpecificUtilities.c