Par Statistics
Total Non-vccgnd Signals=7242
Total Non-vccgnd Design Pins=27161
Total Non-vccgnd Conns=27161
Total Non-vccgnd Timing Constrained Conns=25353
Phase 1 CPU=13.4 sec
Phase 2 CPU=14.6 sec
Phase 3 CPU=27.5 sec
Phase 4 CPU=28.8 sec
Phase 5 CPU=58.1 sec
Phase 6 CPU=58.1 sec
Phase 7 CPU=58.1 sec
Phase 8 CPU=58.1 sec
Phase 9 CPU=58.9 sec
Phase 10 CPU=61.9 sec
AvgWirelenPerPin Fanout 1=4.0
AvgWirelenPerPin Fanout 2=4.5
AvgWirelenPerPin Fanout 3=4.0
AvgWirelenPerPin Fanout 4=5.3
AvgWirelenPerPin Fanout 10=3.6
AvgWirelenPerPin Fanout 50=3.6
AvgWirelenPerPin Fanout 100=10.0
AvgWirelenPerPin Fanout 500=9.0
AvgWirelenPerPin Fanout 5000=5.5
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=39.0984