Par Statistics
Total Non-vccgnd Signals=473
Total Non-vccgnd Design Pins=1372
Total Non-vccgnd Conns=1372
Total Non-vccgnd Timing Constrained Conns=1322
Phase 1 CPU=24.8 sec
Phase 2 CPU=25.2 sec
Phase 3 CPU=26.5 sec
Phase 4 CPU=31.8 sec
Phase 5 CPU=32.6 sec
Phase 6 CPU=32.6 sec
Phase 7 CPU=32.6 sec
Phase 8 CPU=32.6 sec
Phase 9 CPU=32.8 sec
AvgWirelenPerPin Fanout 1=15.0
AvgWirelenPerPin Fanout 2=14.0
AvgWirelenPerPin Fanout 3=2.0
AvgWirelenPerPin Fanout 4=1.0
AvgWirelenPerPin Fanout 10=2.7
AvgWirelenPerPin Fanout 50=4.8
AvgWirelenPerPin Fanout 100=39.4
AvgWirelenPerPin Fanout 500=0.0
AvgWirelenPerPin Fanout 5000=0.0
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=1.0231